Cytosim PI Cytoskeleton Simulator

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

Variables
Parameters of Nucleator
All object parameters

## Variables
real | nucleation_rate
| rate for nucleation (also known as `nucleate`[0])
std::string | nucleated_fiber
| type of fiber that is nucleated (also known as `nucleate`[1])
std::string | nucleation_spec
| specifications of a new fiber (also known as `nucleate`[2]) More...
Specificity | specificity
| specifies the direction of the new Fiber More...
FiberEnd | track_end
| option to track a specified end [none, plus_end, minus_end, nearest_end] More...
bool | addictive
| if true, set the Dynamic State of the nearest filament end to STATE_RED upon detachment

## Detailed Description

Inherits Parameters of Hand. Check the examples!

## Variable Documentation

std::string nucleation_spec

Options valid for the command 'new fiber' may be specified here: see Fiber and Derived Activities.

Specificity specificity

The `specificity` can be:

- none (default)
- parallel
- antiparallel

With 'specificity=none', the direction will follow the value of 'orientation', specified within `nucleation_spec`.

FiberEnd track_end

By default the Hand will remain attached at the MINUS_END of any fiber that it has nucleated. But other values are possible:

- none
- plus_end
- minus_end
- nearest_end