Cytosim PI Cytoskeleton Simulator

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

Variables
Parameters of Motor
All object parameters

## Variables
real | stall_force
| force at which speed becomes zero (positive)
real | max_speed
| speed when the force is zero More...
bool | limit_speed
| if true, the speed is limited to the range [0, 2*max_speed] More...

## Detailed Description

Inherits Parameters of Hand. Check the examples!

## Variable Documentation

bool limit_speed

With ( limit_speed = 1 ), a plus-end directed motor will not move towards the minus-end, and also will not exceed 2x its max speed. For a minus-end directed motor, the permitted range is [2*max_speed, 0], thus also excluding backward steps.

real max_speed

A positive value specifies a plus-end directed motor. A negative value specifies a minus-end directed motor.