Table of Contents

Program Version:EnergyPlus, Version 24.2.0-94a887817b, YMD=2025.09.12 10:23

Tabular Output Report in Format: HTML

Building: Two story apartment

Environment: RUN PERIOD 1 ** MILAN - ITA IWEC Data WMO#=160660

Simulation Timestamp: 2025-09-12 10:23:48

Table of Contents

Report: Annual Building Utility Performance Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Values gathered over 8760.00 hours
Site and Source Energy

| Total Energy [GJ] | Energy Per Total Building Area [MJ/m2] | Energy Per Conditioned Building Area [MJ/m2]
Total Site Energy | 142.97 | 687.36 | 876.05
Net Site Energy | 142.97 | 687.36 | 876.05
Total Source Energy | 485.85 | 2335.80 | 2977.00
Net Source Energy | 485.85 | 2335.80 | 2977.00

Site to Source Energy Conversion Factors

| Site=>Source Conversion Factor
Electricity | 3.167
Natural Gas | 1.084
District Cooling | 1.056
District Heating Water | 3.613
District Heating Steam | 1.200
Gasoline | 1.050
Diesel | 1.050
Coal | 1.050
Fuel Oil No 1 | 1.050
Fuel Oil No 2 | 1.050
Propane | 1.050
Other Fuel 1 | 1.000
Other Fuel 2 | 1.000

Building Area

| Area [m2]
Total Building Area | 208.00
Net Conditioned Building Area | 163.20
Unconditioned Building Area | 44.80

End Uses

| Electricity [GJ] | Natural Gas [GJ] | Gasoline [GJ] | Diesel [GJ] | Coal [GJ] | Fuel Oil No 1 [GJ] | Fuel Oil No 2 [GJ] | Propane [GJ] | Other Fuel 1 [GJ] | Other Fuel 2 [GJ] | District Cooling [GJ] | District Heating Water [GJ] | District Heating Steam [GJ] | Water [m3]
Heating | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 98.95 | 0.00 | 0.00
Cooling | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.26 | 0.00 | 0.00 | 0.00
Interior Lighting | 20.54 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 18.22 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total End Uses | 38.76 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.26 | 98.95 | 0.00 | 0.00

Note: District heating water appears to be the principal heating source based on energy usage.
End Uses By Subcategory

| Subcategory | Electricity [GJ] | Natural Gas [GJ] | Gasoline [GJ] | Diesel [GJ] | Coal [GJ] | Fuel Oil No 1 [GJ] | Fuel Oil No 2 [GJ] | Propane [GJ] | Other Fuel 1 [GJ] | Other Fuel 2 [GJ] | District Cooling [GJ] | District Heating Water [GJ] | District Heating Steam [GJ] | Water [m3]
Heating | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 98.95 | 0.00 | 0.00
Cooling | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.26 | 0.00 | 0.00 | 0.00
Interior Lighting | General | 20.54 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | General | 18.22 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

End Uses By Space Type

| Space Type | Electricity [GJ] | Natural Gas [GJ] | Gasoline [GJ] | Diesel [GJ] | Coal [GJ] | Fuel Oil No 1 [GJ] | Fuel Oil No 2 [GJ] | Propane [GJ] | Other Fuel 1 [GJ] | Other Fuel 2 [GJ] | District Cooling [GJ] | District Heating Water [GJ] | District Heating Steam [GJ] | Water [m3]
Heating | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 98.95 | 0.00 | 0.00
Cooling | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.26 | 0.00 | 0.00 | 0.00
Interior Lighting | MIDRISEAPARTMENT APARTMENT | 6.55 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| MIDRISEAPARTMENT CORRIDOR | 13.99 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | MIDRISEAPARTMENT APARTMENT | 18.22 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Normalized Metrics
Utility Use Per Conditioned Floor Area

| Electricity Intensity [MJ/m2] | Natural Gas Intensity [MJ/m2] | Gasoline Intensity [MJ/m2] | Diesel Intensity [MJ/m2] | Coal Intensity [MJ/m2] | Fuel Oil No 1 Intensity [MJ/m2] | Fuel Oil No 2 Intensity [MJ/m2] | Propane Intensity [MJ/m2] | Other Fuel 1 Intensity [MJ/m2] | Other Fuel 2 Intensity [MJ/m2] | District Cooling Intensity [MJ/m2] | District Heating Water Intensity [MJ/m2] | District Heating Steam Intensity [MJ/m2] | Water Intensity [m3/m2]
Lighting | 125.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
HVAC | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 32.23 | 606.30 | 0.00 | 0.00
Other | 111.67 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total | 237.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 32.23 | 606.30 | 0.00 | 0.00

Utility Use Per Total Floor Area

| Electricity Intensity [MJ/m2] | Natural Gas Intensity [MJ/m2] | Gasoline Intensity [MJ/m2] | Diesel Intensity [MJ/m2] | Coal Intensity [MJ/m2] | Fuel Oil No 1 Intensity [MJ/m2] | Fuel Oil No 2 Intensity [MJ/m2] | Propane Intensity [MJ/m2] | Other Fuel 1 Intensity [MJ/m2] | Other Fuel 2 Intensity [MJ/m2] | District Cooling Intensity [MJ/m2] | District Heating Water Intensity [MJ/m2] | District Heating Steam Intensity [MJ/m2] | Water Intensity [m3/m2]
Lighting | 98.74 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |
HVAC | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 25.29 | 475.71 | 0.00 |
Other | 87.61 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |
Total | 186.36 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 25.29 | 475.71 | 0.00 |

Electric Loads Satisfied

| Electricity [GJ] | Percent Electricity [%]
Fuel-Fired Power Generation | 0.000 | 0.00
High Temperature Geothermal* | 0.000 | 0.00
Photovoltaic Power | 0.000 | 0.00
Wind Power | 0.000 | 0.00
Power Conversion | 0.000 | 0.00
Net Decrease in On-Site Storage | 0.000 | 0.00
Total On-Site Electric Sources | 0.000 | 0.00
Electricity Coming From Utility | 38.763 | 100.00
Surplus Electricity Going To Utility | 0.000 | 0.00
Net Electricity From Utility | 38.763 | 100.00
Total On-Site and Utility Electric Sources | 38.763 | 100.00
Total Electricity End Uses | 38.763 | 100.00

On-Site Thermal Sources

| Heat [GJ] | Percent Heat [%]
Water-Side Heat Recovery | 0.00 |
Air to Air Heat Recovery for Cooling | 0.00 |
Air to Air Heat Recovery for Heating | 0.00 |
High-Temperature Geothermal* | 0.00 |
Solar Water Thermal | 0.00 |
Solar Air Thermal | 0.00 |
Total On-Site Thermal Sources | 0.00 |

Water Source Summary

| Water [m3] | Percent Water [%]
Rainwater Collection | 0.00 | -
Condensate Collection | 0.00 | -
Groundwater Well | 0.00 | -
Total On Site Water Sources | 0.00 | -
- | - | -
Initial Storage | 0.00 | -
Final Storage | 0.00 | -
Change in Storage | 0.00 | -
- | - | -
Water Supplied by Utility | 0.00 | -
- | - | -
Total On Site, Change in Storage, and Utility Water Sources | 0.00 | -
Total Water End Uses | 0.00 | -

Setpoint Not Met Criteria

| Degrees [deltaC]
Tolerance for Zone Heating Setpoint Not Met Time | 0.20
Tolerance for Zone Cooling Setpoint Not Met Time | 0.20

Comfort and Setpoint Not Met Summary

| Facility [Hours]
Time Setpoint Not Met During Occupied Heating | 0.00
Time Setpoint Not Met During Occupied Cooling | 0.00
Time Not Comfortable Based on Simple ASHRAE 55-2004 | 7044.83

Note 1: An asterisk (*) indicates that the feature is not yet implemented.

Table of Contents

Top
Annual Building Utility Performance Summary
Input Verification and Results Summary
Demand End Use Components Summary
Source Energy End Use Components Summary
Component Sizing Summary
Surface Shadowing Summary
Adaptive Comfort Summary
Initialization Summary
Annual Heat Emissions Summary
Annual Thermal Resilience Summary
Climatic Data Summary
Envelope Summary
Shading Summary
Lighting Summary
Equipment Summary
HVAC Sizing Summary
Coil Sizing Details
System Summary
HVAC Topology
Outdoor Air Summary
Outdoor Air Details
Object Count Summary
Energy Meters
Sensible Heat Gain Summary
LEED Summary
Annual CO2 Resilience Summary
Annual Visual Resilience Summary

BUILDING ENERGY PERFORMANCE - ELECTRICITY

| Meter |

BUILDING ENERGY PERFORMANCE - DISTRICT HEATING WATER

| Meter |

BUILDING ENERGY PERFORMANCE - DISTRICT COOLING

| Meter |

BUILDING ENERGY PERFORMANCE - ELECTRICITY PEAK DEMAND

| Meter |

BUILDING ENERGY PERFORMANCE - DISTRICT HEATING WATER PEAK DEMAND

| Meter |

BUILDING ENERGY PERFORMANCE - DISTRICT COOLING PEAK DEMAND

| Meter |

Life-Cycle Cost Report

| Entire Facility |

Table of Contents

Report: Input Verification and Results Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

General

| Value
Program Version and Build | EnergyPlus, Version 24.2.0-94a887817b, YMD=2025.09.12 10:23
RunPeriod | RUN PERIOD 1
Weather File | MILAN - ITA IWEC Data WMO#=160660
Latitude [deg] | 45.62
Longitude [deg] | 8.73
Elevation [m] | 211.00
Time Zone | 1.00
North Axis Angle [deg] | -45.0
Rotation for Appendix G [deg] | 0.00
Hours Simulated [hrs] | 8760.00

ENVELOPE
Window-Wall Ratio

| Total | North (315 to 45 deg) | East (45 to 135 deg) | South (135 to 225 deg) | West (225 to 315 deg)
Gross Wall Area [m2] | 226.80 | 70.20 | 43.20 | 70.20 | 43.20
Above Ground Wall Area [m2] | 226.80 | 70.20 | 43.20 | 70.20 | 43.20
Window Opening Area [m2] | 21.44 | 11.20 | 2.24 | 0.00 | 8.00
Gross Window-Wall Ratio [%] | 9.45 | 15.95 | 5.19 | 0.00 | 18.52
Above Ground Window-Wall Ratio [%] | 9.45 | 15.95 | 5.19 | 0.00 | 18.52

Conditioned Window-Wall Ratio

| Total | North (315 to 45 deg) | East (45 to 135 deg) | South (135 to 225 deg) | West (225 to 315 deg)
Gross Wall Area [m2] | 153.36 | 55.08 | 43.20 | 55.08 | 0.00
Above Ground Wall Area [m2] | 153.36 | 55.08 | 43.20 | 55.08 | 0.00
Window Opening Area [m2] | 13.44 | 11.20 | 2.24 | 0.00 | 0.00
Gross Window-Wall Ratio [%] | 8.76 | 20.33 | 5.19 | 0.00 | 0.00
Above Ground Window-Wall Ratio [%] | 8.76 | 20.33 | 5.19 | 0.00 | 0.00

Skylight-Roof Ratio

| Total
Gross Roof Area [m2] | 104.00
Skylight Area [m2] | 0.00
Skylight-Roof Ratio [%] | 0.00

PERFORMANCE
Zone Summary

| Area [m2] | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Volume [m3] | Multipliers | Above Ground Gross Wall Area [m2] | Underground Gross Wall Area [m2] | Window Glass Area [m2] | Opening Area [m2] | Lighting [W/m2] | People [m2 per person] | Plug and Process [W/m2]
TZ_0-A1.B | 24.68 | Yes | Yes | 66.63 | 1.00 | 25.92 | 0.00 | 2.24 | 2.24 | 3.8750 | 35.32 | 5.3820
TZ_0-A1.LK | 45.20 | Yes | Yes | 122.04 | 1.00 | 30.51 | 0.00 | 3.36 | 3.36 | 3.8750 | 35.32 | 5.3820
TZ_0-A1.WC | 11.72 | Yes | Yes | 31.65 | 1.00 | 20.25 | 0.00 | 1.12 | 1.12 | 3.8750 | 35.32 | 5.3820
TZ_0-H | 22.40 | No | Yes | 60.48 | 1.00 | 36.72 | 0.00 | 5.76 | 5.76 | 9.9028 |  | 0.0000
TZ_1-A2.B | 24.68 | Yes | Yes | 66.63 | 1.00 | 25.92 | 0.00 | 2.24 | 2.24 | 3.8750 | 35.32 | 5.3820
TZ_1-A2.LK | 45.20 | Yes | Yes | 122.04 | 1.00 | 30.51 | 0.00 | 3.36 | 3.36 | 3.8750 | 35.32 | 5.3820
TZ_1-A2.WC | 11.72 | Yes | Yes | 31.65 | 1.00 | 20.25 | 0.00 | 1.12 | 1.12 | 3.8750 | 35.32 | 5.3820
TZ_1-H | 22.40 | No | Yes | 60.48 | 1.00 | 36.72 | 0.00 | 2.24 | 2.24 | 9.9028 |  | 0.0000
Total | 208.00 |  |  | 561.60 |  | 226.80 | 0.00 | 21.44 | 21.44 | 5.1733 | 45.02 | 4.2228
Conditioned Total | 163.20 |  |  | 440.64 |  | 153.36 | 0.00 | 13.44 | 13.44 | 3.8750 | 35.32 | 5.3820
Unconditioned Total | 44.80 |  |  | 120.96 |  | 73.44 | 0.00 | 8.00 | 8.00 | 9.9028 |  | 0.0000
Not Part of Total | 0.00 |  |  | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 |  |  |

Space Summary

| Area [m2] | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Multipliers | Zone Name | Space Type | Radiant/Solar Enclosure Name | Lighting [W/m2] | People [m2 per person] | Plug and Process [W/m2] | Tags
0-A1.B | 24.68 | Yes | Yes | 1.00 | TZ_0-A1.B | MIDRISEAPARTMENT APARTMENT | 0-A1.B | 3.8750 | 35.32 | 5.3820 |
0-A1.LK | 45.20 | Yes | Yes | 1.00 | TZ_0-A1.LK | MIDRISEAPARTMENT APARTMENT | 0-A1.LK | 3.8750 | 35.32 | 5.3820 |
0-A1.WC | 11.72 | Yes | Yes | 1.00 | TZ_0-A1.WC | MIDRISEAPARTMENT APARTMENT | 0-A1.WC | 3.8750 | 35.32 | 5.3820 |
0-H | 22.40 | No | Yes | 1.00 | TZ_0-H | MIDRISEAPARTMENT CORRIDOR | 0-H | 9.9028 | 0.00 | 0.0000 |
1-A2.B | 24.68 | Yes | Yes | 1.00 | TZ_1-A2.B | MIDRISEAPARTMENT APARTMENT | 1-A2.B | 3.8750 | 35.32 | 5.3820 |
1-A2.LK | 45.20 | Yes | Yes | 1.00 | TZ_1-A2.LK | MIDRISEAPARTMENT APARTMENT | 1-A2.LK | 3.8750 | 35.32 | 5.3820 |
1-A2.WC | 11.72 | Yes | Yes | 1.00 | TZ_1-A2.WC | MIDRISEAPARTMENT APARTMENT | 1-A2.WC | 3.8750 | 35.32 | 5.3820 |
1-H | 22.40 | No | Yes | 1.00 | TZ_1-H | MIDRISEAPARTMENT CORRIDOR | 1-H | 9.9028 | 0.00 | 0.0000 |
Total | 208.00 |  |  |  |  |  |  | 5.1733 | 45.02 | 4.2228 |
Conditioned Total | 163.20 |  |  |  |  |  |  | 3.8750 | 35.32 | 5.3820 |
Unconditioned Total | 44.80 |  |  |  |  |  |  | 9.9028 | 0.00 | 0.0000 |
Not Part of Total | 0.00 |  |  |  |  |  |  | 0.0000 | 0.00 | 0.0000 |

Space Type Summary

| Total Area [m2] | Conditioned Area [m2] | Unconditioned Area [m2] | Not Part of Total Area [m2] | Lighting [W/m2] | People [m2 per person] | Plug and Process [W/m2]
MIDRISEAPARTMENT APARTMENT | 163.20 | 163.20 | 0.00 | 0.00 | 3.8750 | 35.32 | 5.3820
MIDRISEAPARTMENT CORRIDOR | 44.80 | 0.00 | 44.80 | 0.00 | 9.9028 | 0.00 | 0.0000
Total | 208.00 | 163.20 | 44.80 | 0.00 |  |  |

Table of Contents

Report: Demand End Use Components Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

End Uses

| Electricity [W] | Natural Gas [W] | Gasoline [W] | Diesel [W] | Coal [W] | Fuel Oil No 1 [W] | Fuel Oil No 2 [W] | Propane [W] | Other Fuel 1 [W] | Other Fuel 2 [W] | District Cooling [W] | District Heating Water [W] | District Heating Steam [W] | Water [m3/s]
Time of Peak | 01-JAN-19:20 | - | - | - | - | - | - | - | - | - | 21-JUL-18:10 | 30-JAN-03:10 | - | -
Heating | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14319.37 | 0.00 | 0.00
Cooling | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5825.27 | 0.00 | 0.00 | 0.00
Interior Lighting | 1067.19 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total End Uses | 1884.04 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5825.27 | 14319.37 | 0.00 | 0.00

End Uses By Subcategory

| Subcategory | Electricity [W] | Natural Gas [W] | Gasoline [W] | Diesel [W] | Coal [W] | Fuel Oil No 1 [W] | Fuel Oil No 2 [W] | Propane [W] | Other Fuel 1 [W] | Other Fuel 2 [W] | District Cooling [W] | District Heating Water [W] | District Heating Steam [W] | Water [m3/s]
Heating | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14319.37 | 0.00 | 0.00
Cooling | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5825.27 | 0.00 | 0.00 | 0.00
Interior Lighting | General | 1067.19 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | General | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Source Energy End Use Components Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Values gathered over 8760.00 hours
Source Energy End Use Components Summary

| Source Electricity [GJ] | Source Natural Gas [GJ] | Source Gasoline [GJ] | Source Diesel [GJ] | Source Coal [GJ] | Source Fuel Oil No 1 [GJ] | Source Fuel Oil No 2 [GJ] | Source Propane [GJ] | Source Other Fuel 1 [GJ] | Source Other Fuel 2 [GJ] | Source District Cooling [GJ] | Source District Heating Water [GJ] | Source District Heating Steam [GJ]
Heating | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 357.53 | 0.00
Cooling | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.55 | 0.00 | 0.00
Interior Lighting | 65.05 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 57.71 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 122.76 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.55 | 357.53 | 0.00

Normalized Metrics
Source Energy End Use Components Per Conditioned Floor Area

| Source Electricity [MJ/m2] | Source Natural Gas [MJ/m2] | Source Gasoline [MJ/m2] | Source Diesel [MJ/m2] | Source Coal [MJ/m2] | Source Fuel Oil No 1 [MJ/m2] | Source Fuel Oil No 2 [MJ/m2] | Source Propane [MJ/m2] | Source Other Fuel 1 [MJ/m2] | Source Other Fuel 2 [MJ/m2] | Source District Cooling [MJ/m2] | Source District Heating Water [MJ/m2] | Source District Heating Steam [MJ/m2]
Heating | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 2190.76 | 0.00
Cooling | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 34.03 | 0.00 | 0.00
Interior Lighting | 398.57 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 353.64 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 752.21 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 34.03 | 2190.76 | 0.00

Source Energy End Use Components Per Total Floor Area

| Source Electricity [MJ/m2] | Source Natural Gas [MJ/m2] | Source Gasoline [MJ/m2] | Source Diesel [MJ/m2] | Source Coal [MJ/m2] | Source Fuel Oil No 1 [MJ/m2] | Source Fuel Oil No 2 [MJ/m2] | Source Propane [MJ/m2] | Source Other Fuel 1 [MJ/m2] | Source Other Fuel 2 [MJ/m2] | Source District Cooling [MJ/m2] | Source District Heating Water [MJ/m2] | Source District Heating Steam [MJ/m2]
Heating | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1718.90 | 0.00
Cooling | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 26.70 | 0.00 | 0.00
Interior Lighting | 312.72 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 277.47 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 590.20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 26.70 | 1718.90 | 0.00

Table of Contents

Report: Component Sizing Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Table of Contents

Report: Surface Shadowing Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Surfaces (Walls, Roofs, etc) that may be Shadowed by Other Surfaces

| None

Subsurfaces (Windows and Doors) that may be Shadowed by Surfaces

| Possible Shadow Receivers
FACE 61 | FACE 62 |
FACE 16 | FACE 17 |
FACE 36 | FACE 37 |
FACE 5 | FACE 6 |
FACE 88 | FACE 89 |
FACE 65 | FACE 66 |
FACE 94 | FACE 95 |
FACE 76 | FACE 77 |

Table of Contents

Report: Adaptive Comfort Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Time Not Meeting the Adaptive Comfort Models during Occupied Hours

| ASHRAE55 90% Acceptability Limits [Hours] | ASHRAE55 80% Acceptability Limits [Hours] | CEN15251 Category I Acceptability Limits [Hours] | CEN15251 Category II Acceptability Limits [Hours] | CEN15251 Category III Acceptability Limits [Hours]

Table of Contents

Report: Initialization Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Version

| Version ID
1 | 24.2

Timesteps per Hour

| #TimeSteps | Minutes per TimeStep {minutes}
1 | 6 | 10

System Convergence Limits

| Minimum System TimeStep {minutes} | Max HVAC Iterations | Minimum Plant Iterations | Maximum Plant Iterations
1 | 1 | 20 | 2 | 8

Simulation Control

| Do Zone Sizing | Do System Sizing | Do Plant Sizing | Do Design Days | Do Weather Simulation | Do HVAC Sizing Simulation
1 | No | No | No | Yes | Yes | No

Performance Precision Tradeoffs

| Use Coil Direct Simulation | Zone Radiant Exchange Algorithm | Override Mode | Number of Timestep In Hour | Force Euler Method | Minimum Number of Warmup Days | Force Suppress All Begin Environment Resets | Minimum System Timestep | MaxZoneTempDiff | MaxAllowedDelTemp
1 | No | ScriptF | Normal | 6 | No | 1 | No | 1.0 | 0.300 | 2.0000E-003

Output Reporting Tolerances

| Tolerance for Time Heating Setpoint Not Met | Tolerance for Zone Cooling Setpoint Not Met Time
1 | 0.200 | 0.200

Site:GroundTemperature:BuildingSurface

| Jan{C} | Feb{C} | Mar{C} | Apr{C} | May{C} | Jun{C} | Jul{C} | Aug{C} | Sep{C} | Oct{C} | Nov{C} | Dec{C}
1 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00 | 18.00

Site:GroundTemperature:FCfactorMethod

| Jan{C} | Feb{C} | Mar{C} | Apr{C} | May{C} | Jun{C} | Jul{C} | Aug{C} | Sep{C} | Oct{C} | Nov{C} | Dec{C}
1 | 2.39 | 1.46 | 3.10 | 5.66 | 12.35 | 17.52 | 21.00 | 22.06 | 20.26 | 16.25 | 10.89 | 5.91

Site:GroundTemperature:Shallow

| Jan{C} | Feb{C} | Mar{C} | Apr{C} | May{C} | Jun{C} | Jul{C} | Aug{C} | Sep{C} | Oct{C} | Nov{C} | Dec{C}
1 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00 | 13.00

Site:GroundTemperature:Deep

| Jan{C} | Feb{C} | Mar{C} | Apr{C} | May{C} | Jun{C} | Jul{C} | Aug{C} | Sep{C} | Oct{C} | Nov{C} | Dec{C}
1 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00 | 16.00

Site:GroundReflectance

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Site:GroundReflectance:SnowModifier

| Normal | Daylighting {dimensionless}
1 | 1.000 | 1.000

Site:GroundReflectance:Snow

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Site:GroundReflectance:Snow:Daylighting

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Environment:Weather Station

| Wind Sensor Height Above Ground {m} | Wind Speed Profile Exponent {} | Wind Speed Profile Boundary Layer Thickness {m} | Air Temperature Sensor Height Above Ground {m} | Wind Speed Modifier Coefficient-Internal | Temperature Modifier Coefficient-Internal
1 | 10.000 | 0.140 | 270.000 | 1.500 | 1.586 | 9.750E-003

Site:Location

| Location Name | Latitude {N+/S- Deg} | Longitude {E+/W- Deg} | Time Zone Number {GMT+/-} | Elevation {m} | Standard Pressure at Elevation {Pa} | Standard RhoAir at Elevation
1 | MILAN - ITA IWEC Data WMO#=160660 | 45.62 | 8.73 | 1.00 | 211.00 | 98816 | 1.1745

Site Water Mains Temperature Information

| Calculation Method{} | Water Mains Temperature Schedule Name{} | Annual Average Outdoor Air Temperature{C} | Maximum Difference In Monthly Average Outdoor Air Temperatures{deltaC} | Fixed Default Water Mains Temperature{C}
1 | FixedDefault | NA | NA | NA | 10.0

Building Information

| Building Name | North Axis {deg} | Terrain | Loads Convergence Tolerance Value | Temperature Convergence Tolerance Value | Solar Distribution | Maximum Number of Warmup Days | Minimum Number of Warmup Days
1 | Two story apartment | -45.000 | Suburbs | 4.00000E-002 | 0.40000 | FullExterior | 25 | 1

Inside Convection Algorithm

| Algorithm {Simple TARP CeilingDiffuser AdaptiveConvectionAlgorithm}
1 | TARP

Outside Convection Algorithm

| Algorithm {SimpleCombined TARP MoWitt DOE-2 AdaptiveConvectionAlgorithm}
1 | DOE-2

Sky Radiance Distribution

| Value {Anisotropic}
1 | Anisotropic

Zone Air Solution Algorithm

| Algorithm {ThirdOrderBackwardDifference AnalyticalSolution EulerMethod} | Space Heat Balance Sizing | Space Heat Balance Simulation
1 | ThirdOrderBackwardDifference | No | No

Zone Air Carbon Dioxide Balance Simulation

| Simulation {Yes/No} | Carbon Dioxide Concentration
1 | No | N/A

Zone Air Generic Contaminant Balance Simulation

| Simulation {Yes/No} | Generic Contaminant Concentration
1 | No | N/A

Zone Air Mass Flow Balance Simulation

| Enforce Mass Balance | Adjust Zone Mixing and Return {AdjustMixingOnly AdjustReturnOnly AdjustMixingThenReturn AdjustReturnThenMixing None} | Adjust Zone Infiltration {AddInfiltration AdjustInfiltration None} | Infiltration Zones {MixingSourceZonesOnly AllZones}
1 | No | N/A | N/A | N/A

HVACSystemRootFindingAlgorithm

| Value {RegulaFalsi Bisection BisectionThenRegulaFalsi RegulaFalsiThenBisection}
1 | RegulaFalsi

Environment:Site Atmospheric Variation

| Wind Speed Profile Exponent {} | Wind Speed Profile Boundary Layer Thickness {m} | Air Temperature Gradient Coefficient {K/m}
1 | 0.220 | 370.000 | 6.500000E-003

Shadowing/Sun Position Calculations Annual Simulations

| Shading Calculation Method | Shading Calculation Update Frequency Method | Shading Calculation Update Frequency {days} | Maximum Figures in Shadow Overlap Calculations {} | Polygon Clipping Algorithm | Pixel Counting Resolution | Sky Diffuse Modeling Algorithm | Output External Shading Calculation Results | Disable Self-Shading Within Shading Zone Groups | Disable Self-Shading From Shading Zone Groups to Other Zones
1 | PolygonClipping | Periodic | 20 | 15000 | SutherlandHodgman | 512 | SimpleSkyDiffuseModeling | No | No | No

Surface Geometry

| Starting Corner | Vertex Input Direction | Coordinate System | Daylight Reference Point Coordinate System | Rectangular (Simple) Surface Coordinate System
1 | UpperLeftCorner | Counterclockwise | RelativeCoordinateSystem | RelativeCoordinateSystem | RelativeToZoneOrigin

Surface Heat Transfer Algorithm

| Value {CTF - ConductionTransferFunction EMPD - MoisturePenetrationDepthConductionTransferFunction CondFD - ConductionFiniteDifference HAMT - CombinedHeatAndMoistureFiniteElement} - Description | Inside Surface Max Temperature Limit{C} | Surface Convection Coefficient Lower Limit {W/m2-K} | Surface Convection Coefficient Upper Limit {W/m2-K}
1 | CTF - ConductionTransferFunction | 200 | 0.10 | 1000.0

Shading Summary

| Number of Fixed Detached Shades | Number of Building Detached Shades | Number of Attached Shades
1 | 0 | 0 | 0

Zone Summary

| Number of Zones | Number of Zone Surfaces | Number of SubSurfaces
1 | 8 | 78 | 20

Zone Information

| Zone Name | North Axis {deg} | Origin X-Coordinate {m} | Origin Y-Coordinate {m} | Origin Z-Coordinate {m} | Centroid X-Coordinate {m} | Centroid Y-Coordinate {m} | Centroid Z-Coordinate {m} | Type | Zone Multiplier | Zone List Multiplier | Minimum X {m} | Maximum X {m} | Minimum Y {m} | Maximum Y {m} | Minimum Z {m} | Maximum Z {m} | Ceiling Height {m} | Volume {m3} | Zone Inside Convection Algorithm {Simple-Detailed-CeilingDiffuser-TrombeWall} | Zone Outside Convection Algorithm {Simple-Detailed-Tarp-MoWitt-DOE-2-BLAST} | Floor Area {m2} | Exterior Gross Wall Area {m2} | Exterior Net Wall Area {m2} | Exterior Window Area {m2} | Number of Surfaces | Number of SubSurfaces | Number of Shading SubSurfaces | Part of Total Building Area
1 | TZ_0-A1.B | 0.0 | 0.00 | 0.00 | 0.00 | 4.12 | 10.82 | 1.35 | 1 | 1 | 1 | 0.32 | 7.11 | 7.35 | 14.85 | 0.00 | 2.70 | 2.70 | 66.63 | TARP | DOE-2 | 24.68 | 25.92 | 23.68 | 2.24 | 8 | 2 | 0 | Yes
2 | TZ_0-A1.LK | 0.0 | 0.00 | 0.00 | 0.00 | 1.15 | 6.81 | 1.35 | 1 | 1 | 1 | -3.68 | 5.98 | 1.98 | 11.63 | 0.00 | 2.70 | 2.70 | 122.04 | TARP | DOE-2 | 45.20 | 30.51 | 27.15 | 3.36 | 7 | 3 | 0 | Yes
3 | TZ_0-A1.WC | 0.0 | 0.00 | 0.00 | 0.00 | 6.55 | 8.62 | 1.35 | 1 | 1 | 1 | 4.60 | 9.19 | 5.98 | 11.28 | 0.00 | 2.70 | 2.70 | 31.65 | TARP | DOE-2 | 11.72 | 20.25 | 19.13 | 1.12 | 8 | 3 | 0 | Yes
4 | TZ_0-H | 0.0 | 0.00 | 0.00 | 0.00 | -1.84 | 3.82 | 1.35 | 1 | 1 | 1 | -5.66 | 1.98 | 0.00 | 7.64 | 0.00 | 2.70 | 2.70 | 60.48 | TARP | DOE-2 | 22.40 | 36.72 | 30.96 | 5.76 | 6 | 2 | 0 | Yes
5 | TZ_1-A2.B | 0.0 | 0.00 | 0.00 | 0.00 | 4.12 | 10.82 | 4.05 | 1 | 1 | 1 | 0.32 | 7.11 | 7.35 | 14.85 | 2.70 | 5.40 | 2.70 | 66.63 | TARP | DOE-2 | 24.68 | 25.92 | 23.68 | 2.24 | 8 | 2 | 0 | Yes
6 | TZ_1-A2.LK | 0.0 | 0.00 | 0.00 | 0.00 | 1.15 | 6.81 | 4.05 | 1 | 1 | 1 | -3.68 | 5.98 | 1.98 | 11.63 | 2.70 | 5.40 | 2.70 | 122.04 | TARP | DOE-2 | 45.20 | 30.51 | 27.15 | 3.36 | 7 | 3 | 0 | Yes
7 | TZ_1-A2.WC | 0.0 | 0.00 | 0.00 | 0.00 | 6.55 | 8.62 | 4.05 | 1 | 1 | 1 | 4.60 | 9.19 | 5.98 | 11.28 | 2.70 | 5.40 | 2.70 | 31.65 | TARP | DOE-2 | 11.72 | 20.25 | 19.13 | 1.12 | 8 | 3 | 0 | Yes
8 | TZ_1-H | 0.0 | 0.00 | 0.00 | 0.00 | -1.84 | 3.82 | 4.05 | 1 | 1 | 1 | -5.66 | 1.98 | 0.00 | 7.64 | 2.70 | 5.40 | 2.70 | 60.48 | TARP | DOE-2 | 22.40 | 36.72 | 34.48 | 2.24 | 6 | 2 | 0 | Yes

Zone Internal Gains Nominal

| Zone Name | Floor Area {m2} | # Occupants | Area per Occupant {m2/person} | Occupant per Area {person/m2} | Interior Lighting {W/m2} | Electric Load {W/m2} | Gas Load {W/m2} | Other Load {W/m2} | Hot Water Eq {W/m2} | Steam Equipment {W/m2} | Sum Loads per Area {W/m2} | Outdoor Controlled Baseboard Heat
1 | TZ_0-A1.B | 24.68 | 0.7 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
2 | TZ_0-A1.LK | 45.20 | 1.3 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
3 | TZ_0-A1.WC | 11.72 | 0.3 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
4 | TZ_0-H | 22.40 | 0.0 | N/A | 0.000 | 9.903 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 9.903 | No
5 | TZ_1-A2.B | 24.68 | 0.7 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
6 | TZ_1-A2.LK | 45.20 | 1.3 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
7 | TZ_1-A2.WC | 11.72 | 0.3 | 35.324 | 2.831E-002 | 3.875 | 5.382 | 0.000 | 0.000 | 0.000 | 0.000 | 9.257 | No
8 | TZ_1-H | 22.40 | 0.0 | N/A | 0.000 | 9.903 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 9.903 | No

People Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {m2} | # Zone Occupants | Number of People {} | People/Floor Area {person/m2} | Floor Area per person {m2/person} | Fraction Radiant | Fraction Convected | Sensible Fraction Calculation | Activity level | ASHRAE 55 Warnings | Carbon Dioxide Generation Rate | Minimum Number of People for All Day Types | Maximum Number of People for All Day Types | Minimum Number of People for Weekdays | Maximum Number of People for Weekdays | Minimum Number of People for Weekends/Holidays | Maximum Number of People for Weekends /Holidays | Minimum Number of People for Summer Design Days | Maximum Number of People for Summer Design Days | Minimum Number of People for Winter Design Days | Maximum Number of People for Winter Design Days
1 | 1-A2.WC MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.WC | 11.72 | 0.3 | 0.3 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3
2 | 1-A2.LK MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.LK | 45.20 | 1.3 | 1.3 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3
3 | 0-A1.WC MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.WC | 11.72 | 0.3 | 0.3 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3 | 8.3E-002 | 0.3
4 | 1-A2.B MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.B | 24.68 | 0.7 | 0.7 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7
5 | 0-A1.B MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.B | 24.68 | 0.7 | 0.7 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7 | 0.2 | 0.7
6 | 0-A1.LK MIDRISEAPARTMENT APARTMENT PEOPLE | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.LK | 45.20 | 1.3 | 1.3 | 2.831E-002 | 35.324 | 0.300 | 0.700 | AutoCalculate | MIDRISEAPARTMENT ACTIVITY | No | 3.8200E-008 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3 | 0.3 | 1.3

Lights Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {m2} | # Zone Occupants | Lighting Level {W} | Lights/Floor Area {W/m2} | Lights per person {W/person} | Fraction Return Air | Fraction Radiant | Fraction Short Wave | Fraction Convected | Fraction Replaceable | End-Use | Minimum Lighting Level for All Day Types {W} | Maximum Lighting Level for All Day Types {W} | Minimum Lighting Level for Weekdays {W} | Maximum Lighting Level for Weekdays {W} | Minimum Lighting Level for Weekends/Holidays {W} | Maximum Lighting Level for Weekends /Holidays {W} | Minimum Lighting Level for Summer Design Days {W} | Maximum Lighting Level for Summer Design Days {W} | Minimum Lighting Level for Winter Design Days {W} | Maximum Lighting Level for Winter Design Days {W}
1 | 1-A2.WC MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_1-A2.WC | 11.72 | 0.3 | 45.425 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 3.043 | 45.425 | 3.043 | 45.4 | 3.043 | 45.425 | 3.043 | 45.425 | 3.043 | 45.425
2 | 1-A2.LK MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_1-A2.LK | 45.20 | 1.3 | 175.150 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 11.735 | 175.150 | 11.735 | 175.2 | 11.735 | 175.150 | 11.735 | 175.150 | 11.735 | 175.150
3 | 0-A1.WC MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_0-A1.WC | 11.72 | 0.3 | 45.425 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 3.043 | 45.425 | 3.043 | 45.4 | 3.043 | 45.425 | 3.043 | 45.425 | 3.043 | 45.425
4 | 1-A2.B MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_1-A2.B | 24.68 | 0.7 | 95.626 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 6.407 | 95.626 | 6.407 | 95.6 | 6.407 | 95.626 | 6.407 | 95.626 | 6.407 | 95.626
5 | 0-A1.B MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_0-A1.B | 24.68 | 0.7 | 95.626 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 6.407 | 95.626 | 6.407 | 95.6 | 6.407 | 95.626 | 6.407 | 95.626 | 6.407 | 95.626
6 | 0-A1.LK MIDRISEAPARTMENT APARTMENT LIGHTS | MIDRISEAPARTMENT APARTMENT LIGHT | TZ_0-A1.LK | 45.20 | 1.3 | 175.150 | 3.875 | 136.882 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 11.735 | 175.150 | 11.735 | 175.2 | 11.735 | 175.150 | 11.735 | 175.150 | 11.735 | 175.150
7 | 1-H MIDRISEAPARTMENT CORRIDOR LIGHTS | MIDRISEAPARTMENT CORRIDOR LIGHT | TZ_1-H | 22.40 | 0.0 | 221.823 | 9.903 | N/A | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 221.823 | 221.823 | 221.823 | 221.8 | 221.823 | 221.823 | 221.823 | 221.823 | 221.823 | 221.823
8 | 0-H MIDRISEAPARTMENT CORRIDOR LIGHTS | MIDRISEAPARTMENT CORRIDOR LIGHT | TZ_0-H | 22.40 | 0.0 | 221.823 | 9.903 | N/A | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | General | 221.823 | 221.823 | 221.823 | 221.8 | 221.823 | 221.823 | 221.823 | 221.823 | 221.823 | 221.823

ElectricEquipment Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {m2} | # Zone Occupants | Equipment Level {W} | Equipment/Floor Area {W/m2} | Equipment per person {W/person} | Fraction Latent | Fraction Radiant | Fraction Lost | Fraction Convected | End-Use SubCategory | Minimum Equipment Level for All Day Types {W} | Maximum Equipment Level for All Day Types {W} | Minimum Equipment Level for Weekdays {W} | Maximum Equipment Level for Weekdays {W} | Minimum Equipment Level for Weekends/Holidays {W} | Maximum Equipment Level for Weekends /Holidays {W} | Minimum Equipment Level for Summer Design Days {W} | Maximum Equipment Level for Summer Design Days {W} | Minimum Equipment Level for Winter Design Days {W} | Maximum Equipment Level for Winter Design Days {W}
1 | 1-A2.WC MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_1-A2.WC | 11.72 | 0.3 | 63.090 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090
2 | 1-A2.LK MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_1-A2.LK | 45.20 | 1.3 | 243.264 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264
3 | 0-A1.WC MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_0-A1.WC | 11.72 | 0.3 | 63.090 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090 | 23.974 | 63.090
4 | 1-A2.B MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_1-A2.B | 24.68 | 0.7 | 132.813 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813
5 | 0-A1.B MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_0-A1.B | 24.68 | 0.7 | 132.813 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813 | 50.469 | 132.813
6 | 0-A1.LK MIDRISEAPARTMENT APARTMENT ELEC EQUIP | APARTMENTMIDRISE EQP_APT_SCH | TZ_0-A1.LK | 45.20 | 1.3 | 243.264 | 5.382 | 190.114 | 0.000 | 0.500 | 0.000 | 0.500 | General | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264 | 92.440 | 243.264

ZoneInfiltration Airflow Stats Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {m2} | # Zone Occupants | Design Volume Flow Rate {m3/s} | Volume Flow Rate/Floor Area {m3/s-m2} | Volume Flow Rate/Exterior Surface Area {m3/s-m2} | ACH - Air Changes per Hour | Equation A - Constant Term Coefficient {} | Equation B - Temperature Term Coefficient {1/C} | Equation C - Velocity Term Coefficient {s/m} | Equation D - Velocity Squared Term Coefficient {s2/m2}
1 | 1-A2.WC MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_1-A2.WC | 11.72 | 0.3 | 2.294E-002 | 1.957E-003 | 7.175E-004 | 2.609 | 1.000 | 0.000 | 0.000 | 0.000
2 | 1-A2.LK MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_1-A2.LK | 45.20 | 1.3 | 3.456E-002 | 7.647E-004 | 4.565E-004 | 1.020 | 1.000 | 0.000 | 0.000 | 0.000
3 | 0-A1.WC MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_0-A1.WC | 11.72 | 0.3 | 2.294E-002 | 1.957E-003 | 1.133E-003 | 2.609 | 1.000 | 0.000 | 0.000 | 0.000
4 | 1-A2.B MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_1-A2.B | 24.68 | 0.7 | 2.936E-002 | 1.190E-003 | 5.803E-004 | 1.587 | 1.000 | 0.000 | 0.000 | 0.000
5 | 0-A1.B MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_0-A1.B | 24.68 | 0.7 | 2.936E-002 | 1.190E-003 | 1.133E-003 | 1.587 | 1.000 | 0.000 | 0.000 | 0.000
6 | 0-A1.LK MIDRISEAPARTMENT APARTMENT INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_0-A1.LK | 45.20 | 1.3 | 3.456E-002 | 7.647E-004 | 1.133E-003 | 1.020 | 1.000 | 0.000 | 0.000 | 0.000
7 | 1-H MIDRISEAPARTMENT CORRIDOR INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_1-H | 22.40 | 0.0 | 4.160E-002 | 1.857E-003 | 7.036E-004 | 2.476 | 1.000 | 0.000 | 0.000 | 0.000
8 | 0-H MIDRISEAPARTMENT CORRIDOR INFILTRATION | MIDRISEAPARTMENT INFIL | TZ_0-H | 22.40 | 0.0 | 4.160E-002 | 1.857E-003 | 1.133E-003 | 2.476 | 1.000 | 0.000 | 0.000 | 0.000

ZoneVentilation Airflow Stats Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {m2} | # Zone Occupants | Design Volume Flow Rate {m3/s} | Volume Flow Rate/Floor Area {m3/s-m2} | Volume Flow Rate/person Area {m3/s-person} | ACH - Air Changes per Hour | Fan Type {Exhaust;Intake;Natural} | Fan Pressure Rise {Pa} | Fan Efficiency {} | Equation A - Constant Term Coefficient {} | Equation B - Temperature Term Coefficient {1/C} | Equation C - Velocity Term Coefficient {s/m} | Equation D - Velocity Squared Term Coefficient {s2/m2} | Minimum Indoor Temperature{C}/Schedule | Maximum Indoor Temperature{C}/Schedule | Delta Temperature{C}/Schedule | Minimum Outdoor Temperature{C}/Schedule | Maximum Outdoor Temperature{C}/Schedule | Maximum WindSpeed{m/s}
1 | TZ_0-A1.B VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.B | 24.68 | 0.7 | 1.187E-002 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00
2 | TZ_0-A1.LK VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.LK | 45.20 | 1.3 | 2.174E-002 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00
3 | TZ_0-A1.WC VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_0-A1.WC | 11.72 | 0.3 | 5.638E-003 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00
4 | TZ_1-A2.B VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.B | 24.68 | 0.7 | 1.187E-002 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00
5 | TZ_1-A2.LK VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.LK | 45.20 | 1.3 | 2.174E-002 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00
6 | TZ_1-A2.WC VENTILATION PER PERSON | MIDRISEAPARTMENT APARTMENT OCC | TZ_1-A2.WC | 11.72 | 0.3 | 5.638E-003 | 4.810E-004 | 1.699E-002 | 0.641 | Natural | 0.000 | 1.0 | 1.000 | 0.000 | 0.000 | 0.000 | -100.00 | 100.00 | -100.00 | -100.00 | 100.00 | 40.00

AirFlow Model

| Simple
1 | Simple

RoomAir Model

| Zone Name | Mixing/Mundt/UCSDDV/UCSDCV/UCSDUFI/UCSDUFE/User Defined
1 | TZ_0-A1.B | Mixing/Well-Stirred
2 | TZ_0-A1.LK | Mixing/Well-Stirred
3 | TZ_0-A1.WC | Mixing/Well-Stirred
4 | TZ_0-H | Mixing/Well-Stirred
5 | TZ_1-A2.B | Mixing/Well-Stirred
6 | TZ_1-A2.LK | Mixing/Well-Stirred
7 | TZ_1-A2.WC | Mixing/Well-Stirred
8 | TZ_1-H | Mixing/Well-Stirred

AirflowNetwork Model:Control

| No Multizone or Distribution/Multizone with Distribution/Multizone without Distribution/Multizone with Distribution only during Fan Operation
1 | NoMultizoneOrDistribution

Zone Volume Capacitance Multiplier

| Sensible Heat Capacity Multiplier | Moisture Capacity Multiplier | Carbon Dioxide Capacity Multiplier | Generic Contaminant Capacity Multiplier
1 | 1.000 | 1.000 | 1.000 | 1.000

Environment

| Environment Name | Environment Type | Start Date | End Date | Start DayOfWeek | Duration {#days} | Source:Start DayOfWeek | Use Daylight Saving | Use Holidays | Apply Weekend Holiday Rule | Use Rain Values | Use Snow Values | Sky Temperature Model
1 | RUN PERIOD 1 | WeatherFileRunPeriod | 01/01/2006 | 12/31/2006 | Sunday | 365 | Use RunPeriod Specified Day | No | No | No | Yes | Yes | Clark and Allen

Environment:Daylight Saving

| Daylight Saving Indicator | Source | Start Date | End Date
1 | No | RunPeriod Object |  |

Environment:WarmupDays

| NumberofWarmupDays
1 | 3

Tabular Report

| Style | Unit Conversion
1 | HTML | None

Warmup Convergence Information

| Zone Name | Environment Type/Name | Average Warmup Temperature Difference {deltaC} | Std Dev Warmup Temperature Difference {deltaC} | Max Temperature Pass/Fail Convergence | Min Temperature Pass/Fail Convergence | Average Warmup Load Difference {W} | Std Dev Warmup Load Difference {W} | Heating Load Pass/Fail Convergence | Cooling Load Pass/Fail Convergence
1 | TZ_0-A1.B | RunPeriod: RUN PERIOD 1 | 2.8125649957E-015 | 2.5077827735E-015 | Pass | Pass | 9.4580939019E-003 | 1.2372011297E-002 | Pass | Pass
2 | TZ_0-A1.LK | RunPeriod: RUN PERIOD 1 | 2.4178190314E-015 | 2.4646938799E-015 | Pass | Pass | 1.0701214396E-002 | 1.4780426427E-002 | Pass | Pass
3 | TZ_0-A1.WC | RunPeriod: RUN PERIOD 1 | 2.3684757859E-015 | 2.5467998871E-015 | Pass | Pass | 8.9014758115E-003 | 9.4112009438E-003 | Pass | Pass
4 | TZ_0-H | RunPeriod: RUN PERIOD 1 | 6.1540942109E-002 | 5.4425444127E-002 | Pass | Pass | 0.0000000000 | 0.0000000000 | Pass | Pass
5 | TZ_1-A2.B | RunPeriod: RUN PERIOD 1 | 2.7632217502E-015 | 2.5620503222E-015 | Pass | Pass | 1.0842778217E-002 | 1.2072100036E-002 | Pass | Pass
6 | TZ_1-A2.LK | RunPeriod: RUN PERIOD 1 | 2.6151920136E-015 | 2.1343449234E-015 | Pass | Pass | 1.2342606550E-002 | 1.3810584922E-002 | Pass | Pass
7 | TZ_1-A2.WC | RunPeriod: RUN PERIOD 1 | 2.6892068819E-015 | 2.4502039327E-015 | Pass | Pass | 1.0022103323E-002 | 9.7993503863E-003 | Pass | Pass
8 | TZ_1-H | RunPeriod: RUN PERIOD 1 | 6.5230391682E-002 | 5.7175040416E-002 | Pass | Pass | 0.0000000000 | 0.0000000000 | Pass | Pass

Table of Contents

Report: Annual Heat Emissions Report

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Annual Heat Emissions Summary

| Envelope Convection | Zone Exfiltration | Zone Exhaust Air | HVAC Relief Air | HVAC Reject Heat | Total
Heat Emissions [GJ] | 258.87 | 108.45 | 0.00 | 0.00 | 0.00 | 367.32

Table of Contents

Report: Annual Thermal Resilience Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Heat Index Hours

| Safe (≤ 26.7°C) [hr] | Caution (> 26.7°C, ≤ 32.2°C) [hr] | Extreme Caution (> 32.2°C, ≤ 39.4°C) [hr] | Danger (> 39.4°C, ≤ 51.7°C) [hr] | Extreme Danger (> 51.7°C) [hr]
TZ_0-A1.B | 8756.17 | 3.83 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 8756.67 | 3.33 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 8755.67 | 4.33 | 0.00 | 0.00 | 0.00
TZ_0-H | 8133.33 | 606.83 | 19.83 | 0.00 | 0.00
TZ_1-A2.B | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 7589.67 | 974.33 | 195.17 | 0.83 | 0.00
Min | 7589.67 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8760.00 | 974.33 | 195.17 | 0.83 | 0.00
Average | 8533.94 | 199.08 | 26.87 | 0.10 | 0.00
Sum | 68271.50 | 1592.67 | 215.00 | 0.83 | 0.00

Heat Index OccupantHours

| Safe (≤ 26.7°C) [hr] | Caution (> 26.7°C, ≤ 32.2°C) [hr] | Extreme Caution (> 32.2°C, ≤ 39.4°C) [hr] | Danger (> 39.4°C, ≤ 51.7°C) [hr] | Extreme Danger (> 51.7°C) [hr]
TZ_0-A1.B | 4185.73 | 1.17 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 7667.08 | 1.77 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 1988.26 | 0.64 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 4186.90 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 7668.85 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 1988.90 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 7668.85 | 1.77 | 0.00 | 0.00 | 0.00
Average | 3460.71 | 0.45 | 0.00 | 0.00 | 0.00
Sum | 27685.72 | 3.58 | 0.00 | 0.00 | 0.00

Heat Index OccupiedHours

| Safe (≤ 26.7°C) [hr] | Caution (> 26.7°C, ≤ 32.2°C) [hr] | Extreme Caution (> 32.2°C, ≤ 39.4°C) [hr] | Danger (> 39.4°C, ≤ 51.7°C) [hr] | Extreme Danger (> 51.7°C) [hr]
TZ_0-A1.B | 8756.17 | 3.83 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 8756.67 | 3.33 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 8755.67 | 4.33 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8760.00 | 4.33 | 0.00 | 0.00 | 0.00
Average | 6568.56 | 1.44 | 0.00 | 0.00 | 0.00
Sum | 52548.50 | 11.50 | 0.00 | 0.00 | 0.00

Humidex Hours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
TZ_0-A1.B | 7912.67 | 847.33 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 7845.50 | 914.50 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 7912.83 | 847.17 | 0.00 | 0.00 | 0.00
TZ_0-H | 7481.83 | 1276.33 | 1.83 | 0.00 | 0.00
TZ_1-A2.B | 7687.83 | 1072.17 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 7667.67 | 1092.33 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 7718.50 | 1041.50 | 0.00 | 0.00 | 0.00
TZ_1-H | 7095.67 | 1609.00 | 55.33 | 0.00 | 0.00
Min | 7095.67 | 847.17 | 0.00 | 0.00 | 0.00
Max | 7912.83 | 1609.00 | 55.33 | 0.00 | 0.00
Average | 7665.31 | 1087.54 | 7.15 | 0.00 | 0.00
Sum | 61322.50 | 8700.33 | 57.17 | 0.00 | 0.00

Humidex OccupantHours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
TZ_0-A1.B | 3811.04 | 375.87 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 6907.33 | 761.52 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 1817.71 | 171.19 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 3719.76 | 467.14 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 6762.01 | 906.84 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 1777.01 | 211.89 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 6907.33 | 906.84 | 0.00 | 0.00 | 0.00
Average | 3099.36 | 361.81 | 0.00 | 0.00 | 0.00
Sum | 24794.86 | 2894.44 | 0.00 | 0.00 | 0.00

Humidex OccupiedHours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
TZ_0-A1.B | 7912.67 | 847.33 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 7845.50 | 914.50 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 7912.83 | 847.17 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 7687.83 | 1072.17 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 7667.67 | 1092.33 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 7718.50 | 1041.50 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 7912.83 | 1092.33 | 0.00 | 0.00 | 0.00
Average | 5843.13 | 726.87 | 0.00 | 0.00 | 0.00
Sum | 46745.00 | 5815.00 | 0.00 | 0.00 | 0.00

Hours of Safety for Cold Events

| Hours of Safety [hr] | End Time of the Safety Duration | Safe Temperature Exceedance Hours [hr] | Safe Temperature Exceedance OccupantHours [hr] | Safe Temperature Exceedance OccupiedHours [hr]
TZ_0-A1.B | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | - | 0.00 | 0.00 | 0.00
Min | 0.00 | - | 0.00 | 0.00 | 0.00
Max | 8760.00 | - | 0.00 | 0.00 | 0.00
Average | 6570.00 | - | 0.00 | 0.00 | 0.00
Sum | 52560.00 | - | 0.00 | 0.00 | 0.00

Hours of Safety for Heat Events

| Hours of Safety [hr] | End Time of the Safety Duration | Safe Temperature Exceedance Hours [hr] | Safe Temperature Exceedance OccupantHours [hr] | Safe Temperature Exceedance OccupiedHours [hr]
TZ_0-A1.B | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 8760.00 | - | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | - | 0.00 | 0.00 | 0.00
Min | 0.00 | - | 0.00 | 0.00 | 0.00
Max | 8760.00 | - | 0.00 | 0.00 | 0.00
Average | 6570.00 | - | 0.00 | 0.00 | 0.00
Sum | 52560.00 | - | 0.00 | 0.00 | 0.00

Unmet Degree-Hours

| Cooling Setpoint Unmet Degree-Hours [°C·hr] | Cooling Setpoint Unmet Occupant-Weighted Degree-Hours [°C·hr] | Cooling Setpoint Unmet Occupied Degree-Hours [°C·hr] | Heating Setpoint Unmet Degree-Hours [°C·hr] | Heating Setpoint Unmet Occupant-Weighted Degree-Hours [°C·hr] | Heating Setpoint Unmet Occupied Degree-Hours [°C·hr]
TZ_0-A1.B | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Average | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Sum | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Discomfort-weighted Exceedance OccupantHours

| Very-cold Exceedance OccupantHours [hr] | Cool Exceedance OccupantHours [hr] | Warm Exceedance OccupantHours [hr] | Very-hot Exceedance OccupantHours [hr]
TZ_0-A1.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.00 | 0.00 | 0.00 | 0.00
Average | 0.00 | 0.00 | 0.00 | 0.00
Sum | 0.00 | 0.00 | 0.00 | 0.00

Discomfort-weighted Exceedance OccupiedHours

| Very-cold Exceedance OccupantHours [hr] | Cool Exceedance OccupantHours [hr] | Warm Exceedance OccupantHours [hr] | Very-hot Exceedance OccupantHours [hr]
TZ_0-A1.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.00 | 0.00 | 0.00 | 0.00
Average | 0.00 | 0.00 | 0.00 | 0.00
Sum | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Climatic Data Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

SizingPeriod:DesignDay

| Maximum Dry Bulb [C] | Daily Temperature Range [deltaC] | Humidity Value | Humidity Type | Wind Speed [m/s] | Wind Direction
None |  |  |  |  |  |

Monthly Precipitation Summary

| Monthly Total Precipitation from .epw [mm] | Monthly Total Hours of Rain from .epw | Monthly Total Precipitation in Site:Precipitation [mm] | Monthly Total Roof Irrigation Depth [mm] | Monthly Total Rain Collection Volume [m3]
Jan | 70.00 | 68 |  |  |
Feb | 44.00 | 44 |  |  |
Mar | 52.00 | 47 |  |  |
Apr | 102.00 | 95 |  |  |
May | 96.00 | 90 |  |  |
Jun | 46.00 | 46 |  |  |
Jul | 24.00 | 24 |  |  |
Aug | 42.00 | 42 |  |  |
Sep | 12.00 | 12 |  |  |
Oct | 60.00 | 58 |  |  |
Nov | 98.00 | 89 |  |  |
Dec | 14.00 | 14 |  |  |

Weather Statistics File

| Value
None |

Table of Contents

Report: Envelope Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Opaque Exterior

| Construction | Zone | Reflectance | U-Factor with Film [W/m2-K] | U-Factor no Film [W/m2-K] | Gross Area [m2] | Net Area [m2] | Azimuth [deg] | Tilt [deg] | Cardinal Direction
FACE 20 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.B | 0.30 | 0.505 | 0.547 | 13.64 | 13.64 | 45.00 | 90.00 | E
FACE 61 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.B | 0.30 | 0.505 | 0.547 | 12.29 | 10.05 | 315.00 | 90.00 | N
FACE 18 | TYPICAL INSULATED CARPETED 6IN SLAB FLOOR | TZ_0-A1.B | 0.30 | 2.250 | 3.540 | 24.68 | 24.68 | 315.00 | 180.00 |
FACE 13 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.LK | 0.30 | 0.505 | 0.547 | 15.25 | 15.25 | 135.00 | 90.00 | S
FACE 16 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.LK | 0.30 | 0.505 | 0.547 | 15.25 | 11.89 | 315.00 | 90.00 | N
FACE 8 | TYPICAL INSULATED CARPETED 6IN SLAB FLOOR | TZ_0-A1.LK | 0.30 | 2.250 | 3.540 | 45.20 | 45.20 | 225.00 | 180.00 |
FACE 36 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.WC | 0.30 | 0.505 | 0.547 | 7.96 | 6.84 | 45.00 | 90.00 | E
FACE 38 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-A1.WC | 0.30 | 0.505 | 0.547 | 12.29 | 12.29 | 135.00 | 90.00 | S
FACE 28 | TYPICAL INSULATED CARPETED 6IN SLAB FLOOR | TZ_0-A1.WC | 0.30 | 2.250 | 3.540 | 11.72 | 11.72 | 135.00 | 180.00 |
FACE 4 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-H | 0.30 | 0.505 | 0.547 | 7.56 | 7.56 | 135.00 | 90.00 | S
FACE 5 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-H | 0.30 | 0.505 | 0.547 | 21.60 | 15.84 | 225.00 | 90.00 | W
FACE 7 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_0-H | 0.30 | 0.505 | 0.547 | 7.56 | 7.56 | 315.00 | 90.00 | N
FACE 0 | TYPICAL INSULATED CARPETED 6IN SLAB FLOOR | TZ_0-H | 0.30 | 2.250 | 3.540 | 22.40 | 22.40 | 315.00 | 180.00 |
FACE 84 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.B | 0.30 | 0.505 | 0.547 | 13.64 | 13.64 | 45.00 | 90.00 | E
FACE 88 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.B | 0.30 | 0.505 | 0.547 | 12.29 | 10.05 | 315.00 | 90.00 | N
FACE 81 | TYPICAL IEAD ROOF R-17.24 10 | TZ_1-A2.B | 0.30 | 0.329 | 0.345 | 24.68 | 24.68 | 135.00 | 0.00 |
FACE 65 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.LK | 0.30 | 0.505 | 0.547 | 15.25 | 11.89 | 315.00 | 90.00 | N
FACE 68 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.LK | 0.30 | 0.505 | 0.547 | 15.25 | 15.25 | 135.00 | 90.00 | S
FACE 67 | TYPICAL IEAD ROOF R-17.24 10 | TZ_1-A2.LK | 0.30 | 0.329 | 0.345 | 45.20 | 45.20 | 135.00 | 0.00 |
FACE 94 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.WC | 0.30 | 0.505 | 0.547 | 7.96 | 6.84 | 45.00 | 90.00 | E
FACE 96 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-A2.WC | 0.30 | 0.505 | 0.547 | 12.29 | 12.29 | 135.00 | 90.00 | S
FACE 98 | TYPICAL IEAD ROOF R-17.24 10 | TZ_1-A2.WC | 0.30 | 0.329 | 0.345 | 11.72 | 11.72 | 315.00 | 0.00 |
FACE 76 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-H | 0.30 | 0.505 | 0.547 | 21.60 | 19.36 | 225.00 | 90.00 | W
FACE 78 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-H | 0.30 | 0.505 | 0.547 | 7.56 | 7.56 | 135.00 | 90.00 | S
FACE 79 | TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | TZ_1-H | 0.30 | 0.505 | 0.547 | 7.56 | 7.56 | 315.00 | 90.00 | N
FACE 40 | TYPICAL IEAD ROOF R-17.24 10 | TZ_1-H | 0.30 | 0.329 | 0.345 | 22.40 | 22.40 | 135.00 | 0.00 |

Opaque Interior

| Construction | Zone | Adjacent Surface | Reflectance | U-Factor with Film [W/m2-K] | U-Factor no Film [W/m2-K] | Gross Area [m2] | Net Area [m2] | Azimuth [deg] | Tilt [deg] | Cardinal Direction
FACE 58 | TYPICAL INTERIOR WALL | TZ_0-A1.B | FACE 32 | 0.30 | 2.511 | 6.300 | 4.59 | 2.91 | 135.00 | 90.00 | S
FACE 60 | TYPICAL INTERIOR WALL | TZ_0-A1.B | FACE 10 | 0.30 | 2.511 | 6.300 | 16.34 | 16.34 | 225.00 | 90.00 | W
FACE 63 | TYPICAL INTERIOR WALL | TZ_0-A1.B | FACE 35 | 0.30 | 2.511 | 6.300 | 7.70 | 7.70 | 135.00 | 90.00 | S
FACE 64 | TYPICAL INTERIOR WALL | TZ_0-A1.B | FACE 34 | 0.30 | 2.511 | 6.300 | 2.70 | 2.70 | 45.00 | 90.00 | E
FACE 19 | TYPICAL INTERIOR CEILING | TZ_0-A1.B | FACE 80 | 0.30 | 1.887 | 3.839 | 24.68 | 24.68 | 135.00 | 0.00 |
FACE 10 | TYPICAL INTERIOR WALL | TZ_0-A1.LK | FACE 60 | 0.30 | 2.511 | 6.300 | 16.34 | 16.34 | 45.00 | 90.00 | E
FACE 11 | TYPICAL INTERIOR WALL | TZ_0-A1.LK | FACE 30 | 0.30 | 2.511 | 6.300 | 5.26 | 3.59 | 45.00 | 90.00 | E
FACE 14 | TYPICAL INTERIOR WALL | TZ_0-A1.LK | FACE 2 | 0.30 | 2.511 | 6.300 | 21.60 | 19.71 | 225.00 | 90.00 | W
FACE 9 | TYPICAL INTERIOR CEILING | TZ_0-A1.LK | FACE 72 | 0.30 | 1.887 | 3.839 | 45.20 | 45.20 | 315.00 | 0.00 |
FACE 30 | TYPICAL INTERIOR WALL | TZ_0-A1.WC | FACE 11 | 0.30 | 2.511 | 6.300 | 5.26 | 3.59 | 225.00 | 90.00 | W
FACE 32 | TYPICAL INTERIOR WALL | TZ_0-A1.WC | FACE 58 | 0.30 | 2.511 | 6.300 | 4.59 | 2.91 | 315.00 | 90.00 | N
FACE 34 | TYPICAL INTERIOR WALL | TZ_0-A1.WC | FACE 64 | 0.30 | 2.511 | 6.300 | 2.70 | 2.70 | 225.00 | 90.00 | W
FACE 35 | TYPICAL INTERIOR WALL | TZ_0-A1.WC | FACE 63 | 0.30 | 2.511 | 6.300 | 7.70 | 7.70 | 315.00 | 90.00 | N
FACE 29 | TYPICAL INTERIOR CEILING | TZ_0-A1.WC | FACE 97 | 0.30 | 1.887 | 3.839 | 11.72 | 11.72 | 315.00 | 0.00 |
FACE 2 | TYPICAL INTERIOR WALL | TZ_0-H | FACE 14 | 0.30 | 2.511 | 6.300 | 21.60 | 19.71 | 45.00 | 90.00 | E
FACE 1 | TYPICAL INTERIOR CEILING | TZ_0-H | FACE 39 | 0.30 | 1.887 | 3.839 | 22.40 | 22.40 | 315.00 | 0.00 |
FACE 82 | TYPICAL INTERIOR WALL | TZ_1-A2.B | FACE 90 | 0.30 | 2.511 | 6.300 | 2.70 | 2.70 | 45.00 | 90.00 | E
FACE 83 | TYPICAL INTERIOR WALL | TZ_1-A2.B | FACE 69 | 0.30 | 2.511 | 6.300 | 16.34 | 16.34 | 225.00 | 90.00 | W
FACE 85 | TYPICAL INTERIOR WALL | TZ_1-A2.B | FACE 91 | 0.30 | 2.511 | 6.300 | 7.70 | 7.70 | 135.00 | 90.00 | S
FACE 86 | TYPICAL INTERIOR WALL | TZ_1-A2.B | FACE 92 | 0.30 | 2.511 | 6.300 | 4.59 | 2.91 | 135.00 | 90.00 | S
FACE 80 | TYPICAL INTERIOR FLOOR | TZ_1-A2.B | FACE 19 | 0.30 | 1.887 | 3.839 | 24.68 | 24.68 | 315.00 | 180.00 |
FACE 69 | TYPICAL INTERIOR WALL | TZ_1-A2.LK | FACE 83 | 0.30 | 2.511 | 6.300 | 16.34 | 16.34 | 45.00 | 90.00 | E
FACE 70 | TYPICAL INTERIOR WALL | TZ_1-A2.LK | FACE 99 | 0.30 | 2.511 | 6.300 | 5.26 | 3.59 | 45.00 | 90.00 | E
FACE 73 | TYPICAL INTERIOR WALL | TZ_1-A2.LK | FACE 41 | 0.30 | 2.511 | 6.300 | 21.60 | 19.71 | 225.00 | 90.00 | W
FACE 72 | TYPICAL INTERIOR FLOOR | TZ_1-A2.LK | FACE 9 | 0.30 | 1.887 | 3.839 | 45.20 | 45.20 | 315.00 | 180.00 |
FACE 90 | TYPICAL INTERIOR WALL | TZ_1-A2.WC | FACE 82 | 0.30 | 2.511 | 6.300 | 2.70 | 2.70 | 225.00 | 90.00 | W
FACE 91 | TYPICAL INTERIOR WALL | TZ_1-A2.WC | FACE 85 | 0.30 | 2.511 | 6.300 | 7.70 | 7.70 | 315.00 | 90.00 | N
FACE 92 | TYPICAL INTERIOR WALL | TZ_1-A2.WC | FACE 86 | 0.30 | 2.511 | 6.300 | 4.59 | 2.91 | 315.00 | 90.00 | N
FACE 99 | TYPICAL INTERIOR WALL | TZ_1-A2.WC | FACE 70 | 0.30 | 2.511 | 6.300 | 5.26 | 3.59 | 225.00 | 90.00 | W
FACE 97 | TYPICAL INTERIOR FLOOR | TZ_1-A2.WC | FACE 29 | 0.30 | 1.887 | 3.839 | 11.72 | 11.72 | 315.00 | 180.00 |
FACE 41 | TYPICAL INTERIOR WALL | TZ_1-H | FACE 73 | 0.30 | 2.511 | 6.300 | 21.60 | 19.71 | 45.00 | 90.00 | E
FACE 39 | TYPICAL INTERIOR FLOOR | TZ_1-H | FACE 1 | 0.30 | 1.887 | 3.839 | 22.40 | 22.40 | 315.00 | 180.00 |

Exterior Fenestration

| Construction | Frame and Divider | Glass Area [m2] | Frame Area [m2] | Divider Area [m2] | Area of One Opening [m2] | Area of Multiplied Openings [m2] | Glass U-Factor [W/m2-K] | Glass SHGC | Glass Visible Transmittance | Frame Conductance [W/m2-K] | Divider Conductance [W/m2-K] | NFRC Product Type | Assembly U-Factor [W/m2-K] | Assembly SHGC | Assembly Visible Transmittance | Shade Control | Parent Surface | Azimuth [deg] | Tilt [deg] | Cardinal Direction
FACE 62 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 2.24 | 0.00 | 0.00 | 2.24 | 2.24 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 61 | 315.00 | 90.00 | N
FACE 17 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 3.36 | 0.00 | 0.00 | 3.36 | 3.36 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 16 | 315.00 | 90.00 | N
FACE 37 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 1.12 | 0.00 | 0.00 | 1.12 | 1.12 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 36 | 45.00 | 90.00 | E
FACE 6 | U 0.88 SHGC 0.16 SGL REF-A-L CLR 6MM |  | 5.76 | 0.00 | 0.00 | 5.76 | 5.76 | 4.440 | 0.202 | 0.080 |  |  |  |  |  |  | No | FACE 5 | 225.00 | 90.00 | W
FACE 89 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 2.24 | 0.00 | 0.00 | 2.24 | 2.24 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 88 | 315.00 | 90.00 | N
FACE 66 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 3.36 | 0.00 | 0.00 | 3.36 | 3.36 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 65 | 315.00 | 90.00 | N
FACE 95 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 1.12 | 0.00 | 0.00 | 1.12 | 1.12 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 94 | 45.00 | 90.00 | E
FACE 77 | U 0.59 SHGC 0.36 SIMPLE GLAZING WINDOW U-0.59 SHGC 0.36 23 |  | 2.24 | 0.00 | 0.00 | 2.24 | 2.24 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  | No | FACE 76 | 225.00 | 90.00 | W
Total or Average |  |  |  |  |  |  | 21.44 | 3.646 | 0.318 | 0.220 |  |  |  |  |  |  |  |  |  |  |
North Total or Average |  |  |  |  |  |  | 11.20 | 3.354 | 0.361 | 0.271 |  |  |  |  |  |  |  |  |  |  |
Non-North Total or Average |  |  |  |  |  |  | 10.24 | 3.965 | 0.271 | 0.164 |  |  |  |  |  |  |  |  |  |  |

Exterior Fenestration Shaded State

| Frame and Divider | Glass U-Factor [W/m2-K] | Glass SHGC | Glass Visible Transmittance | NFRC Product Type | Assembly U-Factor [W/m2-K] | Assembly SHGC | Assembly Visible Transmittance
None |  |  |  |  |  |  |  |

Interior Fenestration

| Construction | Area of One Opening [m2] | Area of Openings [m2] | Glass U-Factor [W/m2-K] | Glass SHGC | Glass Visible Transmittance | Parent Surface
Total or Average |  |  | 0.00 | - | - | - |

Exterior Door

| Construction | U-Factor with Film [W/m2-K] | U-Factor no Film [W/m2-K] | Gross Area [m2] | Parent Surface
None |  |  |  |  |

Interior Door

| Construction | U-Factor with Film [W/m2-K] | U-Factor no Film [W/m2-K] | Gross Area [m2] | Parent Surface
FACE 59 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 58
FACE 12 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 11
FACE 15 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.89 | FACE 14
FACE 31 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 30
FACE 33 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 32
FACE 3 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.89 | FACE 2
FACE 87 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 86
FACE 71 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 70
FACE 74 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.89 | FACE 73
FACE 93 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 92
FACE 100 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.68 | FACE 99
FACE 75 | TYPICAL INTERIOR DOOR | 2.446 | 5.906 | 1.89 | FACE 41

Opaque Construction Layers

| Layer 1 | Layer 2 | Layer 3 | Layer 4 | Layer 5 | Layer 6 | Layer 7 | Layer 8 | Layer 9 | Layer 10
TYPICAL IEAD ROOF R-17.24 10 | Roof Membrane | TYPICAL INSULATION R-16.12 10 | Metal Roof Surface |  |  |  |  |  |  |
TYPICAL INSULATED CARPETED 6IN SLAB FLOOR | 6 in. Normalweight Concrete Floor | TYPICAL CARPET PAD |  |  |  |  |  |  |  |
TYPICAL INSULATED STEEL FRAMED EXTERIOR WALL R-11.24 4 | 25mm Stucco | 5/8 in. Gypsum Board | TYPICAL INSULATION R-9.06 4 | 5/8 in. Gypsum Board |  |  |  |  |  |
TYPICAL INTERIOR CEILING | CP02 CARPET PAD 1 | 100mm Normalweight concrete floor |  |  |  |  |  |  |  |
TYPICAL INTERIOR DOOR | G05 25mm wood |  |  |  |  |  |  |  |  |
TYPICAL INTERIOR FLOOR | 100mm Normalweight concrete floor | CP02 CARPET PAD 1 |  |  |  |  |  |  |  |
TYPICAL INTERIOR WALL | G01 13mm gypsum board | G01 13mm gypsum board |  |  |  |  |  |  |  |

Table of Contents

Report: Shading Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Sunlit Fraction

| March 21 9am | March 21 noon | March 21 3pm | June 21 9am | June 21 noon | June 21 3pm | December 21 9am | December 21 noon | December 21 3pm
FACE 62 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 0.00
FACE 17 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 0.00
FACE 37 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00
FACE 6 | 0.00 | 1.00 | 1.00 | 0.00 | 1.00 | 1.00 | 0.00 | 1.00 | 1.00
FACE 89 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 0.00
FACE 66 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 0.00
FACE 95 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00
FACE 77 | 0.00 | 1.00 | 1.00 | 0.00 | 1.00 | 1.00 | 0.00 | 1.00 | 1.00

Window Control

| Name | Type | Shaded Construction | Control | Glare Control
None |  |  |  |  |

Table of Contents

Report: Lighting Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Interior Lighting

| Zone Name | Space Name | Space Type | Lighting Power Density [W/m2] | Space Area [m2] | Total Power [W] | End Use Subcategory | Schedule Name | Scheduled Hours/Week [hr] | Hours/Week > 1% [hr] | Full Load Hours/Week [hr] | Return Air Fraction | Conditioned (Y/N) | Consumption [GJ]
1-A2.WC MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_1-A2.WC | 1-A2.WC | MIDRISEAPARTMENT APARTMENT | 3.8750 | 11.72 | 45.42 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 0.47
1-A2.LK MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_1-A2.LK | 1-A2.LK | MIDRISEAPARTMENT APARTMENT | 3.8750 | 45.20 | 175.15 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 1.81
0-A1.WC MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_0-A1.WC | 0-A1.WC | MIDRISEAPARTMENT APARTMENT | 3.8750 | 11.72 | 45.42 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 0.47
1-A2.B MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_1-A2.B | 1-A2.B | MIDRISEAPARTMENT APARTMENT | 3.8750 | 24.68 | 95.63 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 0.99
0-A1.B MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_0-A1.B | 0-A1.B | MIDRISEAPARTMENT APARTMENT | 3.8750 | 24.68 | 95.63 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 0.99
0-A1.LK MIDRISEAPARTMENT APARTMENT LIGHTS | TZ_0-A1.LK | 0-A1.LK | MIDRISEAPARTMENT APARTMENT | 3.8750 | 45.20 | 175.15 | General | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 168.00 | 55.16 | 0.0000 | Y | 1.81
1-H MIDRISEAPARTMENT CORRIDOR LIGHTS | TZ_1-H | 1-H | MIDRISEAPARTMENT CORRIDOR | 9.9028 | 22.40 | 221.82 | General | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.00 | 168.00 | 168.00 | 0.0000 | N | 7.00
0-H MIDRISEAPARTMENT CORRIDOR LIGHTS | TZ_0-H | 0-H | MIDRISEAPARTMENT CORRIDOR | 9.9028 | 22.40 | 221.82 | General | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.00 | 168.00 | 168.00 | 0.0000 | N | 7.00
Interior Lighting Total |  |  |  | 5.1733 | 208.00 | 1076.05 |  |  |  |  |  |  |  | 20.54

Daylighting

| Zone | Control Name | Daylighting Method | Control Type | Fraction Controlled | Lighting Installed in Zone [W] | Lighting Controlled [W]
None |  |  |  |  |  |  |

Exterior Lighting

| Total Watts | Astronomical Clock/Schedule | Schedule Name | Scheduled Hours/Week [hr] | Hours/Week > 1% [hr] | Full Load Hours/Week [hr] | Consumption [GJ]
Exterior Lighting Total | 0.00 |  |  |  |  |  | 0.00

Table of Contents

Report: Equipment Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Central Plant

| Type | Reference Capacity [W] | Reference Efficiency [W/W] | Rated Capacity [W] | Rated Efficiency [W/W] | IPLV in SI Units [W/W] | IPLV in IP Units [Btu/W-h]
None |  |  |  |  |  |  |

Cooling Coils

| Type | Design Coil Load [W] | Nominal Total Capacity [W] | Nominal Sensible Capacity [W] | Nominal Latent Capacity [W] | Nominal Sensible Heat Ratio | Nominal Efficiency [W/W] | Nominal Coil UA Value [W/C] | Nominal Coil Surface Area [m2]
None |  |  |  |  |  |  |  |  |

DX Cooling Coil Standard Ratings 2017

| Cooling Coil Type [1] | Standard Rating Net Cooling Capacity [W][2] | Standard Rating Net COP [W/W][2] | EER [Btu/W-h][2] | SEER User [Btu/W-h][2,3] | SEER Standard [Btu/W-h][2,3] | IEER [Btu/W-h][2]
None |  |  |  |  |  |  |

DX Cooling Coil Standard Ratings 2023

| Cooling Coil Type [1] | Standard Rating Net Cooling Capacity [W][2] | Standard Rating Net COP2 [W/W][2,4] | EER2 [Btu/W-h][2,4] | SEER2 User [Btu/W-h][2,3] | SEER2 Standard [Btu/W-h][2,3] | IEER [Btu/W-h][2]
None |  |  |  |  |  |  |

DX Cooling Coil ASHRAE 127 Standard Ratings Report

| DX Cooling Coil Type | Rated Net Cooling Capacity Test A [W] | Rated Electric Power Test A [W] | Rated Net Cooling Capacity Test B [W] | Rated Electric Power Test B [W] | Rated Net Cooling Capacity Test C [W] | Rated Electric Power Test C [W] | Rated Net Cooling Capacity Test D [W] | Rated Electric Power Test D [W]
None |  |  |  |  |  |  |  |  |

Water-to-Air Heat Pumps at Rated Temperatures Report

| Coil Type | Rated Total Capacity [W] | Rated Sensible Capacity [W] | Rated Power[W] | Rated COP [W/W] | Rated Air Dry-bulb Temperature [C] | Rated Air Wet-bulb Temperature [C] | Rated Water Temperature [C] | Design Day used for Sizing
None |  |  |  |  |  |  |  |  |

DX Heating Coils

| DX Heating Coil Type | High Temperature Heating (net) Rating Capacity [W] | Low Temperature Heating (net) Rating Capacity [W] | HSPF [Btu/W-h] | Region Number | Minimum Outdoor Dry-Bulb Temperature for Compressor Operation [C] | Supplemental Heat High Shutoff Temperature [C] | Airloop Name
None |  |  |  |  |  |  |  |

DX Heating Coils AHRI 2023

| DX Heating Coil Type | High Temperature Heating (net) Rating Capacity [W] | Low Temperature Heating (net) Rating Capacity [W] | HSPF2 [Btu/W-h] | Region Number | Minimum Outdoor Dry-Bulb Temperature for Compressor Operation [C] | Airloop Name
None |  |  |  |  |  |  |

Heating Coils

| Type | Design Coil Load [W] | Nominal Total Capacity [W] | Nominal Efficiency [W/W] | Used as Supplementary Heat | Airloop Name | Plantloop Name
None |  |  |  |  |  |  |

Fans

| Type | Total Efficiency [W/W] | Delta Pressure [pa] | Max Air Flow Rate [m3/s] | Rated Electricity Rate [W] | Rated Power Per Max Air Flow Rate [W-s/m3] | Motor Heat In Air Fraction | Fan Energy Index | End Use Subcategory | Design Day Name for Fan Sizing Peak | Date/Time for Fan Sizing Peak | Purpose | Is Autosized | Motor Efficiency | Motor Heat to Zone Fraction | Motor Loss Zone Name | Airloop Name
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Pumps

| Type | Control | Head [pa] | Water Flow [m3/s] | Electricity Rate [W] | Power Per Water Flow Rate [W-s/m3] | Motor Efficiency [W/W] | End Use Subcategory | Is Autosized | Plantloop Name | Plantloop Branch Name
None |  |  |  |  |  |  |  |  |  |  |

Service Water Heating

| Type | Storage Volume [m3] | Input [W] | Thermal Efficiency [W/W] | Recovery Efficiency [W/W] | Energy Factor
None |  |  |  |  |  |

Chillers

| Type | Reference Capacity[W] | TypeReference Efficiency [W/W] | Rated Capacity [W] | Rated Efficiency [W/W] | IPLV in SI Units [W/W] | IPLV in IP Units [Btu/W-h] | Minimum Part Load Ratio | Fuel Type | Rated Entering Condenser Temperature [C] | Rated Leaving Evaporator Temperature [C] | Reference Entering Condenser Temperature [C] | Reference Leaving Evaporator Temperature [C] | Design Size Reference Chilled Water Flow Rate [kg/s] | Design Size Reference Condenser Fluid Flow Rate [kg/s] | Plantloop Name | Plantloop Branch Name | Condenser Loop Name | Condenser Loop Branch Name | Heat Recovery Plantloop Name | Heat Recovery Plantloop Branch Name | Recovery Relative Capacity Fraction
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Boilers

| Type | Reference Capacity [W] | Reference Efficiency[W/W] | Rated Capacity [W] | Rated Efficiency [W/W] | Minimum Part Load Ratio | Fuel Type | Parasitic Electric Load [W] | Plantloop Name | Plantloop Branch Name
None |  |  |  |  |  |  |  |  |  |

Cooling Towers and Fluid Coolers

| Type | Fluid Type | Range [C] | Approach [C] | Design Fan Power [W] | Design Inlet Air Wet-Bulb Temperature [C] | Design Water Flow Rate [m3/s] | Leaving Water Setpoint Temperature [C] | Condenser Loop Name | Condenser Loop Branch Name
None |  |  |  |  |  |  |  |  |  |

PlantLoop or CondenserLoop

| Type | Provides Heating | Provides Cooling | Maximum Loop Flow Rate [m3/s] | Minimum Loop Flow Rate [m3/s]
None |  |  |  |  |

Air Terminals

| Zone Name | Minimum Flow [m3/s] | Minimum Outdoor Flow [m3/s] | Supply Cooling Setpoint [C] | Supply Heating Setpoint [C] | Heating Capacity [W] | Cooling Capacity [W] | Type of Input Object | Heat/Reheat Coil Object Type | Chilled Water Coil Object Type | Fan Object Type | Fan Name | Primary Air Flow Rate [m3/s] | Secondary Air Flow Rate [m3/s] | Minimum Flow Schedule Name | Maximum Flow During Reheat [m3/s] | Minimum Outdoor Flow Schedule Name
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Air Heat Recovery

| Name | Input object type | Plate/Rotary | Sensible Effectiveness at 100% Heating Air Flow | Sensible Effectiveness at 100% Cooling Air Flow | Latent Effectiveness at 100% Heating Air Flow | Latent Effectiveness at 100% Cooling Air Flow | Exhaust Airflow [kg/s] | Outdoor Airflow [kg/s]
None |  |  |  |  |  |  |  |  |

Table of Contents

Report: HVAC Sizing Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Space Sensible Cooling

| Calculated Design Load [W] | User Design Load [W] | User Design Load per Area [W/m2] | Calculated Design Air Flow [m3/s] | User Design Air Flow [m3/s] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [C] | Indoor Temperature at Peak Load [C] | Indoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Outdoor Temperature at Peak Load [C] | Outdoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Minimum Outdoor Air Flow Rate [m3/s] | Heat Gain Rate from DOAS [W]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the space sensible load only. It does not include any system effects or ventilation loads.
Zone Sensible Cooling

| Calculated Design Load [W] | User Design Load [W] | User Design Load per Area [W/m2] | Calculated Design Air Flow [m3/s] | User Design Air Flow [m3/s] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [C] | Indoor Temperature at Peak Load [C] | Indoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Outdoor Temperature at Peak Load [C] | Outdoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Minimum Outdoor Air Flow Rate [m3/s] | Heat Gain Rate from DOAS [W]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the zone sensible load only. It does not include any system effects or ventilation loads.
Space Sensible Heating

| Calculated Design Load [W] | User Design Load [W] | User Design Load per Area [W/m2] | Calculated Design Air Flow [m3/s] | User Design Air Flow [m3/s] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [C] | Indoor Temperature at Peak Load [C] | Indoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Outdoor Temperature at Peak Load [C] | Outdoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Minimum Outdoor Air Flow Rate [m3/s] | Heat Gain Rate from DOAS [W]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the space sensible load only. It does not include any system effects or ventilation loads.
Zone Sensible Heating

| Calculated Design Load [W] | User Design Load [W] | User Design Load per Area [W/m2] | Calculated Design Air Flow [m3/s] | User Design Air Flow [m3/s] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [C] | Indoor Temperature at Peak Load [C] | Indoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Outdoor Temperature at Peak Load [C] | Outdoor Humidity Ratio at Peak Load [kgWater/kgDryAir] | Minimum Outdoor Air Flow Rate [m3/s] | Heat Gain Rate from DOAS [W]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the zone sensible load only. It does not include any system effects or ventilation loads.
System Design Air Flow Rates

| Calculated cooling [m3/s] | User cooling [m3/s] | Calculated heating [m3/s] | User heating [m3/s] | Adjusted cooling [m3/s] | Adjusted heating [m3/s] | Adjusted main [m3/s] | Calculated Heating Air Flow Ratio [] | User Heating Air Flow Ratio []
None |  |  |  |  |  |  |  |  |

Plant Loop Coincident Design Fluid Flow Rate Adjustments

| Previous Design Volume Flow Rate [m3/s] | Algorithm Volume Flow Rate [m3/s] | Coincident Design Volume Flow Rate [m3/s] | Coincident Size Adjusted | Peak Sizing Period Name | Peak Day into Period {TIMESTAMP}[day] | Peak Hour Of Day {TIMESTAMP}[hr] | Peak Step Start Minute {TIMESTAMP}[min]
None |  |  |  |  |  |  |  |

Coil Sizing Summary

| Coil Type | HVAC Type | HVAC Name | Coil Final Gross Total Capacity [W] | Coil Final Gross Sensible Capacity [W] | Coil Final Reference Air Volume Flow Rate [m3/s] | Coil Final Reference Plant Fluid Volume Flow Rate [m3/s] | Coil U-value Times Area Value [W/K] | Design Day Name at Sensible Ideal Loads Peak | Date/Time at Sensible Ideal Loads Peak | Design Day Name at Air Flow Ideal Loads Peak | Date/Time at Air Flow Ideal Loads Peak | Coil Total Capacity at Ideal Loads Peak [W] | Coil Sensible Capacity at Ideal Loads Peak [W] | Coil Air Volume Flow Rate at Ideal Loads Peak [m3/s] | Coil Entering Air Drybulb at Ideal Loads Peak [C] | Coil Entering Air Wetbulb at Ideal Loads Peak [C] | Coil Entering Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Coil Leaving Air Drybulb at Ideal Loads Peak [C] | Coil Leaving Air Wetbulb at Ideal Loads Peak [C] | Coil Leaving Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Outdoor Air Drybulb at Ideal Loads Peak [C] | Outdoor Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Outdoor Air Wetbulb at Ideal Loads Peak [C] | Outdoor Air Flow Percentage at Ideal Loads Peak [%] | Zone Air Drybulb at Ideal Loads Peak [C] | Zone Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Zone Air Relative Humidity at Ideal Loads Peak [%] | Zone Sensible Heat Gain at Ideal Loads Peak [W] | Zone Latent Heat Gain at Ideal Loads Peak [W] | Coil Total Capacity at Rating Conditions [W] | Coil Sensible Capacity at Rating Conditions [W]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Table of Contents

Report: Coil Sizing Details

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Coils

| Coil Type | Coil Location | HVAC Type | HVAC Name | Zone Name(s) | System Sizing Method Concurrence | System Sizing Method Capacity | System Sizing Method Air Flow | Autosized Coil Capacity? | Autosized Coil Airflow? | Autosized Coil Water Flow? | OA Pretreated prior to coil inlet? | Coil Final Gross Total Capacity [W] | Coil Final Gross Sensible Capacity [W] | Coil Final Reference Air Volume Flow Rate [m3/s] | Coil Final Reference Plant Fluid Volume Flow Rate [m3/s] | Coil U-value Times Area Value [W/K] | Terminal Unit Reheat Coil Multiplier | DX Coil Capacity Increase Ratio from Too Low Flow/Capacity Ratio | DX Coil Capacity Decrease Ratio from Too High Flow/Capacity Ratio | Moist Air Heat Capacity [J/kg-K] | Dry Air Heat Capacity [J/kg-K] | Standard Air Density Adjusted for Elevation [kg/m3] | Supply Fan Name for Coil | Supply Fan Type for Coil | Supply Fan Maximum Air Volume Flow Rate [m3/s] | Supply Fan Maximum Air Mass Flow Rate [kg/s] | Plant Name for Coil | Plant Fluid Specific Heat Capacity [J/kg-K] | Plant Fluid Density [kg/m3] | Plant Maximum Fluid Mass Flow Rate [kg/s] | Plant Design Fluid Return Temperature [C] | Plant Design Fluid Supply Temperature [C] | Plant Design Fluid Temperature Difference [deltaC] | Plant Design Capacity [W] | Coil Capacity Percentage of Plant Design Capacity [%] | Coil Fluid Flow Rate Percentage of Plant Design Flow Rate [%] | Design Day Name at Sensible Ideal Loads Peak | Date/Time at Sensible Ideal Loads Peak | Design Day Name at Total Ideal Loads Peak | Date/Time at Total Ideal Loads Peak | Design Day Name at Air Flow Ideal Loads Peak | Date/Time at Air Flow Ideal Loads Peak | Peak Load Type to Size On | Coil Total Capacity at Ideal Loads Peak [W] | Coil Sensible Capacity at Ideal Loads Peak [W] | Coil Off-Rating Capacity Modifier at Ideal Loads Peak [ ] | Coil Air Mass Flow Rate at Ideal Loads Peak [kg/s] | Coil Air Volume Flow Rate at Ideal Loads Peak [m3/s] | Coil Entering Air Drybulb at Ideal Loads Peak [C] | Coil Entering Air Wetbulb at Ideal Loads Peak [C] | Coil Entering Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Coil Entering Air Enthalpy at Ideal Loads Peak [J/KG-K] | Coil Leaving Air Drybulb at Ideal Loads Peak [C] | Coil Leaving Air Wetbulb at Ideal Loads Peak [C] | Coil Leaving Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Coil Leaving Air Enthalpy at Ideal Loads Peak [J/KG-K] | Coil Plant Fluid Mass Flow Rate at Ideal Loads Peak [kg/s] | Coil Entering Plant Fluid Temperature at Ideal Loads Peak [C] | Coil Leaving Plant Fluid Temperature at Ideal Loads Peak [C] | Coil Plant Fluid Temperature Difference at Ideal Loads Peak [deltaC] | Supply Fan Air Heat Gain at Ideal Loads Peak [W] | Coil and Fan Net Total Capacity at Ideal Loads Peak [W] | Outdoor Air Drybulb at Ideal Loads Peak [C] | Outdoor Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Outdoor Air Wetbulb at Ideal Loads Peak [C] | Outdoor Air Volume Flow Rate at Ideal Loads Peak [m3/s] | Outdoor Air Flow Percentage at Ideal Loads Peak [%] | System Return Air Drybulb at Ideal Loads Peak [C] | System Return Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Zone Air Drybulb at Ideal Loads Peak [C] | Zone Air Humidity Ratio at Ideal Loads Peak [kgWater/kgDryAir] | Zone Air Relative Humidity at Ideal Loads Peak [%] | Zone Sensible Heat Gain at Ideal Loads Peak [W] | Zone Latent Heat Gain at Ideal Loads Peak [W] | Coil Total Capacity at Rating Conditions [W] | Coil Sensible Capacity at Rating Conditions [W] | Coil Air Mass Flow Rate at Rating Conditions [kg/s] | Coil Entering Air Drybulb at Rating Conditions [C] | Coil Entering Air Wetbulb at Rating Conditions [C] | Coil Entering Air Humidity Ratio at Rating Conditions [kgWater/kgDryAir] | Coil Entering Air Enthalpy at Rating Conditions [J/KG-K] | Coil Leaving Air Drybulb at Rating Conditions [C] | Coil Leaving Air Wetbulb at Rating Conditions [C] | Coil Leaving Air Humidity Ratio at Rating Conditions [kgWater/kgDryAir] | Coil Leaving Air Enthalpy at Rating Conditions [J/KG-K]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Coil Connections

| Coil Name | Coil Type | Coil Location | HVAC Type | HVAC Name | Zone Name(s) | Supply Fan Name for HVAC | Supply Fan Type for HVAC | Airloop Name | Plant Name for Coil | Plant Loop Name
None |  |  |  |  |  |  |  |  |  |  |

Table of Contents

Report: System Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Economizer

| High Limit Shutoff Control | Minimum Outdoor Air [m3/s] | Maximum Outdoor Air [m3/s] | Return Air Temp Limit | Return Air Enthalpy Limit | Outdoor Air Temperature Limit [C] | Outdoor Air Enthalpy Limit [C]
None |  |  |  |  |  |  |

Demand Controlled Ventilation using Controller:MechanicalVentilation

| Controller:MechanicalVentilation Name | Outdoor Air Per Person [m3/s-person] | Outdoor Air Per Area [m3/s-m2] | Outdoor Air Per Zone [m3/s] | Outdoor Air ACH [ach] | Outdoor Air Method | Outdoor Air Schedule Name | Air Distribution Effectiveness in Cooling Mode | Air Distribution Effectiveness in Heating Mode | Air Distribution Effectiveness Schedule Name | Type
None |  |  |  |  |  |  |  |  |  |  |

Time Not Comfortable Based on Simple ASHRAE 55-2004

| Winter Clothes [hr] | Summer Clothes [hr] | Summer or Winter Clothes [hr]
TZ_0-A1.B | 6996.50 | 8451.17 | 6763.00
TZ_0-A1.LK | 6951.50 | 8421.17 | 6697.00
TZ_0-A1.WC | 6971.33 | 8372.00 | 6667.17
TZ_1-A2.B | 7308.50 | 7828.33 | 6465.83
TZ_1-A2.LK | 7339.67 | 7792.67 | 6468.00
TZ_1-A2.WC | 7289.50 | 7845.67 | 6463.67
TZ_0-H | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00
Facility | 7817.33 | 8580.17 | 7044.83

Aggregated over the RunPeriods for Weather
Time Setpoint Not Met

| During Heating [hr] | During Cooling [hr] | During Occupied Heating [hr] | During Occupied Cooling [hr]
TZ_0-A1.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-A1.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.B | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 0.00 | 0.00 | 0.00 | 0.00
TZ_0-H | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | 0.00 | 0.00 | 0.00 | 0.00
Facility | 0.00 | 0.00 | 0.00 | 0.00

Aggregated over the RunPeriods for Weather
Thermostat Schedules

| Thermostat Name 1 | Control Type Schedule | Control Type | Control Type Name | Heating Schedule | Cooling Schedule
TZ_0-A1.B | TZ_0-A1.B THERMOSTAT | TZ_0-A1.B THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 1 | HEATING SETPOINT | COOLING SETPOINT
TZ_0-A1.LK | TZ_0-A1.LK THERMOSTAT | TZ_0-A1.LK THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 2 | HEATING SETPOINT | COOLING SETPOINT
TZ_0-A1.WC | TZ_0-A1.WC THERMOSTAT | TZ_0-A1.WC THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 3 | HEATING SETPOINT | COOLING SETPOINT
TZ_1-A2.B | TZ_1-A2.B THERMOSTAT | TZ_1-A2.B THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 6 | HEATING SETPOINT | COOLING SETPOINT
TZ_1-A2.LK | TZ_1-A2.LK THERMOSTAT | TZ_1-A2.LK THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 4 | HEATING SETPOINT | COOLING SETPOINT
TZ_1-A2.WC | TZ_1-A2.WC THERMOSTAT | TZ_1-A2.WC THERMOSTAT SCHEDULE | DualSetPointWithDeadBand | THERMOSTAT SETPOINT DUAL SETPOINT 5 | HEATING SETPOINT | COOLING SETPOINT

Table of Contents

Report: HVAC Topology

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Air Loop Supply Side Component Arrangement

| Airloop Name | Splitter Name | Supply Branch Name | Supply Branch Type | Component Type | Component Name | Sub-Component Type | Sub-Component Name | Sub-Sub-Component Type | Sub-Sub-Component Name | Mixer Name
None |  |  |  |  |  |  |  |  |  |  |

Air Loop Demand Side Component Arrangement

| Airloop Name | Supply Branch Name | Supply Branch Type | Supply Path Component Type | Supply Path Component Name | Terminal Unit Type | Terminal Unit Name | Zone Name | Return Path Component Type | Return Path Component Name
None |  |  |  |  |  |  |  |  |  |

Zone Equipment Component Arrangement

| Zone Name | Component Type | Component Name | Sub-Component Type | Sub-Component Name | Sub-Sub-Component Type | Sub-Sub-Component Name
1 | TZ_0-A1.B |  |  |  |  |  |
2 | TZ_0-A1.B | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_0-A1.B IDEAL LOADS AIR SYSTEM |  |  |  |
3 | TZ_0-A1.LK |  |  |  |  |  |
4 | TZ_0-A1.LK | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_0-A1.LK IDEAL LOADS AIR SYSTEM |  |  |  |
5 | TZ_0-A1.WC |  |  |  |  |  |
6 | TZ_0-A1.WC | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_0-A1.WC IDEAL LOADS AIR SYSTEM |  |  |  |
7 | TZ_0-H |  |  |  |  |  |
8 | TZ_1-A2.B |  |  |  |  |  |
9 | TZ_1-A2.B | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_1-A2.B IDEAL LOADS AIR SYSTEM |  |  |  |
10 | TZ_1-A2.LK |  |  |  |  |  |
11 | TZ_1-A2.LK | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_1-A2.LK IDEAL LOADS AIR SYSTEM |  |  |  |
12 | TZ_1-A2.WC |  |  |  |  |  |
13 | TZ_1-A2.WC | ZONEHVAC:IDEALLOADSAIRSYSTEM | TZ_1-A2.WC IDEAL LOADS AIR SYSTEM |  |  |  |
14 | TZ_1-H |  |  |  |  |  |

Plant Loop Component Arrangement

| Loop Type | Loop Name | Side | Splitter Name | Branch Name | Component Type | Component Name | Mixer Name
None |  |  |  |  |  |  |  |

Table of Contents

Report: Outdoor Air Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Average Outdoor Air During Occupied Hours

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume [m3] | Mechanical Ventilation [ach] | Infiltration [ach] | AFN Infiltration [ach] | Simple Ventilation [ach]
TZ_0-A1.B | 0.48 | 0.70 | 66.63 | 0.000 | 1.639 | 0.000 | 0.455
TZ_0-A1.LK | 0.88 | 1.28 | 122.04 | 0.000 | 1.054 | 0.000 | 0.455
TZ_0-A1.WC | 0.23 | 0.33 | 31.65 | 0.000 | 2.695 | 0.000 | 0.455
TZ_1-A2.B | 0.48 | 0.70 | 66.63 | 0.000 | 1.641 | 0.000 | 0.456
TZ_1-A2.LK | 0.88 | 1.28 | 122.04 | 0.000 | 1.055 | 0.000 | 0.456
TZ_1-A2.WC | 0.23 | 0.33 | 31.65 | 0.000 | 2.698 | 0.000 | 0.455

Values shown for a single zone without multipliers
Minimum Outdoor Air During Occupied Hours

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume [m3] | Mechanical Ventilation [ach] | Infiltration [ach] | AFN Infiltration [ach] | Simple Ventilation [ach]
TZ_0-A1.B | 0.48 | 0.70 | 66.63 | 0.000 | 0.088 | 0.000 | 0.009
TZ_0-A1.LK | 0.88 | 1.28 | 122.04 | 0.000 | 0.056 | 0.000 | 0.009
TZ_0-A1.WC | 0.23 | 0.33 | 31.65 | 0.000 | 0.144 | 0.000 | 0.009
TZ_1-A2.B | 0.48 | 0.70 | 66.63 | 0.000 | 0.088 | 0.000 | 0.009
TZ_1-A2.LK | 0.88 | 1.28 | 122.04 | 0.000 | 0.056 | 0.000 | 0.009
TZ_1-A2.WC | 0.23 | 0.33 | 31.65 | 0.000 | 0.144 | 0.000 | 0.009

Values shown for a single zone without multipliers

Table of Contents

Report: Outdoor Air Details

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Mechanical Ventilation Parameters by Zone

| AirLoop Name | Average Number of Occupants | Nominal Number of Occupants | Zone Volume [m3] | Zone Area [m2] | Design Zone Outdoor Airflow - Voz [m3/s] | Minimum Dynamic Target Ventilation - Voz-dyn-min [m3/s]
TZ_0-A1.B |  | 0.48 | 0.70 | 66.63 | 24.68 |  | 0.000
TZ_0-A1.LK |  | 0.88 | 1.28 | 122.04 | 45.20 |  | 0.000
TZ_0-A1.WC |  | 0.23 | 0.33 | 31.65 | 11.72 |  | 0.000
TZ_1-A2.B |  | 0.48 | 0.70 | 66.63 | 24.68 |  | 0.000
TZ_1-A2.LK |  | 0.88 | 1.28 | 122.04 | 45.20 |  | 0.000
TZ_1-A2.WC |  | 0.23 | 0.33 | 31.65 | 11.72 |  | 0.000
Total Facility |  | 3.16 | 4.62 | 440.64 | 163.20 | 0.0000 | 0.000

Total Outdoor Air by Zone

| Mechanical Ventilation [m3] | Natural Ventilation [m3] | Total Ventilation [m3] | Infiltration [m3] | Total Ventilation and Infiltration [m3] | Dynamic Target Ventilation - Voz-dyn [m3] | Time Below Voz-dyn [hr] | Time At Voz-dyn [hr] | Time Above Voz-dyn [hr] | Time Above Zero When Unoccupied [hr]
TZ_0-A1.B | 0.00 | 262554.51 | 262554.51 | 944979.68 | 1207534.18 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
TZ_0-A1.LK | 0.00 | 480902.19 | 480902.19 | 1112319.83 | 1593222.01 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
TZ_0-A1.WC | 0.00 | 124720.71 | 124720.71 | 738265.37 | 862986.08 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
TZ_1-A2.B | 0.00 | 262570.79 | 262570.79 | 945038.01 | 1207608.79 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
TZ_1-A2.LK | 0.00 | 480932.00 | 480932.00 | 1112388.49 | 1593320.49 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
TZ_1-A2.WC | 0.00 | 124728.44 | 124728.44 | 738310.94 | 863039.38 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00
Total Facility | 0.00 | 1736408.63 | 1736408.63 | 5591302.32 | 7327710.94 | 0.00 | 0.00 | 0.00 | 8760.00 | 0.00

Average Outdoor Air During Occupancy by Zone - Flow Rates

| Mechanical Ventilation [m3/s] | Natural Ventilation [m3/s] | Total Ventilation [m3/s] | Infiltration [m3/s] | Total Ventilation and Infiltration [m3/s] | Dynamic Target Ventilation - Voz-dyn [m3/s] | Time Below Voz-dyn [hr] | Time At Voz-dyn [hr] | Time Above Voz-dyn [hr]
TZ_0-A1.B | 0.0000 | 0.0083 | 0.0083 | 0.0300 | 0.0383 | 0.0000 | 0.00 | 0.00 | 8760.00
TZ_0-A1.LK | 0.0000 | 0.0152 | 0.0152 | 0.0353 | 0.0505 | 0.0000 | 0.00 | 0.00 | 8760.00
TZ_0-A1.WC | 0.0000 | 0.0040 | 0.0040 | 0.0234 | 0.0274 | 0.0000 | 0.00 | 0.00 | 8760.00
TZ_1-A2.B | 0.0000 | 0.0083 | 0.0083 | 0.0300 | 0.0383 | 0.0000 | 0.00 | 0.00 | 8760.00
TZ_1-A2.LK | 0.0000 | 0.0153 | 0.0153 | 0.0353 | 0.0505 | 0.0000 | 0.00 | 0.00 | 8760.00
TZ_1-A2.WC | 0.0000 | 0.0040 | 0.0040 | 0.0234 | 0.0274 | 0.0000 | 0.00 | 0.00 | 8760.00
Total Facility | 0.0000 | 0.0551 | 0.0551 | 0.1773 | 0.2324 | 0.0000 | 0.00 | 0.00 | 8760.00

Total Outdoor Air by AirLoop

| Mechanical Ventilation [m3] | Natural Ventilation [m3] | Total Ventilation [m3] | Sum Zone Dynamic Target Ventilation - Voz-sum-dyn [m3] | Time Below Voz-sum-dyn [hr] | Time At Voz-sum-dyn [hr] | Time Above Voz-sum-dyn [hr] | Time Above Zero When Unoccupied [hr]
None |  |  |  |  |  |  |  |

Average Outdoor Air During Occupancy by AirLoop

| Mechanical Ventilation [m3/s] | Natural Ventilation [m3/s] | Total Ventilation [m3/s] | Sum Zone Dynamic Target Ventilation - Voz-sum-dyn [m3/s] | Time Below Voz-sum-dyn [hr] | Time At Voz-sum-dyn [hr] | Time Above Voz-sum-dyn [hr]
None |  |  |  |  |  |  |

Outdoor Air Controller Limiting Factors by AirLoop

| No Limiting Factor [hr] | Limits and Scheduled Limits [hr] | Economizer [hr] | Exhaust Flow [hr] | Mixed Air Flow [hr] | High Humidity [hr] | Demand Controlled Ventilation [hr] | Night Ventilation [hr] | Demand Limiting [hr] | Energy Management System [hr]
None |  |  |  |  |  |  |  |  |  |

Average Outdoor Air for Limiting Factors During Occupancy

| No Limiting Factor [m3/s] | Limits and Scheduled Limits [m3/s] | Economizer [m3/s] | Exhaust Flow [m3/s] | Mixed Air Flow [m3/s] | High Humidity [m3/s] | Demand Controlled Ventilation [m3/s] | Night Ventilation [m3/s] | Demand Limiting [m3/s] | Energy Management System [m3/s]
None |  |  |  |  |  |  |  |  |  |

Table of Contents

Report: Object Count Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Surfaces by Class

| Total | Outdoors
Wall | 42 | 18
Floor | 8 | 4
Roof | 8 | 4
Internal Mass | 0 | 0
Building Detached Shading | 0 | 0
Fixed Detached Shading | 0 | 0
Window | 8 | 8
Door | 12 | 0
Glass Door | 1 | 1
Shading | 0 | 0
Overhang | 0 | 0
Fin | 0 | 0
Tubular Daylighting Device Dome | 0 | 0
Tubular Daylighting Device Diffuser | 0 | 0

HVAC

| Count
HVAC Air Loops | 0
Conditioned Zones | 6
Unconditioned Zones | 2
Supply Plenums | 0
Return Plenums | 0

Input Fields

| Count
IDF Objects | 310
Defaulted Fields | 382
Fields with Defaults | 849
Autosized Fields | 0
Autosizable Fields | 24
Autocalculated Fields | 205
Autocalculatable Fields | 205

Table of Contents

Report: Energy Meters

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Annual and Peak Values - Electricity

| Electricity Annual Value [GJ] | Electricity Minimum Value [W] | Timestamp of Minimum {TIMESTAMP} | Electricity Maximum Value [W] | Timestamp of Maximum {TIMESTAMP}
Electricity:Facility | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
Electricity:Building | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
Electricity:Zone:TZ_1-A2.WC | 1.78 | 27.02 | 01-JAN-03:10 | 103.46 | 01-JAN-19:10
Electricity:SpaceType:MIDRISEAPARTMENT APARTMENT | 24.77 | 376.14 | 01-JAN-03:10 | 1440.40 | 01-JAN-19:10
InteriorLights:Electricity | 20.54 | 486.02 | 01-JAN-00:10 | 1076.05 | 01-JAN-20:10
InteriorLights:Electricity:Zone:TZ_1-A2.WC | 0.47 | 3.04 | 01-JAN-00:10 | 45.42 | 01-JAN-20:10
InteriorLights:Electricity:SpaceType:MIDRISEAPARTMENT APARTMENT | 6.55 | 42.37 | 01-JAN-00:10 | 632.40 | 01-JAN-20:10
General:InteriorLights:Electricity | 20.54 | 486.02 | 01-JAN-00:10 | 1076.05 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_1-A2.WC | 0.47 | 3.04 | 01-JAN-00:10 | 45.42 | 01-JAN-20:10
General:InteriorLights:Electricity:SpaceType:MIDRISEAPARTMENT APARTMENT | 6.55 | 42.37 | 01-JAN-00:10 | 632.40 | 01-JAN-20:10
Electricity:Zone:TZ_1-A2.LK | 6.86 | 104.18 | 01-JAN-03:10 | 398.93 | 01-JAN-19:10
InteriorLights:Electricity:Zone:TZ_1-A2.LK | 1.81 | 11.74 | 01-JAN-00:10 | 175.15 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_1-A2.LK | 1.81 | 11.74 | 01-JAN-00:10 | 175.15 | 01-JAN-20:10
Electricity:Zone:TZ_0-A1.WC | 1.78 | 27.02 | 01-JAN-03:10 | 103.46 | 01-JAN-19:10
InteriorLights:Electricity:Zone:TZ_0-A1.WC | 0.47 | 3.04 | 01-JAN-00:10 | 45.42 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_0-A1.WC | 0.47 | 3.04 | 01-JAN-00:10 | 45.42 | 01-JAN-20:10
Electricity:Zone:TZ_1-A2.B | 3.75 | 56.88 | 01-JAN-03:10 | 217.80 | 01-JAN-19:10
InteriorLights:Electricity:Zone:TZ_1-A2.B | 0.99 | 6.41 | 01-JAN-00:10 | 95.63 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_1-A2.B | 0.99 | 6.41 | 01-JAN-00:10 | 95.63 | 01-JAN-20:10
Electricity:Zone:TZ_0-A1.B | 3.75 | 56.88 | 01-JAN-03:10 | 217.80 | 01-JAN-19:10
InteriorLights:Electricity:Zone:TZ_0-A1.B | 0.99 | 6.41 | 01-JAN-00:10 | 95.63 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_0-A1.B | 0.99 | 6.41 | 01-JAN-00:10 | 95.63 | 01-JAN-20:10
Electricity:Zone:TZ_0-A1.LK | 6.86 | 104.18 | 01-JAN-03:10 | 398.93 | 01-JAN-19:10
InteriorLights:Electricity:Zone:TZ_0-A1.LK | 1.81 | 11.74 | 01-JAN-00:10 | 175.15 | 01-JAN-20:10
General:InteriorLights:Electricity:Zone:TZ_0-A1.LK | 1.81 | 11.74 | 01-JAN-00:10 | 175.15 | 01-JAN-20:10
Electricity:Zone:TZ_1-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
Electricity:SpaceType:MIDRISEAPARTMENT CORRIDOR | 13.99 | 443.65 | 01-JAN-00:10 | 443.65 | 01-JAN-00:10
InteriorLights:Electricity:Zone:TZ_1-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
InteriorLights:Electricity:SpaceType:MIDRISEAPARTMENT CORRIDOR | 13.99 | 443.65 | 01-JAN-00:10 | 443.65 | 01-JAN-00:10
General:InteriorLights:Electricity:Zone:TZ_1-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
General:InteriorLights:Electricity:SpaceType:MIDRISEAPARTMENT CORRIDOR | 13.99 | 443.65 | 01-JAN-00:10 | 443.65 | 01-JAN-00:10
Electricity:Zone:TZ_0-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
InteriorLights:Electricity:Zone:TZ_0-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
General:InteriorLights:Electricity:Zone:TZ_0-H | 7.00 | 221.82 | 01-JAN-00:10 | 221.82 | 01-JAN-00:10
InteriorEquipment:Electricity | 18.22 | 333.77 | 01-JAN-03:10 | 878.34 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_1-A2.WC | 1.31 | 23.97 | 01-JAN-03:10 | 63.09 | 01-JAN-17:10
InteriorEquipment:Electricity:SpaceType:MIDRISEAPARTMENT APARTMENT | 18.22 | 333.77 | 01-JAN-03:10 | 878.34 | 01-JAN-17:10
General:InteriorEquipment:Electricity | 18.22 | 333.77 | 01-JAN-03:10 | 878.34 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.WC | 1.31 | 23.97 | 01-JAN-03:10 | 63.09 | 01-JAN-17:10
General:InteriorEquipment:Electricity:SpaceType:MIDRISEAPARTMENT APARTMENT | 18.22 | 333.77 | 01-JAN-03:10 | 878.34 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_1-A2.LK | 5.05 | 92.44 | 01-JAN-03:10 | 243.26 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.LK | 5.05 | 92.44 | 01-JAN-03:10 | 243.26 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_0-A1.WC | 1.31 | 23.97 | 01-JAN-03:10 | 63.09 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.WC | 1.31 | 23.97 | 01-JAN-03:10 | 63.09 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_1-A2.B | 2.76 | 50.47 | 01-JAN-03:10 | 132.81 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.B | 2.76 | 50.47 | 01-JAN-03:10 | 132.81 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 2.76 | 50.47 | 01-JAN-03:10 | 132.81 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 2.76 | 50.47 | 01-JAN-03:10 | 132.81 | 01-JAN-17:10
InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 5.05 | 92.44 | 01-JAN-03:10 | 243.26 | 01-JAN-17:10
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 5.05 | 92.44 | 01-JAN-03:10 | 243.26 | 01-JAN-17:10
Fans:Electricity | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_0-A1.B | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_0-A1.B | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_0-A1.LK | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_0-A1.LK | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_0-A1.WC | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_0-A1.WC | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_1-A2.B | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_1-A2.B | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_1-A2.LK | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_1-A2.LK | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Fans:Electricity:Zone:TZ_1-A2.WC | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:TZ_1-A2.WC | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
ElectricityPurchased:Facility | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
ElectricityPurchased:Plant | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
Cogeneration:ElectricityPurchased | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
General:Cogeneration:ElectricityPurchased | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
ElectricitySurplusSold:Facility | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
ElectricitySurplusSold:Plant | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Cogeneration:ElectricitySurplusSold | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
General:Cogeneration:ElectricitySurplusSold | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
ElectricityNet:Facility | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
ElectricityNet:Plant | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
Cogeneration:ElectricityNet | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10
General:Cogeneration:ElectricityNet | 38.76 | 819.78 | 01-JAN-03:10 | 1884.04 | 01-JAN-19:10

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Natural Gas

| Natural Gas Annual Value [GJ] | Natural Gas Minimum Value [W] | Timestamp of Minimum {TIMESTAMP} | Natural Gas Maximum Value [W] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Cooling

| Cooling Annual Value [GJ] | Cooling Minimum Value [W] | Timestamp of Minimum {TIMESTAMP} | Cooling Maximum Value [W] | Timestamp of Maximum {TIMESTAMP}
DistrictCooling:Facility | 5.26 | 0.00 | 01-JAN-00:10 | 5825.27 | 21-JUL-19:00
DistrictCooling:HVAC | 5.26 | 0.00 | 01-JAN-00:10 | 5825.27 | 21-JUL-19:00
Cooling:DistrictCooling | 5.26 | 0.00 | 01-JAN-00:10 | 5825.27 | 21-JUL-19:00
General:Cooling:DistrictCooling | 5.26 | 0.00 | 01-JAN-00:10 | 5825.27 | 21-JUL-19:00

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Water

| Annual Value [m3] | Minimum Value [m3/s] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [m3/s] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other by Weight/Mass

| Annual Value [kg] | Minimum Value [kg/s] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [kg/s] | Timestamp of Maximum {TIMESTAMP}
Carbon Equivalent:Facility | 0.00 | 0.000 | 01-JAN-00:10 | 0.000 | 01-JAN-00:10
CarbonEquivalentEmissions:Carbon Equivalent | 0.00 | 0.000 | 01-JAN-00:10 | 0.000 | 01-JAN-00:10

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other Volumetric

| Annual Value [m3] | Minimum Value [m3/s] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [m3/s] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other Liquid/Gas

| Annual Value [L] | Minimum Value [L] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [L] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other

| Annual Value [GJ] | Minimum Value [W] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [W] | Timestamp of Maximum {TIMESTAMP}
EnergyTransfer:Facility | 102.77 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
EnergyTransfer:Building | 102.77 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
EnergyTransfer:Zone:TZ_0-A1.B | 15.23 | 0.00 | 06-MAR-16:10 | 2097.12 | 30-JAN-04:00
Heating:EnergyTransfer | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_0-A1.B | 15.14 | 0.00 | 06-MAR-16:10 | 2097.12 | 30-JAN-04:00
General:Heating:EnergyTransfer | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_0-A1.B | 15.14 | 0.00 | 06-MAR-16:10 | 2097.12 | 30-JAN-04:00
Cooling:EnergyTransfer | 3.82 | 0.00 | 01-JAN-00:10 | 4436.58 | 24-JUL-18:10
Cooling:EnergyTransfer:Zone:TZ_0-A1.B | 0.09 | 0.00 | 01-JAN-00:10 | 444.10 | 24-JUL-18:10
General:Cooling:EnergyTransfer | 3.82 | 0.00 | 01-JAN-00:10 | 4436.58 | 24-JUL-18:10
General:Cooling:EnergyTransfer:Zone:TZ_0-A1.B | 0.09 | 0.00 | 01-JAN-00:10 | 444.10 | 24-JUL-18:10
EnergyTransfer:Zone:TZ_0-A1.LK | 21.65 | 0.00 | 06-MAR-15:20 | 3156.56 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_0-A1.LK | 21.48 | 0.00 | 06-MAR-15:20 | 3156.56 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_0-A1.LK | 21.48 | 0.00 | 06-MAR-15:20 | 3156.56 | 30-JAN-04:00
Cooling:EnergyTransfer:Zone:TZ_0-A1.LK | 0.16 | 0.00 | 01-JAN-00:10 | 724.49 | 24-JUL-18:10
General:Cooling:EnergyTransfer:Zone:TZ_0-A1.LK | 0.16 | 0.00 | 01-JAN-00:10 | 724.49 | 24-JUL-18:10
EnergyTransfer:Zone:TZ_0-A1.WC | 10.94 | 0.00 | 06-MAR-15:30 | 1452.07 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_0-A1.WC | 10.86 | 0.00 | 06-MAR-15:30 | 1452.07 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_0-A1.WC | 10.86 | 0.00 | 06-MAR-15:30 | 1452.07 | 30-JAN-04:00
Cooling:EnergyTransfer:Zone:TZ_0-A1.WC | 0.07 | 0.00 | 01-JAN-00:10 | 263.85 | 21-JUL-19:00
General:Cooling:EnergyTransfer:Zone:TZ_0-A1.WC | 0.07 | 0.00 | 01-JAN-00:10 | 263.85 | 21-JUL-19:00
EnergyTransfer:Zone:TZ_0-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Heating:EnergyTransfer:Zone:TZ_0-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
General:Heating:EnergyTransfer:Zone:TZ_0-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Cooling:EnergyTransfer:Zone:TZ_0-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
General:Cooling:EnergyTransfer:Zone:TZ_0-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
EnergyTransfer:Zone:TZ_1-A2.B | 17.08 | 0.00 | 01-MAR-15:30 | 2332.81 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_1-A2.B | 16.11 | 0.00 | 01-MAR-15:30 | 2332.81 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_1-A2.B | 16.11 | 0.00 | 01-MAR-15:30 | 2332.81 | 30-JAN-04:00
Cooling:EnergyTransfer:Zone:TZ_1-A2.B | 0.96 | 0.00 | 01-JAN-00:10 | 913.88 | 24-JUL-18:10
General:Cooling:EnergyTransfer:Zone:TZ_1-A2.B | 0.96 | 0.00 | 01-JAN-00:10 | 913.88 | 24-JUL-18:10
EnergyTransfer:Zone:TZ_1-A2.LK | 25.91 | 0.00 | 17-FEB-16:10 | 3702.72 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_1-A2.LK | 23.98 | 0.00 | 17-FEB-16:10 | 3702.72 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_1-A2.LK | 23.98 | 0.00 | 17-FEB-16:10 | 3702.72 | 30-JAN-04:00
Cooling:EnergyTransfer:Zone:TZ_1-A2.LK | 1.93 | 0.00 | 01-JAN-00:10 | 1637.14 | 23-JUL-17:10
General:Cooling:EnergyTransfer:Zone:TZ_1-A2.LK | 1.93 | 0.00 | 01-JAN-00:10 | 1637.14 | 23-JUL-17:10
EnergyTransfer:Zone:TZ_1-A2.WC | 11.97 | 0.00 | 01-MAR-14:00 | 1578.08 | 30-JAN-04:00
Heating:EnergyTransfer:Zone:TZ_1-A2.WC | 11.37 | 0.00 | 01-MAR-14:00 | 1578.08 | 30-JAN-04:00
General:Heating:EnergyTransfer:Zone:TZ_1-A2.WC | 11.37 | 0.00 | 01-MAR-14:00 | 1578.08 | 30-JAN-04:00
Cooling:EnergyTransfer:Zone:TZ_1-A2.WC | 0.59 | 0.00 | 01-JAN-00:10 | 526.97 | 24-JUL-13:30
General:Cooling:EnergyTransfer:Zone:TZ_1-A2.WC | 0.59 | 0.00 | 01-JAN-00:10 | 526.97 | 24-JUL-13:30
EnergyTransfer:Zone:TZ_1-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Heating:EnergyTransfer:Zone:TZ_1-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
General:Heating:EnergyTransfer:Zone:TZ_1-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
Cooling:EnergyTransfer:Zone:TZ_1-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
General:Cooling:EnergyTransfer:Zone:TZ_1-H | 0.00 | 0.00 | 01-JAN-00:10 | 0.00 | 01-JAN-00:10
DistrictHeatingWater:Facility | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
DistrictHeatingWater:HVAC | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
Heating:DistrictHeatingWater | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00
General:Heating:DistrictHeatingWater | 98.95 | 0.00 | 06-MAR-16:10 | 14319.37 | 30-JAN-04:00

Values shown are for all completed run periods - including any simulations run during sizing periods

Table of Contents

Report: Sensible Heat Gain Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Annual Building Sensible Heat Gain Components

| HVAC Zone Eq & Other Sensible Air Heating [GJ] | HVAC Zone Eq & Other Sensible Air Cooling [GJ] | HVAC Terminal Unit Sensible Air Heating [GJ] | HVAC Terminal Unit Sensible Air Cooling [GJ] | HVAC Input Heated Surface Heating [GJ] | HVAC Input Cooled Surface Cooling [GJ] | People Sensible Heat Addition [GJ] | Lights Sensible Heat Addition [GJ] | Equipment Sensible Heat Addition [GJ] | Window Heat Addition [GJ] | Interzone Air Transfer Heat Addition [GJ] | Infiltration Heat Addition [GJ] | Opaque Surface Conduction and Other Heat Addition [GJ] | Equipment Sensible Heat Removal [GJ] | Window Heat Removal [GJ] | Interzone Air Transfer Heat Removal [GJ] | Infiltration Heat Removal [GJ] | Opaque Surface Conduction and Other Heat Removal [GJ]
TZ_0-A1.B | 15.139 | -0.093 | 0.000 | 0.000 | 0.000 | 0.000 | 1.254 | 0.990 | 2.756 | 0.958 | 0.000 | 0.224 | 0.000 | 0.000 | -1.438 | 0.000 | -14.108 | -5.680
TZ_0-A1.LK | 21.482 | -0.165 | 0.000 | 0.000 | 0.000 | 0.000 | 2.286 | 1.814 | 5.047 | 1.436 | 0.000 | 0.269 | 0.000 | 0.000 | -2.136 | 0.000 | -18.923 | -11.111
TZ_0-A1.WC | 10.863 | -0.074 | 0.000 | 0.000 | 0.000 | 0.000 | 0.596 | 0.470 | 1.309 | 0.465 | 0.000 | 0.133 | 0.000 | 0.000 | -0.711 | 0.000 | -9.975 | -3.076
TZ_1-A2.B | 16.115 | -0.965 | 0.000 | 0.000 | 0.000 | 0.000 | 1.233 | 0.990 | 2.756 | 0.854 | 0.000 | 0.116 | 0.000 | 0.000 | -1.455 | 0.000 | -14.559 | -5.085
TZ_1-A2.LK | 23.977 | -1.931 | 0.000 | 0.000 | 0.000 | 0.000 | 2.245 | 1.814 | 5.047 | 1.268 | 0.000 | 0.146 | 0.000 | 0.000 | -2.151 | 0.000 | -19.584 | -10.831
TZ_1-A2.WC | 11.373 | -0.593 | 0.000 | 0.000 | 0.000 | 0.000 | 0.588 | 0.470 | 1.309 | 0.420 | 0.000 | 0.085 | 0.000 | 0.000 | -0.722 | 0.000 | -10.290 | -2.640
TZ_0-H | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 6.995 | 0.000 | 3.566 | 0.000 | 0.016 | 2.118 | 0.000 | -2.900 | 0.000 | -9.796 | 0.000
TZ_1-H | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 6.995 | 0.000 | 1.980 | 0.000 | 0.000 | 1.927 | 0.000 | -0.974 | 0.000 | -9.928 | 0.000
Total Facility | 98.948 | -3.821 | 0.000 | 0.000 | 0.000 | 0.000 | 8.202 | 20.539 | 18.224 | 10.947 | 0.000 | 0.990 | 4.045 | 0.000 | -12.488 | 0.000 | -107.163 | -38.422

Peak Cooling Sensible Heat Gain Components

| Time of Peak {TIMESTAMP} | HVAC Zone Eq & Other Sensible Air Heating [W] | HVAC Zone Eq & Other Sensible Air Cooling [W] | HVAC Terminal Unit Sensible Air Heating [W] | HVAC Terminal Unit Sensible Air Cooling [W] | HVAC Input Heated Surface Heating [W] | HVAC Input Cooled Surface Cooling [W] | People Sensible Heat Addition [W] | Lights Sensible Heat Addition [W] | Equipment Sensible Heat Addition [W] | Window Heat Addition [W] | Interzone Air Transfer Heat Addition [W] | Infiltration Heat Addition [W] | Opaque Surface Conduction and Other Heat Addition [W] | Equipment Sensible Heat Removal [W] | Window Heat Removal [W] | Interzone Air Transfer Heat Removal [W] | Infiltration Heat Removal [W] | Opaque Surface Conduction and Other Heat Removal [W]
TZ_0-A1.B | 24-JUL-18:10 | 0.00 | -444.10 | 0.00 | 0.00 | 0.00 | 0.00 | 36.29 | 79.27 | 132.81 | 293.34 | 0.00 | 253.45 | 0.00 | 0.00 | -0.00 | 0.00 | 0.00 | -351.07
TZ_0-A1.LK | 24-JUL-18:10 | 0.00 | -724.51 | 0.00 | 0.00 | 0.00 | 0.00 | 66.47 | 145.20 | 243.26 | 439.58 | 0.00 | 341.49 | 0.00 | 0.00 | -0.00 | 0.00 | 0.00 | -511.50
TZ_0-A1.WC | 21-JUL-18:00 | 0.00 | -263.88 | 0.00 | 0.00 | 0.00 | 0.00 | 17.24 | 37.66 | 63.09 | 24.68 | 0.00 | 202.31 | 0.00 | 0.00 | -0.00 | 0.00 | 0.00 | -81.10
TZ_1-A2.B | 24-JUL-18:10 | 0.00 | -913.94 | 0.00 | 0.00 | 0.00 | 0.00 | 36.29 | 79.27 | 132.81 | 281.38 | 0.00 | 252.67 | 131.51 | 0.00 | -0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.LK | 23-JUL-17:10 | 0.00 | -1637.27 | 0.00 | 0.00 | 0.00 | 0.00 | 39.73 | 107.89 | 243.26 | 572.26 | 0.00 | 275.21 | 398.92 | 0.00 | -0.00 | 0.00 | 0.00 | 0.00
TZ_1-A2.WC | 24-JUL-13:30 | 0.00 | -526.98 | 0.00 | 0.00 | 0.00 | 0.00 | 4.95 | 5.41 | 41.64 | 54.88 | 0.00 | 154.73 | 265.37 | 0.00 | -0.00 | 0.00 | 0.00 | 0.00
TZ_0-H | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Facility | 24-JUL-18:10 | 0.00 | -4436.82 | 0.00 | 0.00 | 0.00 | 0.00 | 240.01 | 967.91 | 878.34 | 1995.26 | 0.00 | 1543.14 | 0.00 | 0.00 | 0.00 | 0.00 | -190.85 | -996.98

Peak Heating Sensible Heat Gain Components

| Time of Peak {TIMESTAMP} | HVAC Zone Eq & Other Sensible Air Heating [W] | HVAC Zone Eq & Other Sensible Air Cooling [W] | HVAC Terminal Unit Sensible Air Heating [W] | HVAC Terminal Unit Sensible Air Cooling [W] | HVAC Input Heated Surface Heating [W] | HVAC Input Cooled Surface Cooling [W] | People Sensible Heat Addition [W] | Lights Sensible Heat Addition [W] | Equipment Sensible Heat Addition [W] | Window Heat Addition [W] | Interzone Air Transfer Heat Addition [W] | Infiltration Heat Addition [W] | Opaque Surface Conduction and Other Heat Addition [W] | Equipment Sensible Heat Removal [W] | Window Heat Removal [W] | Interzone Air Transfer Heat Removal [W] | Infiltration Heat Removal [W] | Opaque Surface Conduction and Other Heat Removal [W]
TZ_0-A1.B | 30-JAN-03:00 | 2097.09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 60.50 | 6.41 | 50.47 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -169.38 | 0.00 | -1700.85 | -344.24
TZ_0-A1.LK | 30-JAN-03:00 | 3156.50 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 110.82 | 11.74 | 92.44 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -250.57 | 0.00 | -2322.52 | -798.41
TZ_0-A1.WC | 30-JAN-03:00 | 1452.05 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 28.74 | 3.04 | 23.97 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -84.40 | 0.00 | -1178.86 | -244.54
TZ_1-A2.B | 30-JAN-03:00 | 2332.77 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 60.50 | 6.41 | 50.47 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -166.18 | 0.00 | -1701.93 | -582.04
TZ_1-A2.LK | 30-JAN-03:00 | 3702.66 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 110.82 | 11.74 | 92.44 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -243.85 | 0.00 | -2323.99 | -1349.82
TZ_1-A2.WC | 30-JAN-03:00 | 1578.06 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 28.74 | 3.04 | 23.97 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -83.03 | 0.00 | -1179.61 | -371.18
TZ_0-H | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
TZ_1-H | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Facility | 30-JAN-03:00 | 14319.12 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 400.11 | 486.02 | 333.77 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -1382.29 | 0.00 | -12067.81 | -2088.92

Table of Contents

Report: LEED Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Sec1.1A-General Information

| Data
Weather File | RUN PERIOD 1 ** MILAN - ITA IWEC Data WMO#=160660
Total gross floor area [m2] | 208.00
Principal Heating Source | District Heating Water

EAp2-1. Space Usage Type

| Space Area [m2] | Regularly Occupied Area [m2] | Unconditioned Area [m2] | Typical Hours/Week in Operation [hr/wk]
TZ_0-A1.B | 24.68 | 24.68 | 0.00 | 168.00
TZ_0-A1.LK | 45.20 | 45.20 | 0.00 | 168.00
TZ_0-A1.WC | 11.72 | 11.72 | 0.00 | 168.00
TZ_1-A2.B | 24.68 | 24.68 | 0.00 | 168.00
TZ_1-A2.LK | 45.20 | 45.20 | 0.00 | 168.00
TZ_1-A2.WC | 11.72 | 11.72 | 0.00 | 168.00
TZ_0-H | 22.40 | 0.00 | 22.40 | 0.00
TZ_1-H | 22.40 | 0.00 | 22.40 | 0.00
Totals | 208.00 | 163.20 | 44.80 |

EAp2-2. Advisory Messages

| Data
Number of hours heating loads not met | 0.00
Number of hours cooling loads not met | 0.00
Number of hours not met | 0.00

EAp2-3. Energy Type Summary

| Utility Rate | Virtual Rate [$/unit energy] | Units of Energy | Units of Demand
None |  |  |  |

EAp2-4/5. Performance Rating Method Compliance

| Electricity Energy Use [GJ] | Electricity Demand [W] | Natural Gas Energy Use [GJ] | Natural Gas Demand [W] | Gasoline Use [GJ] | Gasoline Demand [W] | Diesel Use [GJ] | Diesel Demand [W] | Coal Use [GJ] | Coal Demand [W] | Fuel Oil No 1 Use [GJ] | Fuel Oil No 1 Demand [W] | Fuel Oil No 2 Use [GJ] | Fuel Oil No 2 Demand [W] | Propane Use [GJ] | Propane Demand [W] | Other Fuel 1 Use [GJ] | Other Fuel 1 Demand [W] | Other Fuel 2 Use [GJ] | Other Fuel 2 Demand [W] | District Cooling Use [GJ] | District Cooling Demand [W] | District Heating Water Use [GJ] | District Heating Water Demand [W] | District Heating Steam Use [GJ] | District Heating Steam Demand [W]
Heating -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 98.95 | 14319.37 | 0.00 | 0.00
Cooling -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5.26 | 5825.27 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting -- General | 20.54 | 1076.05 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- General | 18.22 | 878.34 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans -- Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

EAp2-6. Energy Use Summary

| Process Subtotal [GJ] | Total Energy Use [GJ]
Electricity | 18.22 | 38.76
Natural Gas | 0.00 | 0.00
Additional | 0.00 | 104.21
Total | 18.22 | 142.97

EAp2-7. Energy Cost Summary

| Process Subtotal [$] | Total Energy Cost [$]
Electricity | 0.00 |
Natural Gas | 0.00 |
Additional | 0.00 |
Total | 0.00 |

Process energy cost based on ratio of process to total energy.
L-1. Renewable Energy Source Summary

| Rated Capacity [kW] | Annual Energy Generated [GJ]
Photovoltaic | 0.00 | 0.00
Wind | 0.00 | 0.00

EAp2-17a. Energy Use Intensity - Electricity

| Electricty [MJ/m2]
Interior Lighting (All) | 98.74
Space Heating | 0.00
Space Cooling | 0.00
Fans (All) | 0.00
Service Water Heating | 0.00
Receptacle Equipment | 87.61
Miscellaneous (All) | 186.36
Subtotal | 186.36

EAp2-17b. Energy Use Intensity - Natural Gas

| Natural Gas [MJ/m2]
Space Heating | 0.00
Service Water Heating | 0.00
Miscellaneous (All) | 0.00
Subtotal | 0.00

EAp2-17c. Energy Use Intensity - Additional

| Additional [MJ/m2]
Subtotal | 0.00
Miscellaneous | 0.00

EAp2-18. End Use Percentage

| Percent [%]
Interior Lighting (All) | 14.37
Space Heating | 69.21
Space Cooling | 3.68
Fans (All) | 0.00
Service Water Heating | 0.00
Receptacle Equipment | 12.75
Miscellaneous | 0.00

Schedules-Equivalent Full Load Hours (Schedule Type=Fraction)

| Equivalent Full Load Hours of Operation Per Year [hr] | Hours > 1% [hr]
None |  |

Schedules-SetPoints (Schedule Type=Temperature)

| First Object Used | Month Assumed | 11am First Wednesday [C] | Days with Same 11am Value | 11pm First Wednesday [C] | Days with Same 11pm Value
HEATING SETPOINT | THERMOSTAT SETPOINT DUAL SETPOINT 1 | January | 20.00 | 365 | 20.00 | 365
COOLING SETPOINT | THERMOSTAT SETPOINT DUAL SETPOINT 1 | July | 26.00 | 365 | 26.00 | 365

Table of Contents

Report: Annual CO2 Resilience Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

CO2 Level Hours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

CO2 Level OccupantHours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

CO2 Level OccupiedHours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

Table of Contents

Report: Annual Visual Resilience Summary

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Illuminance Level Hours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Illuminance Level OccupantHours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Illuminance Level OccupiedHours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - ELECTRICITY

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| INTERIORLIGHTS:ELECTRICITY [J] | EXTERIORLIGHTS:ELECTRICITY [] | INTERIOREQUIPMENT:ELECTRICITY [J] | EXTERIOREQUIPMENT:ELECTRICITY [] | FANS:ELECTRICITY [J] | PUMPS:ELECTRICITY [] | HEATING:ELECTRICITY [] | COOLING:ELECTRICITY [] | HEATREJECTION:ELECTRICITY [] | HUMIDIFIER:ELECTRICITY [] | HEATRECOVERY:ELECTRICITY [] | WATERSYSTEMS:ELECTRICITY [] | COGENERATION:ELECTRICITY [] | REFRIGERATION:ELECTRICITY []
January | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 0.157559E+10 | 0.00 | 0.139799E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 0.168813E+10 | 0.00 | 0.149784E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 0.168813E+10 | 0.00 | 0.149784E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 0.168813E+10 | 0.00 | 0.149784E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 0.168813E+10 | 0.00 | 0.149784E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average | 0.205389E+11 | 0.00 | 0.182237E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 0.157559E+10 | 0.00 | 0.139799E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 0.174440E+10 | 0.00 | 0.154777E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - DISTRICT HEATING WATER

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| INTERIORLIGHTS:DISTRICTHEATINGWATER [] | EXTERIORLIGHTS:DISTRICTHEATINGWATER [] | INTERIOREQUIPMENT:DISTRICTHEATINGWATER [] | EXTERIOREQUIPMENT:DISTRICTHEATINGWATER [] | FANS:DISTRICTHEATINGWATER [] | PUMPS:DISTRICTHEATINGWATER [] | HEATING:DISTRICTHEATINGWATER [J] | COOLING:DISTRICTHEATINGWATER [] | HEATREJECTION:DISTRICTHEATINGWATER [] | HUMIDIFIER:DISTRICTHEATINGWATER [] | HEATRECOVERY:DISTRICTHEATINGWATER [] | WATERSYSTEMS:DISTRICTHEATINGWATER [] | COGENERATION:DISTRICTHEATINGWATER []
January | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.210439E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.164374E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.113845E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.720673E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.246728E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.735677E+09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 31453800.17 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 87050660.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.173752E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.610833E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.129188E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.187892E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.989479E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 31453800.17 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.210439E+11 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - DISTRICT COOLING

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| INTERIORLIGHTS:DISTRICTCOOLING [] | EXTERIORLIGHTS:DISTRICTCOOLING [] | INTERIOREQUIPMENT:DISTRICTCOOLING [] | EXTERIOREQUIPMENT:DISTRICTCOOLING [] | FANS:DISTRICTCOOLING [] | PUMPS:DISTRICTCOOLING [] | HEATING:DISTRICTCOOLING [] | COOLING:DISTRICTCOOLING [J] | HEATREJECTION:DISTRICTCOOLING [] | HUMIDIFIER:DISTRICTCOOLING [] | HEATRECOVERY:DISTRICTCOOLING [] | WATERSYSTEMS:DISTRICTCOOLING [] | COGENERATION:DISTRICTCOOLING []
January | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.188528E+09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.113575E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.239369E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.134418E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.198386E+09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.526053E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.239369E+10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - ELECTRICITY PEAK DEMAND

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| ELECTRICITY:FACILITY {Maximum} [W] | ELECTRICITY:FACILITY {TIMESTAMP} | INTERIORLIGHTS:ELECTRICITY {AT MAX/MIN} [W] | EXTERIORLIGHTS:ELECTRICITY [] | INTERIOREQUIPMENT:ELECTRICITY {AT MAX/MIN} [W] | EXTERIOREQUIPMENT:ELECTRICITY [] | FANS:ELECTRICITY {AT MAX/MIN} [W] | PUMPS:ELECTRICITY [] | HEATING:ELECTRICITY [] | COOLING:ELECTRICITY [] | HEATREJECTION:ELECTRICITY [] | HUMIDIFIER:ELECTRICITY [] | HEATRECOVERY:ELECTRICITY [] | WATERSYSTEMS:ELECTRICITY [] | COGENERATION:ELECTRICITY [] | REFRIGERATION:ELECTRICITY []
January | 1884.04 | 01-JAN-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 1884.04 | 01-FEB-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 1884.04 | 01-MAR-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 1884.04 | 01-APR-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 1884.04 | 01-MAY-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 1884.04 | 01-JUN-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 1884.04 | 01-JUL-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 1884.04 | 01-AUG-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 1884.04 | 01-SEP-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 1884.04 | 01-OCT-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 1884.04 | 01-NOV-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 1884.04 | 01-DEC-19:20 | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average |  |  |  | 0.00 |  | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 1884.04 |  | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 1884.04 |  | 1067.19 | 0.00 | 816.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - DISTRICT HEATING WATER PEAK DEMAND

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| DISTRICTHEATINGWATER:FACILITY {Maximum} [W] | DISTRICTHEATINGWATER:FACILITY {TIMESTAMP} | INTERIORLIGHTS:DISTRICTHEATINGWATER [] | EXTERIORLIGHTS:DISTRICTHEATINGWATER [] | INTERIOREQUIPMENT:DISTRICTHEATINGWATER [] | EXTERIOREQUIPMENT:DISTRICTHEATINGWATER [] | FANS:DISTRICTHEATINGWATER [] | PUMPS:DISTRICTHEATINGWATER [] | HEATING:DISTRICTHEATINGWATER {AT MAX/MIN} [W] | COOLING:DISTRICTHEATINGWATER [] | HEATREJECTION:DISTRICTHEATINGWATER [] | HUMIDIFIER:DISTRICTHEATINGWATER [] | HEATRECOVERY:DISTRICTHEATINGWATER [] | WATERSYSTEMS:DISTRICTHEATINGWATER [] | COGENERATION:DISTRICTHEATINGWATER []
January | 14319.37 | 30-JAN-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14319.37 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 11752.31 | 24-FEB-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 11752.31 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 10223.06 | 01-MAR-05:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 10223.06 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 9113.99 | 01-APR-05:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 9113.99 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 5246.86 | 22-MAY-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5246.86 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 5053.77 | 13-JUN-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5053.77 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 944.55 | 15-JUL-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 944.55 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 1699.75 | 13-AUG-04:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1699.75 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 4880.79 | 29-SEP-03:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 4880.79 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 8001.38 | 31-OCT-06:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 8001.38 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 10119.46 | 19-NOV-05:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 10119.46 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 12822.72 | 29-DEC-06:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 12822.72 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average |  |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 944.55 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 944.55 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 14319.37 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14319.37 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: BUILDING ENERGY PERFORMANCE - DISTRICT COOLING PEAK DEMAND

For: Meter

Timestamp: 2025-09-12 10:23:48

Custom Monthly Report

| DISTRICTCOOLING:FACILITY {Maximum} [W] | DISTRICTCOOLING:FACILITY {TIMESTAMP} | INTERIORLIGHTS:DISTRICTCOOLING [] | EXTERIORLIGHTS:DISTRICTCOOLING [] | INTERIOREQUIPMENT:DISTRICTCOOLING [] | EXTERIOREQUIPMENT:DISTRICTCOOLING [] | FANS:DISTRICTCOOLING [] | PUMPS:DISTRICTCOOLING [] | HEATING:DISTRICTCOOLING [] | COOLING:DISTRICTCOOLING {AT MAX/MIN} [W] | HEATREJECTION:DISTRICTCOOLING [] | HUMIDIFIER:DISTRICTCOOLING [] | HEATRECOVERY:DISTRICTCOOLING [] | WATERSYSTEMS:DISTRICTCOOLING [] | COGENERATION:DISTRICTCOOLING []
January | 0.00 | 01-JAN-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
February | 0.00 | 01-FEB-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
March | 0.00 | 01-MAR-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
April | 0.00 | 01-APR-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
May | 1931.85 | 25-MAY-17:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1931.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
June | 5509.00 | 26-JUN-18:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5509.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
July | 5825.27 | 21-JUL-18:10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5825.27 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
August | 4366.35 | 06-AUG-17:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 4366.35 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
September | 1912.31 | 01-SEP-16:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 1912.31 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
October | 0.00 | 01-OCT-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
November | 0.00 | 01-NOV-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
December | 0.00 | 01-DEC-00:20 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Annual Sum or Average |  |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Minimum of Months | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Maximum of Months | 5825.27 |  | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 5825.27 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Life-Cycle Cost Report

For: Entire Facility

Timestamp: 2025-09-12 10:23:48

Life-Cycle Cost Parameters

| Value
Name | LIFE CYCLE COST PARAMETERS
Discounting Convention | EndOfYear
Inflation Approach | ConstantDollar
Real Discount Rate | 0.0300
Nominal Discount Rate | -- N/A --
Inflation | -- N/A --
Base Date | January 2011
Service Date | January 2011
Length of Study Period in Years | 25
Tax rate | 0.0000
Depreciation Method | None

Use Price Escalation

| U.S. AVG COMMERCIAL-ELECTRICITY | U.S. AVG COMMERCIAL-DISTILLATE OIL | U.S. AVG COMMERCIAL-RESIDUAL OIL | U.S. AVG COMMERCIAL-NATURAL GAS | U.S. AVG COMMERCIAL-COAL
Resource | Electricity | FuelOilNo1 | FuelOilNo2 | NaturalGas | Coal
Start Date | January 2011 | January 2011 | January 2011 | January 2011 | January 2011
1 | 0.983800 | 0.971400 | 0.846900 | 0.982300 | 0.997000
2 | 0.973000 | 0.973000 | 0.825700 | 0.955700 | 1.008900
3 | 0.963200 | 0.994200 | 0.868100 | 0.927900 | 1.008900
4 | 0.961100 | 1.016400 | 0.898800 | 0.925700 | 0.994100
5 | 0.957100 | 1.054100 | 0.928900 | 0.934600 | 0.994100
6 | 0.955300 | 1.092800 | 0.960400 | 0.941200 | 1.000000
7 | 0.953900 | 1.126700 | 0.989700 | 0.951200 | 1.003000
8 | 0.952100 | 1.158000 | 1.007500 | 0.964500 | 1.005900
9 | 0.954600 | 1.179200 | 1.031400 | 0.985600 | 1.008900
10 | 0.955000 | 1.196700 | 1.055400 | 1.006700 | 1.011900
11 | 0.955300 | 1.220000 | 1.086100 | 1.022200 | 1.014800
12 | 0.956400 | 1.233300 | 1.127800 | 1.041000 | 1.017800
13 | 0.957500 | 1.256600 | 1.149700 | 1.061000 | 1.020800
14 | 0.959600 | 1.270900 | 1.162000 | 1.078700 | 1.026700
15 | 0.961800 | 1.282600 | 1.174300 | 1.094200 | 1.029700
16 | 0.961400 | 1.298500 | 1.185200 | 1.109800 | 1.035600
17 | 0.961800 | 1.310200 | 1.194800 | 1.122000 | 1.041500
18 | 0.961800 | 1.325000 | 1.203700 | 1.130800 | 1.053400
19 | 0.959300 | 1.326100 | 1.207100 | 1.138600 | 1.056400
20 | 0.958900 | 1.328200 | 1.211900 | 1.148600 | 1.059300
21 | 0.960700 | 1.332400 | 1.213900 | 1.161900 | 1.065300
22 | 0.962500 | 1.335600 | 1.219400 | 1.176300 | 1.071200
23 | 0.965000 | 1.343100 | 1.227600 | 1.191800 | 1.074200
24 | 0.970800 | 1.351000 | 1.236500 | 1.211800 | 1.080100
25 | 0.975100 | 1.356800 | 1.242000 | 1.228400 | 1.083100

Cash Flow for Recurring and Nonrecurring Costs (Without Escalation)

| DEFAULT COST
| Nonrecurring
January 2011 | 0.00
January 2012 | 0.00
January 2013 | 0.00
January 2014 | 0.00
January 2015 | 0.00
January 2016 | 0.00
January 2017 | 0.00
January 2018 | 0.00
January 2019 | 0.00
January 2020 | 0.00
January 2021 | 0.00
January 2022 | 0.00
January 2023 | 0.00
January 2024 | 0.00
January 2025 | 0.00
January 2026 | 0.00
January 2027 | 0.00
January 2028 | 0.00
January 2029 | 0.00
January 2030 | 0.00
January 2031 | 0.00
January 2032 | 0.00
January 2033 | 0.00
January 2034 | 0.00
January 2035 | 0.00

Energy and Water Cost Cash Flows (Without Escalation)

| Total
January 2011 | 0.00
January 2012 | 0.00
January 2013 | 0.00
January 2014 | 0.00
January 2015 | 0.00
January 2016 | 0.00
January 2017 | 0.00
January 2018 | 0.00
January 2019 | 0.00
January 2020 | 0.00
January 2021 | 0.00
January 2022 | 0.00
January 2023 | 0.00
January 2024 | 0.00
January 2025 | 0.00
January 2026 | 0.00
January 2027 | 0.00
January 2028 | 0.00
January 2029 | 0.00
January 2030 | 0.00
January 2031 | 0.00
January 2032 | 0.00
January 2033 | 0.00
January 2034 | 0.00
January 2035 | 0.00

Energy and Water Cost Cash Flows (With Escalation)

| Total
January 2011 | 0.00
January 2012 | 0.00
January 2013 | 0.00
January 2014 | 0.00
January 2015 | 0.00
January 2016 | 0.00
January 2017 | 0.00
January 2018 | 0.00
January 2019 | 0.00
January 2020 | 0.00
January 2021 | 0.00
January 2022 | 0.00
January 2023 | 0.00
January 2024 | 0.00
January 2025 | 0.00
January 2026 | 0.00
January 2027 | 0.00
January 2028 | 0.00
January 2029 | 0.00
January 2030 | 0.00
January 2031 | 0.00
January 2032 | 0.00
January 2033 | 0.00
January 2034 | 0.00
January 2035 | 0.00

Capital Cash Flow by Category (Without Escalation)

| Construction | Salvage | OtherCapital | Total
January 2011 | 0.00 | 0.00 | 0.00 | 0.00
January 2012 | 0.00 | 0.00 | 0.00 | 0.00
January 2013 | 0.00 | 0.00 | 0.00 | 0.00
January 2014 | 0.00 | 0.00 | 0.00 | 0.00
January 2015 | 0.00 | 0.00 | 0.00 | 0.00
January 2016 | 0.00 | 0.00 | 0.00 | 0.00
January 2017 | 0.00 | 0.00 | 0.00 | 0.00
January 2018 | 0.00 | 0.00 | 0.00 | 0.00
January 2019 | 0.00 | 0.00 | 0.00 | 0.00
January 2020 | 0.00 | 0.00 | 0.00 | 0.00
January 2021 | 0.00 | 0.00 | 0.00 | 0.00
January 2022 | 0.00 | 0.00 | 0.00 | 0.00
January 2023 | 0.00 | 0.00 | 0.00 | 0.00
January 2024 | 0.00 | 0.00 | 0.00 | 0.00
January 2025 | 0.00 | 0.00 | 0.00 | 0.00
January 2026 | 0.00 | 0.00 | 0.00 | 0.00
January 2027 | 0.00 | 0.00 | 0.00 | 0.00
January 2028 | 0.00 | 0.00 | 0.00 | 0.00
January 2029 | 0.00 | 0.00 | 0.00 | 0.00
January 2030 | 0.00 | 0.00 | 0.00 | 0.00
January 2031 | 0.00 | 0.00 | 0.00 | 0.00
January 2032 | 0.00 | 0.00 | 0.00 | 0.00
January 2033 | 0.00 | 0.00 | 0.00 | 0.00
January 2034 | 0.00 | 0.00 | 0.00 | 0.00
January 2035 | 0.00 | 0.00 | 0.00 | 0.00

Operating Cash Flow by Category (Without Escalation)

| Maintenance | Repair | Operation | Replacement | MinorOverhaul | MajorOverhaul | OtherOperational | Water | Energy | Total
January 2011 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2012 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2013 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2014 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2015 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2016 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2017 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2018 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2019 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2020 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2021 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2022 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2023 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2024 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2025 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2026 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2027 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2028 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2029 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2030 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2031 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2032 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2033 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2034 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2035 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Operating Cash Flow by Category (With Escalation)

| Maintenance | Repair | Operation | Replacement | MinorOverhaul | MajorOverhaul | OtherOperational | Water | Energy | Total
January 2011 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2012 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2013 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2014 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2015 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2016 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2017 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2018 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2019 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2020 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2021 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2022 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2023 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2024 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2025 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2026 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2027 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2028 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2029 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2030 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2031 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2032 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2033 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2034 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
January 2035 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Monthly Total Cash Flow (Without Escalation)

| January | February | March | April | May | June | July | August | September | October | November | December
2011 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2012 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2013 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2014 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2015 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2016 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2017 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2018 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2019 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2020 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2021 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2022 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2023 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2024 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2025 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2026 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2027 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2028 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2029 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2030 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2031 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2032 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2033 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2034 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
2035 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Present Value for Recurring, Nonrecurring and Energy Costs (Before Tax)

| Category | Kind | Cost | Present Value | Present Value Factor
DEFAULT COST | Construction | Nonrecurring | 0.00 | 0.00 | -
TOTAL |  |  |  | 0.00 |

Present Value by Category

| Present Value
Maintenance | 0.00
Repair | 0.00
Operation | 0.00
Replacement | 0.00
Minor Overhaul | 0.00
Major Overhaul | 0.00
Other Operational | 0.00
Water | 0.00
Energy | 0.00
Total Operation | 0.00
Construction | 0.00
Salvage | 0.00
Other Capital | 0.00
Total Capital | 0.00
Total Energy | 0.00
Grand Total | 0.00

Present Value by Year

| Total Cost (Without Escalation) | Total Cost (With Escalation) | Present Value of Costs
January 2011 | 0.00 | 0.00 | 0.00
January 2012 | 0.00 | 0.00 | 0.00
January 2013 | 0.00 | 0.00 | 0.00
January 2014 | 0.00 | 0.00 | 0.00
January 2015 | 0.00 | 0.00 | 0.00
January 2016 | 0.00 | 0.00 | 0.00
January 2017 | 0.00 | 0.00 | 0.00
January 2018 | 0.00 | 0.00 | 0.00
January 2019 | 0.00 | 0.00 | 0.00
January 2020 | 0.00 | 0.00 | 0.00
January 2021 | 0.00 | 0.00 | 0.00
January 2022 | 0.00 | 0.00 | 0.00
January 2023 | 0.00 | 0.00 | 0.00
January 2024 | 0.00 | 0.00 | 0.00
January 2025 | 0.00 | 0.00 | 0.00
January 2026 | 0.00 | 0.00 | 0.00
January 2027 | 0.00 | 0.00 | 0.00
January 2028 | 0.00 | 0.00 | 0.00
January 2029 | 0.00 | 0.00 | 0.00
January 2030 | 0.00 | 0.00 | 0.00
January 2031 | 0.00 | 0.00 | 0.00
January 2032 | 0.00 | 0.00 | 0.00
January 2033 | 0.00 | 0.00 | 0.00
January 2034 | 0.00 | 0.00 | 0.00
January 2035 | 0.00 | 0.00 | 0.00
TOTAL |  |  | 0.00