
OS:Version,
  {11347fb1-b056-449e-95b6-1f3ee75a48b0}, !- Handle
  3.9.0;                                  !- Version Identifier

OS:Site,
  {7cc869db-3472-458f-9d58-fb4eb8be8e96}, !- Handle
  MILAN,                                  !- Name
  45.62,                                  !- Latitude {deg}
  8.73,                                   !- Longitude {deg}
  1,                                      !- Time Zone {hr}
  211,                                    !- Elevation {m}
  ;                                       !- Terrain

OS:YearDescription,
  {b36fd2e6-245d-46dc-a386-dbab26100f31}, !- Handle
  ,                                       !- Calendar Year
  Sunday;                                 !- Day of Week for Start Day

OS:ClimateZones,
  {f3aa98ed-b133-4f1c-b223-35af031f76c9}, !- Handle
  ASHRAE,                                 !- Climate Zone Institution Name 1
  ANSI/ASHRAE Standard 169,               !- Climate Zone Document Name 1
  2006,                                   !- Climate Zone Document Year 1
  ,                                       !- Climate Zone Value 1
  CEC,                                    !- Climate Zone Institution Name 2
  California Climate Zone Descriptions,   !- Climate Zone Document Name 2
  1995,                                   !- Climate Zone Document Year 2
  ;                                       !- Climate Zone Value 2

OS:Building,
  {252f413e-e5d6-417b-9bec-f156ffb1c034}, !- Handle
  Two story apartment,                    !- Name
  ,                                       !- Building Sector Type
  -45,                                    !- North Axis {deg}
  ,                                       !- Nominal Floor to Floor Height {m}
  ,                                       !- Space Type Name
  ,                                       !- Default Construction Set Name
  ;                                       !- Default Schedule Set Name

OS:Facility,
  {b2e046d7-bb87-403b-a985-38e8675e75b5}; !- Handle

OS:SimulationControl,
  {f6065d17-b98d-4951-8792-5931d62aed4a}; !- Handle

OS:Sizing:Parameters,
  {7a4223ad-21eb-4c09-b27d-7f107b24421c}, !- Handle
  1.25,                                   !- Heating Sizing Factor
  1.15;                                   !- Cooling Sizing Factor

OS:Timestep,
  {d24b8f97-e946-433b-87e1-3298da4dabfc}, !- Handle
  6;                                      !- Number of Timesteps per Hour

OS:ShadowCalculation,
  {cea14256-245e-495b-856a-221f5fec78a3}, !- Handle
  PolygonClipping,                        !- Shading Calculation Method
  ,                                       !- Shading Calculation Update Frequency Method
  20,                                     !- Shading Calculation Update Frequency
  15000,                                  !- Maximum Figures in Shadow Overlap Calculations
  ,                                       !- Polygon Clipping Algorithm
  512,                                    !- Pixel Counting Resolution
  ,                                       !- Sky Diffuse Modeling Algorithm
  No,                                     !- Output External Shading Calculation Results
  No,                                     !- Disable Self-Shading Within Shading Zone Groups
  No;                                     !- Disable Self-Shading From Shading Zone Groups to Other Zones

OS:HeatBalanceAlgorithm,
  {31596b78-ee50-48a7-aa52-debf01ba4d20}, !- Handle
  ConductionTransferFunction,             !- Algorithm
  200;                                    !- Surface Temperature Upper Limit {C}

OS:RunPeriod,
  {bafc5356-cb8f-4022-bd4b-546066abe28c}, !- Handle
  Run Period 1,                           !- Name
  1,                                      !- Begin Month
  1,                                      !- Begin Day of Month
  12,                                     !- End Month
  31,                                     !- End Day of Month
  ,                                       !- Use Weather File Holidays and Special Days
  ,                                       !- Use Weather File Daylight Saving Period
  ,                                       !- Apply Weekend Holiday Rule
  ,                                       !- Use Weather File Rain Indicators
  ,                                       !- Use Weather File Snow Indicators
  ;                                       !- Number of Times Runperiod to be Repeated

OS:LifeCycleCost:Parameters,
  {7ab1d78e-04df-4f09-ba3a-b028d718c61d}, !- Handle
  ,                                       !- Analysis Type
  ,                                       !- Discounting Convention
  ,                                       !- Inflation Approach
  ,                                       !- Real Discount Rate
  ,                                       !- Nominal Discount Rate
  ,                                       !- Inflation
  ,                                       !- Base Date Month
  ,                                       !- Base Date Year
  ,                                       !- Service Date Month
  ,                                       !- Service Date Year
  ;                                       !- Length of Study Period in Years

OS:SpaceType,
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Handle
  MidriseApartment Apartment,             !- Name
  ,                                       !- Default Construction Set Name
  {e22694ab-ed21-4639-9741-f1f56d05edbd}, !- Default Schedule Set Name
  {9a61c618-c11e-49ea-a150-95af53e0c33f}, !- Group Rendering Name
  {ab00cd4f-2d9e-4991-a223-6ccfddf607c0}, !- Design Specification Outdoor Air Object Name
  ,                                       !- Standards Template
  MidriseApartment,                       !- Standards Building Type
  Apartment;                              !- Standards Space Type

OS:DefaultScheduleSet,
  {e22694ab-ed21-4639-9741-f1f56d05edbd}, !- Handle
  MidriseApartment Apartment Schedule Set, !- Name
  ,                                       !- Hours of Operation Schedule Name
  {ffb6aeb5-8f0d-44ee-a5c7-b8896cfddaa6}, !- Number of People Schedule Name
  {16b09048-6d79-45de-83b9-c9dd2320f8fe}, !- People Activity Level Schedule Name
  {bdbc5a07-cd5a-49d4-be7d-2e9619770e0b}, !- Lighting Schedule Name
  {a1e8890d-9d79-4cef-81fd-4bd3751b99a4}, !- Electric Equipment Schedule Name
  ,                                       !- Gas Equipment Schedule Name
  ,                                       !- Hot Water Equipment Schedule Name
  {2e92a3d0-e377-4d0c-b596-eca160cd2580}, !- Infiltration Schedule Name
  ,                                       !- Steam Equipment Schedule Name
  ;                                       !- Other Equipment Schedule Name

OS:Rendering:Color,
  {9a61c618-c11e-49ea-a150-95af53e0c33f}, !- Handle
  MidriseApartment Apartment,             !- Name
  78,                                     !- Rendering Red Value
  167,                                    !- Rendering Green Value
  222,                                    !- Rendering Blue Value
  255;                                    !- Rendering Alpha Value

OS:DesignSpecification:OutdoorAir,
  {ab00cd4f-2d9e-4991-a223-6ccfddf607c0}, !- Handle
  MidriseApartment Apartment Ventilation, !- Name
  Sum,                                    !- Outdoor Air Method
  0.0169901079552,                        !- Outdoor Air Flow per Person {m3/s-person}
  ,                                       !- Outdoor Air Flow per Floor Area {m3/s-m2}
  ,                                       !- Outdoor Air Flow Rate {m3/s}
  ,                                       !- Outdoor Air Flow Air Changes per Hour {1/hr}
  ;                                       !- Outdoor Air Flow Rate Fraction Schedule Name

OS:Schedule:Ruleset,
  {ffb6aeb5-8f0d-44ee-a5c7-b8896cfddaa6}, !- Handle
  MidriseApartment Apartment Occ,         !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {4dc5af66-1d40-413c-b4b2-f0033e6b9913}, !- Default Day Schedule Name
  {3c2a8826-4e77-45f6-b994-f80b755d6825}, !- Summer Design Day Schedule Name
  {dd36fe8e-317f-4cd1-a79c-dea8a6032551}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {4dc5af66-1d40-413c-b4b2-f0033e6b9913}, !- Handle
  MidriseApartment Apartment Occ Default, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  7,                                      !- Hour 1
  0,                                      !- Minute 1
  1,                                      !- Value Until Time 1
  8,                                      !- Hour 2
  0,                                      !- Minute 2
  0.85,                                   !- Value Until Time 2
  9,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  16,                                     !- Hour 4
  0,                                      !- Minute 4
  0.25,                                   !- Value Until Time 4
  17,                                     !- Hour 5
  0,                                      !- Minute 5
  0.3,                                    !- Value Until Time 5
  18,                                     !- Hour 6
  0,                                      !- Minute 6
  0.52,                                   !- Value Until Time 6
  21,                                     !- Hour 7
  0,                                      !- Minute 7
  0.87,                                   !- Value Until Time 7
  24,                                     !- Hour 8
  0,                                      !- Minute 8
  1;                                      !- Value Until Time 8

OS:Schedule:Day,
  {3c2a8826-4e77-45f6-b994-f80b755d6825}, !- Handle
  MidriseApartment Apartment Occ Summer Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  7,                                      !- Hour 1
  0,                                      !- Minute 1
  1,                                      !- Value Until Time 1
  8,                                      !- Hour 2
  0,                                      !- Minute 2
  0.85,                                   !- Value Until Time 2
  9,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  16,                                     !- Hour 4
  0,                                      !- Minute 4
  0.25,                                   !- Value Until Time 4
  17,                                     !- Hour 5
  0,                                      !- Minute 5
  0.3,                                    !- Value Until Time 5
  18,                                     !- Hour 6
  0,                                      !- Minute 6
  0.52,                                   !- Value Until Time 6
  21,                                     !- Hour 7
  0,                                      !- Minute 7
  0.87,                                   !- Value Until Time 7
  24,                                     !- Hour 8
  0,                                      !- Minute 8
  1;                                      !- Value Until Time 8

OS:Schedule:Day,
  {dd36fe8e-317f-4cd1-a79c-dea8a6032551}, !- Handle
  MidriseApartment Apartment Occ Winter Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  7,                                      !- Hour 1
  0,                                      !- Minute 1
  1,                                      !- Value Until Time 1
  8,                                      !- Hour 2
  0,                                      !- Minute 2
  0.85,                                   !- Value Until Time 2
  9,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  16,                                     !- Hour 4
  0,                                      !- Minute 4
  0.25,                                   !- Value Until Time 4
  17,                                     !- Hour 5
  0,                                      !- Minute 5
  0.3,                                    !- Value Until Time 5
  18,                                     !- Hour 6
  0,                                      !- Minute 6
  0.52,                                   !- Value Until Time 6
  21,                                     !- Hour 7
  0,                                      !- Minute 7
  0.87,                                   !- Value Until Time 7
  24,                                     !- Hour 8
  0,                                      !- Minute 8
  1;                                      !- Value Until Time 8

OS:Schedule:Ruleset,
  {16b09048-6d79-45de-83b9-c9dd2320f8fe}, !- Handle
  MidriseApartment Activity,              !- Name
  {6e150b12-28e0-4959-b60a-c9dc1f5d44d3}, !- Schedule Type Limits Name
  {605c0733-fb09-4021-ba62-7d675bf43798}, !- Default Day Schedule Name
  {18eedcb9-fcf7-46c3-b458-a9d193c1ae44}, !- Summer Design Day Schedule Name
  {f50b72bf-5994-4f55-8771-2834b70f6b79}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {605c0733-fb09-4021-ba62-7d675bf43798}, !- Handle
  MidriseApartment Activity Default,      !- Name
  {6e150b12-28e0-4959-b60a-c9dc1f5d44d3}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  120;                                    !- Value Until Time 1

OS:Schedule:Day,
  {18eedcb9-fcf7-46c3-b458-a9d193c1ae44}, !- Handle
  MidriseApartment Activity Summer Design Day, !- Name
  {6e150b12-28e0-4959-b60a-c9dc1f5d44d3}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  120;                                    !- Value Until Time 1

OS:Schedule:Day,
  {f50b72bf-5994-4f55-8771-2834b70f6b79}, !- Handle
  MidriseApartment Activity Winter Design Day, !- Name
  {6e150b12-28e0-4959-b60a-c9dc1f5d44d3}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  120;                                    !- Value Until Time 1

OS:Schedule:Ruleset,
  {bdbc5a07-cd5a-49d4-be7d-2e9619770e0b}, !- Handle
  MidriseApartment Apartment Light,       !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {e40f1133-6a4e-4162-a7e4-cb1a7529e2e5}, !- Default Day Schedule Name
  {b0f2be0c-f69f-41ed-b4bf-f6aed649074a}, !- Summer Design Day Schedule Name
  {3d3f0bbf-9448-4a33-aec5-6997edac8ab0}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {e40f1133-6a4e-4162-a7e4-cb1a7529e2e5}, !- Handle
  MidriseApartment Apartment Light Default, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  4,                                      !- Hour 1
  0,                                      !- Minute 1
  0.067,                                  !- Value Until Time 1
  5,                                      !- Hour 2
  0,                                      !- Minute 2
  0.187,                                  !- Value Until Time 2
  6,                                      !- Hour 3
  0,                                      !- Minute 3
  0.394,                                  !- Value Until Time 3
  7,                                      !- Hour 4
  0,                                      !- Minute 4
  0.44,                                   !- Value Until Time 4
  8,                                      !- Hour 5
  0,                                      !- Minute 5
  0.393,                                  !- Value Until Time 5
  9,                                      !- Hour 6
  0,                                      !- Minute 6
  0.172,                                  !- Value Until Time 6
  15,                                     !- Hour 7
  0,                                      !- Minute 7
  0.119,                                  !- Value Until Time 7
  16,                                     !- Hour 8
  0,                                      !- Minute 8
  0.206,                                  !- Value Until Time 8
  17,                                     !- Hour 9
  0,                                      !- Minute 9
  0.439,                                  !- Value Until Time 9
  18,                                     !- Hour 10
  0,                                      !- Minute 10
  0.616,                                  !- Value Until Time 10
  19,                                     !- Hour 11
  0,                                      !- Minute 11
  0.829,                                  !- Value Until Time 11
  20,                                     !- Hour 12
  0,                                      !- Minute 12
  0.986,                                  !- Value Until Time 12
  21,                                     !- Hour 13
  0,                                      !- Minute 13
  1,                                      !- Value Until Time 13
  22,                                     !- Hour 14
  0,                                      !- Minute 14
  0.692,                                  !- Value Until Time 14
  23,                                     !- Hour 15
  0,                                      !- Minute 15
  0.384,                                  !- Value Until Time 15
  24,                                     !- Hour 16
  0,                                      !- Minute 16
  0.16;                                   !- Value Until Time 16

OS:Schedule:Day,
  {b0f2be0c-f69f-41ed-b4bf-f6aed649074a}, !- Handle
  MidriseApartment Apartment Light Summer Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  4,                                      !- Hour 1
  0,                                      !- Minute 1
  0.067,                                  !- Value Until Time 1
  5,                                      !- Hour 2
  0,                                      !- Minute 2
  0.187,                                  !- Value Until Time 2
  6,                                      !- Hour 3
  0,                                      !- Minute 3
  0.394,                                  !- Value Until Time 3
  7,                                      !- Hour 4
  0,                                      !- Minute 4
  0.44,                                   !- Value Until Time 4
  8,                                      !- Hour 5
  0,                                      !- Minute 5
  0.393,                                  !- Value Until Time 5
  9,                                      !- Hour 6
  0,                                      !- Minute 6
  0.172,                                  !- Value Until Time 6
  15,                                     !- Hour 7
  0,                                      !- Minute 7
  0.119,                                  !- Value Until Time 7
  16,                                     !- Hour 8
  0,                                      !- Minute 8
  0.206,                                  !- Value Until Time 8
  17,                                     !- Hour 9
  0,                                      !- Minute 9
  0.439,                                  !- Value Until Time 9
  18,                                     !- Hour 10
  0,                                      !- Minute 10
  0.616,                                  !- Value Until Time 10
  19,                                     !- Hour 11
  0,                                      !- Minute 11
  0.829,                                  !- Value Until Time 11
  20,                                     !- Hour 12
  0,                                      !- Minute 12
  0.986,                                  !- Value Until Time 12
  21,                                     !- Hour 13
  0,                                      !- Minute 13
  1,                                      !- Value Until Time 13
  22,                                     !- Hour 14
  0,                                      !- Minute 14
  0.692,                                  !- Value Until Time 14
  23,                                     !- Hour 15
  0,                                      !- Minute 15
  0.384,                                  !- Value Until Time 15
  24,                                     !- Hour 16
  0,                                      !- Minute 16
  0.16;                                   !- Value Until Time 16

OS:Schedule:Day,
  {3d3f0bbf-9448-4a33-aec5-6997edac8ab0}, !- Handle
  MidriseApartment Apartment Light Winter Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  4,                                      !- Hour 1
  0,                                      !- Minute 1
  0.067,                                  !- Value Until Time 1
  5,                                      !- Hour 2
  0,                                      !- Minute 2
  0.187,                                  !- Value Until Time 2
  6,                                      !- Hour 3
  0,                                      !- Minute 3
  0.394,                                  !- Value Until Time 3
  7,                                      !- Hour 4
  0,                                      !- Minute 4
  0.44,                                   !- Value Until Time 4
  8,                                      !- Hour 5
  0,                                      !- Minute 5
  0.393,                                  !- Value Until Time 5
  9,                                      !- Hour 6
  0,                                      !- Minute 6
  0.172,                                  !- Value Until Time 6
  15,                                     !- Hour 7
  0,                                      !- Minute 7
  0.119,                                  !- Value Until Time 7
  16,                                     !- Hour 8
  0,                                      !- Minute 8
  0.206,                                  !- Value Until Time 8
  17,                                     !- Hour 9
  0,                                      !- Minute 9
  0.439,                                  !- Value Until Time 9
  18,                                     !- Hour 10
  0,                                      !- Minute 10
  0.616,                                  !- Value Until Time 10
  19,                                     !- Hour 11
  0,                                      !- Minute 11
  0.829,                                  !- Value Until Time 11
  20,                                     !- Hour 12
  0,                                      !- Minute 12
  0.986,                                  !- Value Until Time 12
  21,                                     !- Hour 13
  0,                                      !- Minute 13
  1,                                      !- Value Until Time 13
  22,                                     !- Hour 14
  0,                                      !- Minute 14
  0.692,                                  !- Value Until Time 14
  23,                                     !- Hour 15
  0,                                      !- Minute 15
  0.384,                                  !- Value Until Time 15
  24,                                     !- Hour 16
  0,                                      !- Minute 16
  0.16;                                   !- Value Until Time 16

OS:Schedule:Ruleset,
  {a1e8890d-9d79-4cef-81fd-4bd3751b99a4}, !- Handle
  ApartmentMidRise EQP_APT_SCH,           !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {1fdfcd54-e81b-4554-94f8-5177f40fd648}, !- Default Day Schedule Name
  {f970d0ee-a000-4c0b-939d-3f0c53af1255}, !- Summer Design Day Schedule Name
  {9b5145a8-c83a-4565-8008-ef25eece16ab}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {1fdfcd54-e81b-4554-94f8-5177f40fd648}, !- Handle
  ApartmentMidRise EQP_APT_SCH Default,   !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  1,                                      !- Hour 1
  0,                                      !- Minute 1
  0.45,                                   !- Value Until Time 1
  2,                                      !- Hour 2
  0,                                      !- Minute 2
  0.41,                                   !- Value Until Time 2
  3,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  5,                                      !- Hour 4
  0,                                      !- Minute 4
  0.38,                                   !- Value Until Time 4
  6,                                      !- Hour 5
  0,                                      !- Minute 5
  0.43,                                   !- Value Until Time 5
  7,                                      !- Hour 6
  0,                                      !- Minute 6
  0.54,                                   !- Value Until Time 6
  8,                                      !- Hour 7
  0,                                      !- Minute 7
  0.65,                                   !- Value Until Time 7
  9,                                      !- Hour 8
  0,                                      !- Minute 8
  0.66,                                   !- Value Until Time 8
  10,                                     !- Hour 9
  0,                                      !- Minute 9
  0.67,                                   !- Value Until Time 9
  11,                                     !- Hour 10
  0,                                      !- Minute 10
  0.69,                                   !- Value Until Time 10
  12,                                     !- Hour 11
  0,                                      !- Minute 11
  0.7,                                    !- Value Until Time 11
  13,                                     !- Hour 12
  0,                                      !- Minute 12
  0.69,                                   !- Value Until Time 12
  14,                                     !- Hour 13
  0,                                      !- Minute 13
  0.66,                                   !- Value Until Time 13
  15,                                     !- Hour 14
  0,                                      !- Minute 14
  0.65,                                   !- Value Until Time 14
  16,                                     !- Hour 15
  0,                                      !- Minute 15
  0.68,                                   !- Value Until Time 15
  17,                                     !- Hour 16
  0,                                      !- Minute 16
  0.8,                                    !- Value Until Time 16
  19,                                     !- Hour 17
  0,                                      !- Minute 17
  1,                                      !- Value Until Time 17
  20,                                     !- Hour 18
  0,                                      !- Minute 18
  0.93,                                   !- Value Until Time 18
  21,                                     !- Hour 19
  0,                                      !- Minute 19
  0.89,                                   !- Value Until Time 19
  22,                                     !- Hour 20
  0,                                      !- Minute 20
  0.85,                                   !- Value Until Time 20
  23,                                     !- Hour 21
  0,                                      !- Minute 21
  0.71,                                   !- Value Until Time 21
  24,                                     !- Hour 22
  0,                                      !- Minute 22
  0.58;                                   !- Value Until Time 22

OS:Schedule:Day,
  {f970d0ee-a000-4c0b-939d-3f0c53af1255}, !- Handle
  ApartmentMidRise EQP_APT_SCH Summer Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  1,                                      !- Hour 1
  0,                                      !- Minute 1
  0.45,                                   !- Value Until Time 1
  2,                                      !- Hour 2
  0,                                      !- Minute 2
  0.41,                                   !- Value Until Time 2
  3,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  5,                                      !- Hour 4
  0,                                      !- Minute 4
  0.38,                                   !- Value Until Time 4
  6,                                      !- Hour 5
  0,                                      !- Minute 5
  0.43,                                   !- Value Until Time 5
  7,                                      !- Hour 6
  0,                                      !- Minute 6
  0.54,                                   !- Value Until Time 6
  8,                                      !- Hour 7
  0,                                      !- Minute 7
  0.65,                                   !- Value Until Time 7
  9,                                      !- Hour 8
  0,                                      !- Minute 8
  0.66,                                   !- Value Until Time 8
  10,                                     !- Hour 9
  0,                                      !- Minute 9
  0.67,                                   !- Value Until Time 9
  11,                                     !- Hour 10
  0,                                      !- Minute 10
  0.69,                                   !- Value Until Time 10
  12,                                     !- Hour 11
  0,                                      !- Minute 11
  0.7,                                    !- Value Until Time 11
  13,                                     !- Hour 12
  0,                                      !- Minute 12
  0.69,                                   !- Value Until Time 12
  14,                                     !- Hour 13
  0,                                      !- Minute 13
  0.66,                                   !- Value Until Time 13
  15,                                     !- Hour 14
  0,                                      !- Minute 14
  0.65,                                   !- Value Until Time 14
  16,                                     !- Hour 15
  0,                                      !- Minute 15
  0.68,                                   !- Value Until Time 15
  17,                                     !- Hour 16
  0,                                      !- Minute 16
  0.8,                                    !- Value Until Time 16
  19,                                     !- Hour 17
  0,                                      !- Minute 17
  1,                                      !- Value Until Time 17
  20,                                     !- Hour 18
  0,                                      !- Minute 18
  0.93,                                   !- Value Until Time 18
  21,                                     !- Hour 19
  0,                                      !- Minute 19
  0.89,                                   !- Value Until Time 19
  22,                                     !- Hour 20
  0,                                      !- Minute 20
  0.85,                                   !- Value Until Time 20
  23,                                     !- Hour 21
  0,                                      !- Minute 21
  0.71,                                   !- Value Until Time 21
  24,                                     !- Hour 22
  0,                                      !- Minute 22
  0.58;                                   !- Value Until Time 22

OS:Schedule:Day,
  {9b5145a8-c83a-4565-8008-ef25eece16ab}, !- Handle
  ApartmentMidRise EQP_APT_SCH Winter Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  1,                                      !- Hour 1
  0,                                      !- Minute 1
  0.45,                                   !- Value Until Time 1
  2,                                      !- Hour 2
  0,                                      !- Minute 2
  0.41,                                   !- Value Until Time 2
  3,                                      !- Hour 3
  0,                                      !- Minute 3
  0.39,                                   !- Value Until Time 3
  5,                                      !- Hour 4
  0,                                      !- Minute 4
  0.38,                                   !- Value Until Time 4
  6,                                      !- Hour 5
  0,                                      !- Minute 5
  0.43,                                   !- Value Until Time 5
  7,                                      !- Hour 6
  0,                                      !- Minute 6
  0.54,                                   !- Value Until Time 6
  8,                                      !- Hour 7
  0,                                      !- Minute 7
  0.65,                                   !- Value Until Time 7
  9,                                      !- Hour 8
  0,                                      !- Minute 8
  0.66,                                   !- Value Until Time 8
  10,                                     !- Hour 9
  0,                                      !- Minute 9
  0.67,                                   !- Value Until Time 9
  11,                                     !- Hour 10
  0,                                      !- Minute 10
  0.69,                                   !- Value Until Time 10
  12,                                     !- Hour 11
  0,                                      !- Minute 11
  0.7,                                    !- Value Until Time 11
  13,                                     !- Hour 12
  0,                                      !- Minute 12
  0.69,                                   !- Value Until Time 12
  14,                                     !- Hour 13
  0,                                      !- Minute 13
  0.66,                                   !- Value Until Time 13
  15,                                     !- Hour 14
  0,                                      !- Minute 14
  0.65,                                   !- Value Until Time 14
  16,                                     !- Hour 15
  0,                                      !- Minute 15
  0.68,                                   !- Value Until Time 15
  17,                                     !- Hour 16
  0,                                      !- Minute 16
  0.8,                                    !- Value Until Time 16
  19,                                     !- Hour 17
  0,                                      !- Minute 17
  1,                                      !- Value Until Time 17
  20,                                     !- Hour 18
  0,                                      !- Minute 18
  0.93,                                   !- Value Until Time 18
  21,                                     !- Hour 19
  0,                                      !- Minute 19
  0.89,                                   !- Value Until Time 19
  22,                                     !- Hour 20
  0,                                      !- Minute 20
  0.85,                                   !- Value Until Time 20
  23,                                     !- Hour 21
  0,                                      !- Minute 21
  0.71,                                   !- Value Until Time 21
  24,                                     !- Hour 22
  0,                                      !- Minute 22
  0.58;                                   !- Value Until Time 22

OS:Schedule:Ruleset,
  {2e92a3d0-e377-4d0c-b596-eca160cd2580}, !- Handle
  MidriseApartment Infil,                 !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {140b0ca1-2d1a-4e50-af79-691659565fe2}, !- Default Day Schedule Name
  {a5571d07-1a73-4e76-8ead-3719f66f85f3}, !- Summer Design Day Schedule Name
  {25384972-f111-484b-b40e-5d9805d52dfe}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {140b0ca1-2d1a-4e50-af79-691659565fe2}, !- Handle
  MidriseApartment Infil Default,         !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Day,
  {a5571d07-1a73-4e76-8ead-3719f66f85f3}, !- Handle
  MidriseApartment Infil Summer Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Day,
  {25384972-f111-484b-b40e-5d9805d52dfe}, !- Handle
  MidriseApartment Infil Winter Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:ScheduleTypeLimits,
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Handle
  Fractional,                             !- Name
  0,                                      !- Lower Limit Value
  1,                                      !- Upper Limit Value
  Continuous;                             !- Numeric Type

OS:ScheduleTypeLimits,
  {6e150b12-28e0-4959-b60a-c9dc1f5d44d3}, !- Handle
  ActivityLevel,                          !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  ActivityLevel;                          !- Unit Type

OS:People,
  {b52d6fc8-7229-4d8c-a27f-ba09c1e953cb}, !- Handle
  MidriseApartment Apartment People,      !- Name
  {62c04adf-1732-4727-8c7c-0b55c92b6938}, !- People Definition Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space or SpaceType Name
  ,                                       !- Number of People Schedule Name
  ,                                       !- Activity Level Schedule Name
  ,                                       !- Surface Name/Angle Factor List Name
  {c3e8d75f-bc49-4f93-934e-cabf6107a667}, !- Work Efficiency Schedule Name
  {945d4a35-1b53-4f23-a7c6-27456e73dc74}, !- Clothing Insulation Schedule Name
  {57e91d09-5041-4992-8833-2ba7079731b3}, !- Air Velocity Schedule Name
  1;                                      !- Multiplier

OS:People:Definition,
  {62c04adf-1732-4727-8c7c-0b55c92b6938}, !- Handle
  MidriseApartment Apartment People Definition, !- Name
  People/Area,                            !- Number of People Calculation Method
  ,                                       !- Number of People {people}
  0.0283090843959466,                     !- People per Space Floor Area {person/m2}
  ,                                       !- Space Floor Area per Person {m2/person}
  0.3;                                    !- Fraction Radiant

OS:Schedule:Ruleset,
  {c3e8d75f-bc49-4f93-934e-cabf6107a667}, !- Handle
  Work Efficiency Schedule,               !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {e7887bbd-bc39-4c03-a444-a689e121aa90}; !- Default Day Schedule Name

OS:Schedule:Day,
  {e7887bbd-bc39-4c03-a444-a689e121aa90}, !- Handle
  Work Efficiency Schedule Default,       !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  0;                                      !- Value Until Time 1

OS:Schedule:Ruleset,
  {945d4a35-1b53-4f23-a7c6-27456e73dc74}, !- Handle
  Clothing Schedule,                      !- Name
  {1b7a4154-a1c5-4eef-a5e4-be5504d1cf8f}, !- Schedule Type Limits Name
  {3dd778bf-60ad-4c3f-b65d-0594094c2f2c}; !- Default Day Schedule Name

OS:Schedule:Day,
  {3dd778bf-60ad-4c3f-b65d-0594094c2f2c}, !- Handle
  Clothing Schedule Default Winter Clothes, !- Name
  {1b7a4154-a1c5-4eef-a5e4-be5504d1cf8f}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Rule,
  {98bb6ba4-99ac-43d6-aad8-0c8b5891131b}, !- Handle
  Schedule Rule 1,                        !- Name
  {945d4a35-1b53-4f23-a7c6-27456e73dc74}, !- Schedule Ruleset Name
  0,                                      !- Rule Order
  {c0ddc7b3-7fa5-4c78-bc4f-f713e8065e03}, !- Day Schedule Name
  ,                                       !- Apply Sunday
  ,                                       !- Apply Monday
  ,                                       !- Apply Tuesday
  ,                                       !- Apply Wednesday
  ,                                       !- Apply Thursday
  ,                                       !- Apply Friday
  ,                                       !- Apply Saturday
  DateRange,                              !- Date Specification Type
  5,                                      !- Start Month
  1,                                      !- Start Day
  9,                                      !- End Month
  30;                                     !- End Day

OS:Schedule:Day,
  {c0ddc7b3-7fa5-4c78-bc4f-f713e8065e03}, !- Handle
  Clothing Schedule Summer Clothes,       !- Name
  {1b7a4154-a1c5-4eef-a5e4-be5504d1cf8f}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  0.5;                                    !- Value Until Time 1

OS:Schedule:Ruleset,
  {57e91d09-5041-4992-8833-2ba7079731b3}, !- Handle
  Air Velocity Schedule,                  !- Name
  {2d830640-553f-46ab-972b-063726c834ab}, !- Schedule Type Limits Name
  {0a2ac487-cac3-409e-806f-a80c3e9637d8}; !- Default Day Schedule Name

OS:Schedule:Day,
  {0a2ac487-cac3-409e-806f-a80c3e9637d8}, !- Handle
  Air Velocity Schedule Default,          !- Name
  {2d830640-553f-46ab-972b-063726c834ab}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  0.2;                                    !- Value Until Time 1

OS:ScheduleTypeLimits,
  {1b7a4154-a1c5-4eef-a5e4-be5504d1cf8f}, !- Handle
  ClothingInsulation,                     !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  ClothingInsulation;                     !- Unit Type

OS:ScheduleTypeLimits,
  {2d830640-553f-46ab-972b-063726c834ab}, !- Handle
  Velocity,                               !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Velocity;                               !- Unit Type

OS:Lights,
  {73c06d68-5323-4316-b629-d5465e512963}, !- Handle
  MidriseApartment Apartment Lights,      !- Name
  {4cffbc9d-075a-4301-b326-12b95d8b7771}, !- Lights Definition Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space or SpaceType Name
  ,                                       !- Schedule Name
  0,                                      !- Fraction Replaceable
  ,                                       !- Multiplier
  General;                                !- End-Use Subcategory

OS:Lights:Definition,
  {4cffbc9d-075a-4301-b326-12b95d8b7771}, !- Handle
  MidriseApartment Apartment Lights Definition, !- Name
  Watts/Area,                             !- Design Level Calculation Method
  ,                                       !- Lighting Level {W}
  3.8750077500155,                        !- Watts per Space Floor Area {W/m2}
  ,                                       !- Watts per Person {W/person}
  0,                                      !- Fraction Radiant
  0,                                      !- Fraction Visible
  0;                                      !- Return Air Fraction

OS:AdditionalProperties,
  {1f40fa9e-d61d-4eb4-8339-169f43469c83}, !- Handle
  {4cffbc9d-075a-4301-b326-12b95d8b7771}, !- Object Name
  lpd_fraction_linear_fluorescent,        !- Feature Name 1
  Double,                                 !- Feature Data Type 1
  1;                                      !- Feature Value 1

OS:ElectricEquipment,
  {3269cb6d-759d-4421-8fce-9544d22c95e9}, !- Handle
  MidriseApartment Apartment Elec Equip,  !- Name
  {0569a3b0-4abd-4213-b71a-c2710c1bb049}, !- Electric Equipment Definition Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space or SpaceType Name
  ,                                       !- Schedule Name
  ,                                       !- Multiplier
  General;                                !- End-Use Subcategory

OS:ElectricEquipment:Definition,
  {0569a3b0-4abd-4213-b71a-c2710c1bb049}, !- Handle
  MidriseApartment Apartment Elec Equip Definition, !- Name
  Watts/Area,                             !- Design Level Calculation Method
  ,                                       !- Design Level {W}
  5.38195520835486,                       !- Watts per Space Floor Area {W/m2}
  ,                                       !- Watts per Person {W/person}
  0,                                      !- Fraction Latent
  0.5,                                    !- Fraction Radiant
  0;                                      !- Fraction Lost

OS:SpaceInfiltration:DesignFlowRate,
  {22c0bb5b-32e4-4f32-9a21-b083d4d1721e}, !- Handle
  MidriseApartment Apartment Infiltration, !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space or SpaceType Name
  ,                                       !- Schedule Name
  Flow/ExteriorWallArea,                  !- Design Flow Rate Calculation Method
  ,                                       !- Design Flow Rate {m3/s}
  ,                                       !- Flow per Space Floor Area {m3/s-m2}
  0.00113284,                             !- Flow per Exterior Surface Area {m3/s-m2}
  ,                                       !- Air Changes per Hour {1/hr}
  ,                                       !- Constant Term Coefficient
  ,                                       !- Temperature Term Coefficient
  ,                                       !- Velocity Term Coefficient
  ;                                       !- Velocity Squared Term Coefficient

OS:SpaceType,
  {84b88777-4f33-4314-9a3c-f8317275bc9c}, !- Handle
  MidriseApartment Corridor,              !- Name
  ,                                       !- Default Construction Set Name
  {9da6a21f-a035-400b-8f4e-332a272cdd6a}, !- Default Schedule Set Name
  {eb212f8a-46e5-415b-b420-5f5155aec943}, !- Group Rendering Name
  {9db5066c-9901-467f-988f-e6744a6f7cf8}, !- Design Specification Outdoor Air Object Name
  ,                                       !- Standards Template
  MidriseApartment,                       !- Standards Building Type
  Corridor;                               !- Standards Space Type

OS:DefaultScheduleSet,
  {9da6a21f-a035-400b-8f4e-332a272cdd6a}, !- Handle
  MidriseApartment Corridor Schedule Set, !- Name
  ,                                       !- Hours of Operation Schedule Name
  ,                                       !- Number of People Schedule Name
  ,                                       !- People Activity Level Schedule Name
  {2a8a37f9-61aa-4dbb-9e38-66ca1cf068e9}, !- Lighting Schedule Name
  {3cea787e-6432-4042-b724-a7bd88b2f2ee}, !- Electric Equipment Schedule Name
  ,                                       !- Gas Equipment Schedule Name
  ,                                       !- Hot Water Equipment Schedule Name
  {2e92a3d0-e377-4d0c-b596-eca160cd2580}, !- Infiltration Schedule Name
  ,                                       !- Steam Equipment Schedule Name
  ;                                       !- Other Equipment Schedule Name

OS:Rendering:Color,
  {eb212f8a-46e5-415b-b420-5f5155aec943}, !- Handle
  MidriseApartment Corridor,              !- Name
  169,                                    !- Rendering Red Value
  31,                                     !- Rendering Green Value
  31,                                     !- Rendering Blue Value
  255;                                    !- Rendering Alpha Value

OS:DesignSpecification:OutdoorAir,
  {9db5066c-9901-467f-988f-e6744a6f7cf8}, !- Handle
  MidriseApartment Corridor Ventilation,  !- Name
  ,                                       !- Outdoor Air Method
  0,                                      !- Outdoor Air Flow per Person {m3/s-person}
  0,                                      !- Outdoor Air Flow per Floor Area {m3/s-m2}
  ,                                       !- Outdoor Air Flow Rate {m3/s}
  0,                                      !- Outdoor Air Flow Air Changes per Hour {1/hr}
  ;                                       !- Outdoor Air Flow Rate Fraction Schedule Name

OS:Schedule:Ruleset,
  {2a8a37f9-61aa-4dbb-9e38-66ca1cf068e9}, !- Handle
  MidriseApartment Corridor Light,        !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {0605574a-b827-465d-b0c8-4f604e9b688c}, !- Default Day Schedule Name
  {94a1bae2-aeec-414c-8b68-3b2734d1a5be}, !- Summer Design Day Schedule Name
  {12b2e9c9-f81a-4e76-a435-12e9199b0b56}; !- Winter Design Day Schedule Name

OS:Schedule:Day,
  {0605574a-b827-465d-b0c8-4f604e9b688c}, !- Handle
  MidriseApartment Corridor Light Default, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Day,
  {94a1bae2-aeec-414c-8b68-3b2734d1a5be}, !- Handle
  MidriseApartment Corridor Light Summer Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Day,
  {12b2e9c9-f81a-4e76-a435-12e9199b0b56}, !- Handle
  MidriseApartment Corridor Light Winter Design Day, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  1;                                      !- Value Until Time 1

OS:Schedule:Ruleset,
  {3cea787e-6432-4042-b724-a7bd88b2f2ee}, !- Handle
  ApartmentMidRise BLDG_ELEVATORS Pre2004, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  {e75f3015-8a36-4bde-8076-94154654ce05}; !- Default Day Schedule Name

OS:Schedule:Day,
  {e75f3015-8a36-4bde-8076-94154654ce05}, !- Handle
  ApartmentMidRise BLDG_ELEVATORS Pre2004 Default, !- Name
  {26174a88-7f46-4bdf-be71-b140b42591b1}, !- Schedule Type Limits Name
  No,                                     !- Interpolate to Timestep
  4,                                      !- Hour 1
  0,                                      !- Minute 1
  0.05,                                   !- Value Until Time 1
  5,                                      !- Hour 2
  0,                                      !- Minute 2
  0.1,                                    !- Value Until Time 2
  6,                                      !- Hour 3
  0,                                      !- Minute 3
  0.2,                                    !- Value Until Time 3
  7,                                      !- Hour 4
  0,                                      !- Minute 4
  0.4,                                    !- Value Until Time 4
  9,                                      !- Hour 5
  0,                                      !- Minute 5
  0.5,                                    !- Value Until Time 5
  10,                                     !- Hour 6
  0,                                      !- Minute 6
  0.35,                                   !- Value Until Time 6
  16,                                     !- Hour 7
  0,                                      !- Minute 7
  0.15,                                   !- Value Until Time 7
  17,                                     !- Hour 8
  0,                                      !- Minute 8
  0.35,                                   !- Value Until Time 8
  19,                                     !- Hour 9
  0,                                      !- Minute 9
  0.5,                                    !- Value Until Time 9
  21,                                     !- Hour 10
  0,                                      !- Minute 10
  0.4,                                    !- Value Until Time 10
  22,                                     !- Hour 11
  0,                                      !- Minute 11
  0.3,                                    !- Value Until Time 11
  23,                                     !- Hour 12
  0,                                      !- Minute 12
  0.2,                                    !- Value Until Time 12
  24,                                     !- Hour 13
  0,                                      !- Minute 13
  0.1;                                    !- Value Until Time 13

OS:Lights,
  {b091adba-1433-46f0-8e8f-820bcbb5dc50}, !- Handle
  MidriseApartment Corridor Lights,       !- Name
  {b8531fd6-ace6-4042-b2f7-7d8e42dfb0f1}, !- Lights Definition Name
  {84b88777-4f33-4314-9a3c-f8317275bc9c}, !- Space or SpaceType Name
  ,                                       !- Schedule Name
  0,                                      !- Fraction Replaceable
  ,                                       !- Multiplier
  General;                                !- End-Use Subcategory

OS:Lights:Definition,
  {b8531fd6-ace6-4042-b2f7-7d8e42dfb0f1}, !- Handle
  MidriseApartment Corridor Lights Definition, !- Name
  Watts/Area,                             !- Design Level Calculation Method
  ,                                       !- Lighting Level {W}
  9.90279758337294,                       !- Watts per Space Floor Area {W/m2}
  ,                                       !- Watts per Person {W/person}
  0,                                      !- Fraction Radiant
  0,                                      !- Fraction Visible
  0;                                      !- Return Air Fraction

OS:AdditionalProperties,
  {eb2cd5a8-83a7-414a-9823-4225552d0f94}, !- Handle
  {b8531fd6-ace6-4042-b2f7-7d8e42dfb0f1}, !- Object Name
  lpd_fraction_linear_fluorescent,        !- Feature Name 1
  Double,                                 !- Feature Data Type 1
  1;                                      !- Feature Value 1

OS:SpaceInfiltration:DesignFlowRate,
  {9adf01b7-4631-4427-836f-84df2b4d8d83}, !- Handle
  MidriseApartment Corridor Infiltration, !- Name
  {84b88777-4f33-4314-9a3c-f8317275bc9c}, !- Space or SpaceType Name
  ,                                       !- Schedule Name
  Flow/ExteriorWallArea,                  !- Design Flow Rate Calculation Method
  ,                                       !- Design Flow Rate {m3/s}
  ,                                       !- Flow per Space Floor Area {m3/s-m2}
  0.00113284,                             !- Flow per Exterior Surface Area {m3/s-m2}
  ,                                       !- Air Changes per Hour {1/hr}
  ,                                       !- Constant Term Coefficient
  ,                                       !- Temperature Term Coefficient
  ,                                       !- Velocity Term Coefficient
  ;                                       !- Velocity Squared Term Coefficient

OS:DefaultConstructionSet,
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Handle
  DOE Ref 1980-2004 - MidApt - ASHRAE 169-2013-4A, !- Name
  {7c289d1d-48d0-4aa1-b5e1-a73ee486a7b5}, !- Default Exterior Surface Constructions Name
  {4870b931-c0fd-4b4a-87ac-41d269caceb4}, !- Default Interior Surface Constructions Name
  {5cd7ef3e-446d-4238-b26d-5f08472b1380}, !- Default Ground Contact Surface Constructions Name
  {8ca4279e-6717-4222-83d4-61fa9f9c4bd3}, !- Default Exterior SubSurface Constructions Name
  {1cf8d415-8608-4d4f-824b-707c401575de}, !- Default Interior SubSurface Constructions Name
  {68085711-2d85-49be-8dd2-f11b7a4863db}, !- Interior Partition Construction Name
  ,                                       !- Space Shading Construction Name
  ,                                       !- Building Shading Construction Name
  ,                                       !- Site Shading Construction Name
  ;                                       !- Adiabatic Surface Construction Name

OS:DefaultSurfaceConstructions,
  {7c289d1d-48d0-4aa1-b5e1-a73ee486a7b5}, !- Handle
  Default Surface Constructions 763,      !- Name
  {21e2dc63-16d6-4fc7-aab2-fc41f62862b9}, !- Floor Construction Name
  {f31be465-f21a-4570-8999-789bc2aba41e}, !- Wall Construction Name
  {04a91f8a-0f8d-425e-8f06-9436a0d24686}; !- Roof Ceiling Construction Name

OS:DefaultSurfaceConstructions,
  {4870b931-c0fd-4b4a-87ac-41d269caceb4}, !- Handle
  Default Surface Constructions 764,      !- Name
  {6e8d1cd6-5ad2-4550-8cbd-3467e92b0fcb}, !- Floor Construction Name
  {a4ce4fc2-a31e-4aad-9cec-8685ef593107}, !- Wall Construction Name
  {143a4724-2c5b-4f3c-8379-18a36ca31ca3}; !- Roof Ceiling Construction Name

OS:DefaultSurfaceConstructions,
  {5cd7ef3e-446d-4238-b26d-5f08472b1380}, !- Handle
  Default Surface Constructions 765,      !- Name
  {a7f5d1bb-bfa4-4f08-a65b-7db04868050e}, !- Floor Construction Name
  {5cb1700b-a755-4037-af78-4b60ef2021fd}, !- Wall Construction Name
  ;                                       !- Roof Ceiling Construction Name

OS:DefaultSubSurfaceConstructions,
  {8ca4279e-6717-4222-83d4-61fa9f9c4bd3}, !- Handle
  Default Sub Surface Constructions 509,  !- Name
  {6c9fd806-89aa-41a5-b477-f0d3adeeedd7}, !- Fixed Window Construction Name
  {f068b5ea-4cf7-4b16-9770-f196d1a8ae95}, !- Operable Window Construction Name
  {fa4e0411-0324-42c4-ba37-d17411a64268}, !- Door Construction Name
  {d60006e6-76b3-4130-a5d3-6ebfb9274bb6}, !- Glass Door Construction Name
  {7dc348df-8c47-4f01-9f54-4e999fc797a9}, !- Overhead Door Construction Name
  ,                                       !- Skylight Construction Name
  {e95319db-208c-4c01-afb8-5b1aa8973853}, !- Tubular Daylight Dome Construction Name
  {e95319db-208c-4c01-afb8-5b1aa8973853}; !- Tubular Daylight Diffuser Construction Name

OS:DefaultSubSurfaceConstructions,
  {1cf8d415-8608-4d4f-824b-707c401575de}, !- Handle
  Default Sub Surface Constructions 510,  !- Name
  {e95319db-208c-4c01-afb8-5b1aa8973853}, !- Fixed Window Construction Name
  {e95319db-208c-4c01-afb8-5b1aa8973853}, !- Operable Window Construction Name
  {65dbda2b-3f49-4819-81d6-f5073f2162dc}, !- Door Construction Name
  ,                                       !- Glass Door Construction Name
  ,                                       !- Overhead Door Construction Name
  ,                                       !- Skylight Construction Name
  ,                                       !- Tubular Daylight Dome Construction Name
  ;                                       !- Tubular Daylight Diffuser Construction Name

OS:Construction,
  {68085711-2d85-49be-8dd2-f11b7a4863db}, !- Handle
  Typical Interior Partition,             !- Name
  {c68c98aa-6352-4ca0-8d1a-cd8e2206870f}, !- Surface Rendering Name
  {775b7dea-d814-424d-847d-a2d1d90ddb2f}; !- Layer 1

OS:StandardsInformation:Construction,
  {059b6f37-b4c6-43bc-8866-d705f34d489f}, !- Handle
  {68085711-2d85-49be-8dd2-f11b7a4863db}, !- Construction Name
  InteriorPartition,                      !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {21e2dc63-16d6-4fc7-aab2-fc41f62862b9}, !- Handle
  Typical Insulated Exterior Mass Floor,  !- Name
  {5d11ea0b-3de5-4744-941d-427345d347c0}, !- Surface Rendering Name
  {cd82a79f-c189-471d-8aa8-a965237f0394}, !- Layer 1
  {836f86af-2aac-4eb0-9f43-8387617cdd0e}, !- Layer 2
  {7a38806a-684b-41a5-8a91-005964139ab8}; !- Layer 3

OS:StandardsInformation:Construction,
  {208f0c6a-ed75-487b-b78f-d2c89397dbf4}, !- Handle
  {21e2dc63-16d6-4fc7-aab2-fc41f62862b9}, !- Construction Name
  ExteriorFloor,                          !- Intended Surface Type
  Mass;                                   !- Standards Construction Type

OS:Construction,
  {f31be465-f21a-4570-8999-789bc2aba41e}, !- Handle
  Typical Insulated Steel Framed Exterior Wall R-11.24 4, !- Name
  {67e4ebeb-7e1f-49bf-bc9e-f9728adfee57}, !- Surface Rendering Name
  {b3c76bbd-7496-4933-a45f-80c633a7fc93}, !- Layer 1
  {783c0ae5-563b-418b-92a1-fdb92438bc2a}, !- Layer 2
  {29479a6f-f8cd-4246-ba7c-816efc56f417}, !- Layer 3
  {783c0ae5-563b-418b-92a1-fdb92438bc2a}; !- Layer 4

OS:StandardsInformation:Construction,
  {3ebedd9c-e9b3-4f90-a67f-9cc0eb33509c}, !- Handle
  {f31be465-f21a-4570-8999-789bc2aba41e}, !- Construction Name
  ExteriorWall,                           !- Intended Surface Type
  SteelFramed;                            !- Standards Construction Type

OS:Construction,
  {04a91f8a-0f8d-425e-8f06-9436a0d24686}, !- Handle
  Typical IEAD Roof R-17.24 10,           !- Name
  {191080e5-06ad-4d89-91cc-06bdd8234a40}, !- Surface Rendering Name
  {4339fa28-b93e-4651-a17f-b27d04bc2078}, !- Layer 1
  {b15b5610-af05-4443-a22f-b02165dea8ff}, !- Layer 2
  {1ae34c2c-e9a1-44d7-afb1-1d675abb3c4a}; !- Layer 3

OS:StandardsInformation:Construction,
  {a02bc4f1-e535-4bd5-a550-ba2c3feba7fb}, !- Handle
  {04a91f8a-0f8d-425e-8f06-9436a0d24686}, !- Construction Name
  ExteriorRoof,                           !- Intended Surface Type
  IEAD;                                   !- Standards Construction Type

OS:Construction,
  {6e8d1cd6-5ad2-4550-8cbd-3467e92b0fcb}, !- Handle
  Typical Interior Floor,                 !- Name
  {ba56349a-d261-4c77-9a3f-dd204a808c40}, !- Surface Rendering Name
  {26449061-fa31-4556-957f-ed8cec4c5891}, !- Layer 1
  {b011e73d-eae9-4fb8-9847-e3313013becf}; !- Layer 2

OS:StandardsInformation:Construction,
  {6458b139-7739-49d5-a03c-12c2176ee4e1}, !- Handle
  {6e8d1cd6-5ad2-4550-8cbd-3467e92b0fcb}, !- Construction Name
  InteriorFloor,                          !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {a4ce4fc2-a31e-4aad-9cec-8685ef593107}, !- Handle
  Typical Interior Wall,                  !- Name
  {81e6c5b7-055c-4d59-9800-53cddbfe3176}, !- Surface Rendering Name
  {9e43b4c8-a40f-45f8-be58-a78a12b21864}, !- Layer 1
  {9e43b4c8-a40f-45f8-be58-a78a12b21864}; !- Layer 2

OS:StandardsInformation:Construction,
  {381b1170-fdef-43a8-8230-91a9fe4a80f9}, !- Handle
  {a4ce4fc2-a31e-4aad-9cec-8685ef593107}, !- Construction Name
  InteriorWall,                           !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {143a4724-2c5b-4f3c-8379-18a36ca31ca3}, !- Handle
  Typical Interior Ceiling,               !- Name
  {1dc606f4-f3b9-46d2-b242-38b6c577773c}, !- Surface Rendering Name
  {b011e73d-eae9-4fb8-9847-e3313013becf}, !- Layer 1
  {26449061-fa31-4556-957f-ed8cec4c5891}; !- Layer 2

OS:StandardsInformation:Construction,
  {487ee4bb-1faa-488a-8158-f81be5ac6da4}, !- Handle
  {143a4724-2c5b-4f3c-8379-18a36ca31ca3}, !- Construction Name
  InteriorCeiling,                        !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {a7f5d1bb-bfa4-4f08-a65b-7db04868050e}, !- Handle
  Typical Insulated Carpeted 6in Slab Floor, !- Name
  {b3c96535-b45b-42dc-a35c-f5a44d4514b6}, !- Surface Rendering Name
  {d0727782-365b-4b94-8427-23e43af7633a}, !- Layer 1
  {7a38806a-684b-41a5-8a91-005964139ab8}; !- Layer 2

OS:StandardsInformation:Construction,
  {229ed468-a300-494d-9536-1034a7adfa77}, !- Handle
  {a7f5d1bb-bfa4-4f08-a65b-7db04868050e}, !- Construction Name
  GroundContactFloor,                     !- Intended Surface Type
  Mass;                                   !- Standards Construction Type

OS:Construction,
  {5cb1700b-a755-4037-af78-4b60ef2021fd}, !- Handle
  Typical Insulated Basement Mass Wall,   !- Name
  {3f543f93-c83f-4869-90bb-1fa2fd16b293}, !- Surface Rendering Name
  {e911e737-0c12-4a5a-b6d0-e370e4217e79}; !- Layer 1

OS:StandardsInformation:Construction,
  {25875da7-a219-49ac-897c-928121759e5c}, !- Handle
  {5cb1700b-a755-4037-af78-4b60ef2021fd}, !- Construction Name
  GroundContactWall,                      !- Intended Surface Type
  Mass;                                   !- Standards Construction Type

OS:Construction,
  {6c9fd806-89aa-41a5-b477-f0d3adeeedd7}, !- Handle
  U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 22, !- Name
  {73ad3a7d-ba13-41b6-82f7-c76a96cfc760}, !- Surface Rendering Name
  {5c69d8b7-63a6-48f1-aa9f-a30396605ce8}; !- Layer 1

OS:StandardsInformation:Construction,
  {ead8a1c9-5b94-495f-8513-14a6cbfc927b}, !- Handle
  {6c9fd806-89aa-41a5-b477-f0d3adeeedd7}, !- Construction Name
  ExteriorWindow,                         !- Intended Surface Type
  Metal framing (all other),              !- Standards Construction Type
  ,                                       !- Perturbable Layer
  ,                                       !- Perturbable Layer Type
  ,                                       !- Other Perturbable Layer Type
  ,                                       !- Construction Standard
  ,                                       !- Construction Standard Source
  ,                                       !- Fenestration Type
  ,                                       !- Fenestration Assembly Context
  ,                                       !- Fenestration Number of Panes
  Metal Framing;                          !- Fenestration Frame Type

OS:Construction,
  {f068b5ea-4cf7-4b16-9770-f196d1a8ae95}, !- Handle
  U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 23, !- Name
  {0df59329-627c-4329-9e87-aa6e44644b9e}, !- Surface Rendering Name
  {f039016b-2a09-4504-ba38-1fc15ae6dfd6}; !- Layer 1

OS:StandardsInformation:Construction,
  {0e663e34-3cba-4bc2-a0d9-aad70c99af44}, !- Handle
  {f068b5ea-4cf7-4b16-9770-f196d1a8ae95}, !- Construction Name
  ExteriorWindow,                         !- Intended Surface Type
  Metal framing (all other),              !- Standards Construction Type
  ,                                       !- Perturbable Layer
  ,                                       !- Perturbable Layer Type
  ,                                       !- Other Perturbable Layer Type
  ,                                       !- Construction Standard
  ,                                       !- Construction Standard Source
  ,                                       !- Fenestration Type
  ,                                       !- Fenestration Assembly Context
  ,                                       !- Fenestration Number of Panes
  Metal Framing;                          !- Fenestration Frame Type

OS:Construction,
  {fa4e0411-0324-42c4-ba37-d17411a64268}, !- Handle
  Typical Insulated Metal Door,           !- Name
  {95aa99e4-2ff3-42ad-a2d8-4155823ec314}, !- Surface Rendering Name
  {927d8fd9-6ea0-49b9-858d-1de05e12adfc}, !- Layer 1
  {17cea2e1-7e38-4e45-b384-4cef33e00e74}; !- Layer 2

OS:StandardsInformation:Construction,
  {5910d954-4183-4f22-bba9-d487d3639c29}, !- Handle
  {fa4e0411-0324-42c4-ba37-d17411a64268}, !- Construction Name
  ExteriorDoor,                           !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {d60006e6-76b3-4130-a5d3-6ebfb9274bb6}, !- Handle
  U 0.88 SHGC 0.16 Sgl Ref-A-L Clr 6mm,   !- Name
  {a6aafd8f-e120-4787-aa9b-6f9cbd9a7923}, !- Surface Rendering Name
  {1e77c02f-bd7a-4e51-b063-ea2a41c8b723}; !- Layer 1

OS:StandardsInformation:Construction,
  {b6c3f242-2fea-465d-a6bb-7960004c155b}, !- Handle
  {d60006e6-76b3-4130-a5d3-6ebfb9274bb6}, !- Construction Name
  ExteriorWindow,                         !- Intended Surface Type
  Metal framing (all other),              !- Standards Construction Type
  ,                                       !- Perturbable Layer
  ,                                       !- Perturbable Layer Type
  ,                                       !- Other Perturbable Layer Type
  ,                                       !- Construction Standard
  ,                                       !- Construction Standard Source
  ,                                       !- Fenestration Type
  ,                                       !- Fenestration Assembly Context
  ,                                       !- Fenestration Number of Panes
  Metal Framing;                          !- Fenestration Frame Type

OS:Construction,
  {7dc348df-8c47-4f01-9f54-4e999fc797a9}, !- Handle
  Typical Overhead Door,                  !- Name
  {53b41d99-4bdf-4e5b-88a7-0ce391391e6f}, !- Surface Rendering Name
  {17cea2e1-7e38-4e45-b384-4cef33e00e74}; !- Layer 1

OS:StandardsInformation:Construction,
  {ec2791df-4c88-48c1-aa9f-bf3b5d04b2e9}, !- Handle
  {7dc348df-8c47-4f01-9f54-4e999fc797a9}, !- Construction Name
  ExteriorDoor,                           !- Intended Surface Type
  RollUp;                                 !- Standards Construction Type

OS:Construction,
  {e95319db-208c-4c01-afb8-5b1aa8973853}, !- Handle
  Typical Interior Window,                !- Name
  {40e624cb-988a-4bb0-aefa-65201cda5b39}, !- Surface Rendering Name
  {b90abe2c-d37c-4f68-838e-8e87d811e57a}; !- Layer 1

OS:StandardsInformation:Construction,
  {fc8fac2d-6213-45d7-95d9-0174a30a3aef}, !- Handle
  {e95319db-208c-4c01-afb8-5b1aa8973853}, !- Construction Name
  InteriorWindow,                         !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Construction,
  {65dbda2b-3f49-4819-81d6-f5073f2162dc}, !- Handle
  Typical Interior Door,                  !- Name
  {0a6b46d3-5357-4dff-b102-07c307502959}, !- Surface Rendering Name
  {775b7dea-d814-424d-847d-a2d1d90ddb2f}; !- Layer 1

OS:StandardsInformation:Construction,
  {0e2932ff-7369-4222-8599-cfe2942966a1}, !- Handle
  {65dbda2b-3f49-4819-81d6-f5073f2162dc}, !- Construction Name
  InteriorDoor,                           !- Intended Surface Type
  ;                                       !- Standards Construction Type

OS:Material,
  {775b7dea-d814-424d-847d-a2d1d90ddb2f}, !- Handle
  G05 25mm wood,                          !- Name
  MediumSmooth,                           !- Roughness
  0.0254,                                 !- Thickness {m}
  0.15,                                   !- Conductivity {W/m-K}
  608,                                    !- Density {kg/m3}
  1630,                                   !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.5,                                    !- Solar Absorptance
  0.5;                                    !- Visible Absorptance

OS:StandardsInformation:Material,
  {924b8fd8-cf4a-46cd-bd2d-0d9f41207adc}, !- Handle
  {775b7dea-d814-424d-847d-a2d1d90ddb2f}; !- Material Name

OS:Material:NoMass,
  {cd82a79f-c189-471d-8aa8-a965237f0394}, !- Handle
  Typical Insulation R-12.4,              !- Name
  Smooth,                                 !- Roughness
  2.18310873594147,                       !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {836f86af-2aac-4eb0-9f43-8387617cdd0e}, !- Handle
  4 in. Normalweight Concrete Floor,      !- Name
  MediumRough,                            !- Roughness
  0.1016,                                 !- Thickness {m}
  2.31,                                   !- Conductivity {W/m-K}
  2321.99999999999,                       !- Density {kg/m3}
  831.999999999997,                       !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material:NoMass,
  {7a38806a-684b-41a5-8a91-005964139ab8}, !- Handle
  Typical Carpet Pad,                     !- Name
  Smooth,                                 !- Roughness
  0.216479986995276,                      !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.8;                                    !- Visible Absorptance

OS:Material,
  {b3c76bbd-7496-4933-a45f-80c633a7fc93}, !- Handle
  25mm Stucco,                            !- Name
  Smooth,                                 !- Roughness
  0.0254,                                 !- Thickness {m}
  0.719999999999999,                      !- Conductivity {W/m-K}
  1855.99999999999,                       !- Density {kg/m3}
  839.999999999997,                       !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {783c0ae5-563b-418b-92a1-fdb92438bc2a}, !- Handle
  5/8 in. Gypsum Board,                   !- Name
  MediumSmooth,                           !- Roughness
  0.0159,                                 !- Thickness {m}
  0.159999999999999,                      !- Conductivity {W/m-K}
  799.999999999999,                       !- Density {kg/m3}
  1090,                                   !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material:NoMass,
  {29479a6f-f8cd-4246-ba7c-816efc56f417}, !- Handle
  Typical Insulation R-9.06 4,            !- Name
  Smooth,                                 !- Roughness
  1.59504467488221,                       !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {4339fa28-b93e-4651-a17f-b27d04bc2078}, !- Handle
  Roof Membrane,                          !- Name
  VeryRough,                              !- Roughness
  0.0095,                                 !- Thickness {m}
  0.16,                                   !- Conductivity {W/m-K}
  1121.29,                                !- Density {kg/m3}
  1460,                                   !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:StandardsInformation:Material,
  {ad942a3f-a87c-4675-acdb-1919e9675894}, !- Handle
  {4339fa28-b93e-4651-a17f-b27d04bc2078}; !- Material Name

OS:Material:NoMass,
  {b15b5610-af05-4443-a22f-b02165dea8ff}, !- Handle
  Typical Insulation R-16.12 10,          !- Name
  Smooth,                                 !- Roughness
  2.83962386616441,                       !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {1ae34c2c-e9a1-44d7-afb1-1d675abb3c4a}, !- Handle
  Metal Roof Surface,                     !- Name
  Smooth,                                 !- Roughness
  0.000799999999999998,                   !- Thickness {m}
  45.2799999999999,                       !- Conductivity {W/m-K}
  7823.99999999999,                       !- Density {kg/m3}
  499.999999999996,                       !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {26449061-fa31-4556-957f-ed8cec4c5891}, !- Handle
  100mm Normalweight concrete floor,      !- Name
  MediumRough,                            !- Roughness
  0.1016,                                 !- Thickness {m}
  2.31044676686054,                       !- Conductivity {W/m-K}
  2322.00146636525,                       !- Density {kg/m3}
  832.5567858096,                         !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material:NoMass,
  {b011e73d-eae9-4fb8-9847-e3313013becf}, !- Handle
  CP02 CARPET PAD 1,                      !- Name
  Smooth,                                 !- Roughness
  0.216479986995276,                      !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.8;                                    !- Visible Absorptance

OS:Material,
  {9e43b4c8-a40f-45f8-be58-a78a12b21864}, !- Handle
  G01 13mm gypsum board,                  !- Name
  Smooth,                                 !- Roughness
  0.0127,                                 !- Thickness {m}
  0.160030944416258,                      !- Conductivity {W/m-K}
  800.000505207667,                       !- Density {kg/m3}
  1090.7294438736,                        !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.5;                                    !- Visible Absorptance

OS:Material,
  {d0727782-365b-4b94-8427-23e43af7633a}, !- Handle
  6 in. Normalweight Concrete Floor,      !- Name
  MediumRough,                            !- Roughness
  0.1524,                                 !- Thickness {m}
  2.31,                                   !- Conductivity {W/m-K}
  2321.99999999999,                       !- Density {kg/m3}
  831.999999999997,                       !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:Material,
  {e911e737-0c12-4a5a-b6d0-e370e4217e79}, !- Handle
  8 in. Concrete Block Basement Wall,     !- Name
  MediumRough,                            !- Roughness
  0.2032,                                 !- Thickness {m}
  1.326,                                  !- Conductivity {W/m-K}
  1841.99999999999,                       !- Density {kg/m3}
  911.999999999999,                       !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:WindowMaterial:SimpleGlazingSystem,
  {5c69d8b7-63a6-48f1-aa9f-a30396605ce8}, !- Handle
  U 0.59 SHGC 0.36 Simple Glazing U-0.59 SHGC 0.36 22, !- Name
  3.35017537125696,                       !- U-Factor {W/m2-K}
  0.36,                                   !- Solar Heat Gain Coefficient
  0.27;                                   !- Visible Transmittance

OS:WindowMaterial:SimpleGlazingSystem,
  {f039016b-2a09-4504-ba38-1fc15ae6dfd6}, !- Handle
  U 0.59 SHGC 0.36 Simple Glazing U-0.59 SHGC 0.36 23, !- Name
  3.35017537125696,                       !- U-Factor {W/m2-K}
  0.36,                                   !- Solar Heat Gain Coefficient
  0.27;                                   !- Visible Transmittance

OS:Material,
  {927d8fd9-6ea0-49b9-858d-1de05e12adfc}, !- Handle
  F08 Metal surface,                      !- Name
  Smooth,                                 !- Roughness
  0.0008,                                 !- Thickness {m}
  45.2800000000001,                       !- Conductivity {W/m-K}
  7823.99999999999,                       !- Density {kg/m3}
  500,                                    !- Specific Heat {J/kg-K}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:StandardsInformation:Material,
  {540be983-9afc-4c05-a038-46e2f016b1d7}, !- Handle
  {927d8fd9-6ea0-49b9-858d-1de05e12adfc}; !- Material Name

OS:Material:NoMass,
  {17cea2e1-7e38-4e45-b384-4cef33e00e74}, !- Handle
  Typical Insulation R-12.4 1,            !- Name
  Smooth,                                 !- Roughness
  2.18310873594147,                       !- Thermal Resistance {m2-K/W}
  0.9,                                    !- Thermal Absorptance
  0.7,                                    !- Solar Absorptance
  0.7;                                    !- Visible Absorptance

OS:WindowMaterial:Glazing,
  {1e77c02f-bd7a-4e51-b063-ea2a41c8b723}, !- Handle
  REF A CLEAR LO 6MM,                     !- Name
  SpectralAverage,                        !- Optical Data Type
  ,                                       !- Window Glass Spectral Data Set Name
  0.00599999999999998,                    !- Thickness {m}
  0.066,                                  !- Solar Transmittance at Normal Incidence
  0.341,                                  !- Front Side Solar Reflectance at Normal Incidence
  0.493,                                  !- Back Side Solar Reflectance at Normal Incidence
  0.08,                                   !- Visible Transmittance at Normal Incidence
  0.41,                                   !- Front Side Visible Reflectance at Normal Incidence
  0.37,                                   !- Back Side Visible Reflectance at Normal Incidence
  0,                                      !- Infrared Transmittance at Normal Incidence
  0.84,                                   !- Front Side Infrared Hemispherical Emissivity
  0.4,                                    !- Back Side Infrared Hemispherical Emissivity
  0.9,                                    !- Conductivity {W/m-K}
  1,                                      !- Dirt Correction Factor for Solar and Visible Transmittance
  No;                                     !- Solar Diffusing

OS:WindowMaterial:Glazing,
  {b90abe2c-d37c-4f68-838e-8e87d811e57a}, !- Handle
  Clear 3mm 1,                            !- Name
  SpectralAverage,                        !- Optical Data Type
  ,                                       !- Window Glass Spectral Data Set Name
  0.00299999999999999,                    !- Thickness {m}
  0.837,                                  !- Solar Transmittance at Normal Incidence
  0.075,                                  !- Front Side Solar Reflectance at Normal Incidence
  0.075,                                  !- Back Side Solar Reflectance at Normal Incidence
  0.898,                                  !- Visible Transmittance at Normal Incidence
  0.081,                                  !- Front Side Visible Reflectance at Normal Incidence
  0.081,                                  !- Back Side Visible Reflectance at Normal Incidence
  0,                                      !- Infrared Transmittance at Normal Incidence
  0.84,                                   !- Front Side Infrared Hemispherical Emissivity
  0.84,                                   !- Back Side Infrared Hemispherical Emissivity
  0.9,                                    !- Conductivity {W/m-K}
  1,                                      !- Dirt Correction Factor for Solar and Visible Transmittance
  No;                                     !- Solar Diffusing

OS:Rendering:Color,
  {c68c98aa-6352-4ca0-8d1a-cd8e2206870f}, !- Handle
  Rendering Color 1,                      !- Name
  60,                                     !- Rendering Red Value
  113,                                    !- Rendering Green Value
  179;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {5d11ea0b-3de5-4744-941d-427345d347c0}, !- Handle
  Rendering Color 2,                      !- Name
  250,                                    !- Rendering Red Value
  230,                                    !- Rendering Green Value
  240;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {67e4ebeb-7e1f-49bf-bc9e-f9728adfee57}, !- Handle
  Rendering Color 3,                      !- Name
  238,                                    !- Rendering Red Value
  238,                                    !- Rendering Green Value
  130;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {191080e5-06ad-4d89-91cc-06bdd8234a40}, !- Handle
  Rendering Color 4,                      !- Name
  0,                                      !- Rendering Red Value
  0,                                      !- Rendering Green Value
  100;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {ba56349a-d261-4c77-9a3f-dd204a808c40}, !- Handle
  Rendering Color 5,                      !- Name
  238,                                    !- Rendering Red Value
  238,                                    !- Rendering Green Value
  130;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {81e6c5b7-055c-4d59-9800-53cddbfe3176}, !- Handle
  Rendering Color 6,                      !- Name
  245,                                    !- Rendering Red Value
  220,                                    !- Rendering Green Value
  245;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {1dc606f4-f3b9-46d2-b242-38b6c577773c}, !- Handle
  Rendering Color 7,                      !- Name
  210,                                    !- Rendering Red Value
  140,                                    !- Rendering Green Value
  180;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {b3c96535-b45b-42dc-a35c-f5a44d4514b6}, !- Handle
  Rendering Color 8,                      !- Name
  255,                                    !- Rendering Red Value
  213,                                    !- Rendering Green Value
  239;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {3f543f93-c83f-4869-90bb-1fa2fd16b293}, !- Handle
  Rendering Color 9,                      !- Name
  128,                                    !- Rendering Red Value
  0,                                      !- Rendering Green Value
  128;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {73ad3a7d-ba13-41b6-82f7-c76a96cfc760}, !- Handle
  Rendering Color 10,                     !- Name
  255,                                    !- Rendering Red Value
  0,                                      !- Rendering Green Value
  215;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {0df59329-627c-4329-9e87-aa6e44644b9e}, !- Handle
  Rendering Color 11,                     !- Name
  255,                                    !- Rendering Red Value
  220,                                    !- Rendering Green Value
  248;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {95aa99e4-2ff3-42ad-a2d8-4155823ec314}, !- Handle
  Rendering Color 12,                     !- Name
  135,                                    !- Rendering Red Value
  250,                                    !- Rendering Green Value
  206;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {a6aafd8f-e120-4787-aa9b-6f9cbd9a7923}, !- Handle
  Rendering Color 13,                     !- Name
  138,                                    !- Rendering Red Value
  226,                                    !- Rendering Green Value
  43;                                     !- Rendering Blue Value

OS:Rendering:Color,
  {53b41d99-4bdf-4e5b-88a7-0ce391391e6f}, !- Handle
  Rendering Color 14,                     !- Name
  128,                                    !- Rendering Red Value
  0,                                      !- Rendering Green Value
  128;                                    !- Rendering Blue Value

OS:Rendering:Color,
  {40e624cb-988a-4bb0-aefa-65201cda5b39}, !- Handle
  Rendering Color 15,                     !- Name
  186,                                    !- Rendering Red Value
  211,                                    !- Rendering Green Value
  85;                                     !- Rendering Blue Value

OS:Rendering:Color,
  {0a6b46d3-5357-4dff-b102-07c307502959}, !- Handle
  Rendering Color 16,                     !- Name
  0,                                      !- Rendering Red Value
  205,                                    !- Rendering Green Value
  0;                                      !- Rendering Blue Value

OS:StandardsInformation:Material,
  {01445a23-80c4-4b72-afbd-cc5ad83d78e2}, !- Handle
  {cd82a79f-c189-471d-8aa8-a965237f0394}; !- Material Name

OS:StandardsInformation:Material,
  {0247697e-0af8-4813-9c4c-63ff31c691b4}, !- Handle
  {836f86af-2aac-4eb0-9f43-8387617cdd0e}; !- Material Name

OS:StandardsInformation:Material,
  {8cbc301b-0b52-4d9a-ae4a-569d1d46adfa}, !- Handle
  {7a38806a-684b-41a5-8a91-005964139ab8}; !- Material Name

OS:StandardsInformation:Material,
  {b2ed8c9b-1f4a-47f9-ad23-db417770be62}, !- Handle
  {b3c76bbd-7496-4933-a45f-80c633a7fc93}; !- Material Name

OS:StandardsInformation:Material,
  {38373a6d-b3ac-486c-a58e-351f359f084d}, !- Handle
  {783c0ae5-563b-418b-92a1-fdb92438bc2a}; !- Material Name

OS:StandardsInformation:Material,
  {80396461-5c44-4260-84e3-bc3c0fc3ac48}, !- Handle
  {29479a6f-f8cd-4246-ba7c-816efc56f417}; !- Material Name

OS:StandardsInformation:Material,
  {ecd6e939-8849-4d91-b155-234696adfb00}, !- Handle
  {b15b5610-af05-4443-a22f-b02165dea8ff}; !- Material Name

OS:StandardsInformation:Material,
  {31caf900-a723-4cb5-ad22-0df344d04f0e}, !- Handle
  {1ae34c2c-e9a1-44d7-afb1-1d675abb3c4a}; !- Material Name

OS:StandardsInformation:Material,
  {e15a094b-98cb-4aa0-a326-69d41299a643}, !- Handle
  {26449061-fa31-4556-957f-ed8cec4c5891}; !- Material Name

OS:StandardsInformation:Material,
  {94312010-6e6a-4dbc-9a0c-cc5d177b3dd3}, !- Handle
  {b011e73d-eae9-4fb8-9847-e3313013becf}; !- Material Name

OS:StandardsInformation:Material,
  {c2e931cb-2f17-4786-9e94-cde1b1b9f122}, !- Handle
  {9e43b4c8-a40f-45f8-be58-a78a12b21864}; !- Material Name

OS:StandardsInformation:Material,
  {0396d502-5aa8-4924-995e-7b3bfa73ba08}, !- Handle
  {d0727782-365b-4b94-8427-23e43af7633a}; !- Material Name

OS:StandardsInformation:Material,
  {2c86db71-f1b9-40fe-a3bf-df8cf3ad466f}, !- Handle
  {e911e737-0c12-4a5a-b6d0-e370e4217e79}; !- Material Name

OS:StandardsInformation:Material,
  {56d3905f-683c-4041-8f2f-f7f150a9173f}, !- Handle
  {5c69d8b7-63a6-48f1-aa9f-a30396605ce8}; !- Material Name

OS:StandardsInformation:Material,
  {88c1b3d3-1b90-48b9-8c58-f75b74574622}, !- Handle
  {f039016b-2a09-4504-ba38-1fc15ae6dfd6}; !- Material Name

OS:StandardsInformation:Material,
  {04c841c4-703c-4529-bcfb-d4b811f96c14}, !- Handle
  {17cea2e1-7e38-4e45-b384-4cef33e00e74}; !- Material Name

OS:StandardsInformation:Material,
  {28e34a18-ed66-4d95-8d38-4225aaa17273}, !- Handle
  {1e77c02f-bd7a-4e51-b063-ea2a41c8b723}; !- Material Name

OS:StandardsInformation:Material,
  {ee3b4e31-ad07-4495-abac-afeeec28af3f}, !- Handle
  {b90abe2c-d37c-4f68-838e-8e87d811e57a}; !- Material Name

OS:Space,
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Handle
  1-H,                                    !- Name
  {84b88777-4f33-4314-9a3c-f8317275bc9c}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {d1107704-c8ff-4ed5-a094-c42ff3ce64ee}, !- Building Story Name
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:BuildingStory,
  {d1107704-c8ff-4ed5-a094-c42ff3ce64ee}, !- Handle
  First Floor,                            !- Name
  2.7,                                    !- Nominal Z Coordinate {m}
  2.7,                                    !- Nominal Floor to Floor Height {m}
  ,                                       !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  {2dc56ced-30bb-4951-8a26-225297eae4d9}, !- Group Rendering Name
  2.7;                                    !- Nominal Floor to Ceiling Height {m}

OS:Rendering:Color,
  {2dc56ced-30bb-4951-8a26-225297eae4d9}, !- Handle
  Rendering Color 17,                     !- Name
  17,                                     !- Rendering Red Value
  119,                                    !- Rendering Green Value
  51,                                     !- Rendering Blue Value
  255;                                    !- Rendering Alpha Value

OS:Space,
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Handle
  1-A2.LK,                                !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {d1107704-c8ff-4ed5-a094-c42ff3ce64ee}, !- Building Story Name
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Space,
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Handle
  0-A1.WC,                                !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {5af29e95-acc0-44f3-b728-068977f4d352}, !- Building Story Name
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:BuildingStory,
  {5af29e95-acc0-44f3-b728-068977f4d352}, !- Handle
  Ground Floor,                           !- Name
  0,                                      !- Nominal Z Coordinate {m}
  2.7,                                    !- Nominal Floor to Floor Height {m}
  ,                                       !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  {d4f2f1a8-bd20-4e81-8f78-f450d842b92c}, !- Group Rendering Name
  2.7;                                    !- Nominal Floor to Ceiling Height {m}

OS:Rendering:Color,
  {d4f2f1a8-bd20-4e81-8f78-f450d842b92c}, !- Handle
  Rendering Color 18,                     !- Name
  51,                                     !- Rendering Red Value
  34,                                     !- Rendering Green Value
  136,                                    !- Rendering Blue Value
  255;                                    !- Rendering Alpha Value

OS:Space,
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Handle
  0-A1.B,                                 !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {5af29e95-acc0-44f3-b728-068977f4d352}, !- Building Story Name
  {00907fe9-4685-45fc-adcd-fdf152b89b90}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Space,
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Handle
  0-A1.LK,                                !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {5af29e95-acc0-44f3-b728-068977f4d352}, !- Building Story Name
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Space,
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Handle
  1-A2.WC,                                !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {d1107704-c8ff-4ed5-a094-c42ff3ce64ee}, !- Building Story Name
  {3fb89b5f-20ce-4142-85bb-655534344f94}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Space,
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Handle
  1-A2.B,                                 !- Name
  {35349b29-ff9f-42b4-98db-4dfb6ff9f629}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {d1107704-c8ff-4ed5-a094-c42ff3ce64ee}, !- Building Story Name
  {e966c782-dbbc-425c-bb68-6539603cd6a7}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Space,
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Handle
  0-H,                                    !- Name
  {84b88777-4f33-4314-9a3c-f8317275bc9c}, !- Space Type Name
  {ba7691de-1852-4e45-9a8b-11c2eebe1c46}, !- Default Construction Set Name
  ,                                       !- Default Schedule Set Name
  ,                                       !- Direction of Relative North {deg}
  ,                                       !- X Origin {m}
  ,                                       !- Y Origin {m}
  ,                                       !- Z Origin {m}
  {5af29e95-acc0-44f3-b728-068977f4d352}, !- Building Story Name
  {45801895-7ba0-4faf-8ef3-55403bc0271b}, !- Thermal Zone Name
  ,                                       !- Part of Total Floor Area
  ,                                       !- Design Specification Outdoor Air Object Name
  ;                                       !- Building Unit Name

OS:Surface,
  {c0f28596-a2b6-449c-8808-5f7027183f1f}, !- Handle
  Face 18,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Ground,                                 !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 8, 0,                               !- X,Y,Z Vertex 1 {m}
  13, 2.95, 0,                            !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 0,                         !- X,Y,Z Vertex 4 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 5 {m}
  8.45, 8, 0;                             !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {e652add5-5b7f-4368-b98a-1edd03c32f8e}, !- Handle
  Face 19,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {c155a487-6590-4044-b6aa-ca0ce4ebadb4}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 1 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 2 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 3 {m}
  13, 8, 2.7,                             !- X,Y,Z Vertex 4 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 5 {m}
  8.45, 1.95, 2.7;                        !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {d9af1ad5-2ccc-45ce-a61f-3b40ced0b0bc}, !- Handle
  Face 58,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {aed8f34e-ec67-42c1-b18e-11a7744a4414}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 0;                         !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {6c908541-528b-40ad-b785-f8d435680300}, !- Handle
  Face 59,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {d9af1ad5-2ccc-45ce-a61f-3b40ced0b0bc}, !- Surface Name
  {d4817446-0b7b-41b0-a77f-b5f012052861}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.9, 1.95, 2.1,                         !- X,Y,Z Vertex 1 {m}
  8.9, 1.95, 0,                           !- X,Y,Z Vertex 2 {m}
  9.7, 1.95, 0,                           !- X,Y,Z Vertex 3 {m}
  9.7, 1.95, 2.1;                         !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {60bd1aec-e8a2-49b7-a6c9-7c0a9601951f}, !- Handle
  Face 60,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {04eb0b4d-7b59-493d-b21f-52655bbab278}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 1 {m}
  8.45, 8, 0,                             !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 2.7;                        !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {bbb1e54a-7746-45c6-9dc9-d0e783cd4b93}, !- Handle
  Face 61,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 1 {m}
  13, 8, 2.7,                             !- X,Y,Z Vertex 2 {m}
  13, 8, 0,                               !- X,Y,Z Vertex 3 {m}
  8.45, 8, 0;                             !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {450f140b-279d-4d97-b6c4-6964bf4245c7}, !- Handle
  Face 62,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {bbb1e54a-7746-45c6-9dc9-d0e783cd4b93}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  11.4, 8, 2.4,                           !- X,Y,Z Vertex 1 {m}
  11.4, 8, 1,                             !- X,Y,Z Vertex 2 {m}
  9.8, 8, 1,                              !- X,Y,Z Vertex 3 {m}
  9.8, 8, 2.4;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {ebe7e93d-365e-450e-9827-6a4563a6379b}, !- Handle
  Face 63,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {238a45ac-22d0-4b30-8e4a-6af9122a8a3f}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 1 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 2 {m}
  13, 2.95, 0,                            !- X,Y,Z Vertex 3 {m}
  13, 2.95, 2.7;                          !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {9b9ef033-0cec-4914-8690-5e616150801a}, !- Handle
  Face 20,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 8, 2.7,                             !- X,Y,Z Vertex 1 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 2 {m}
  13, 2.95, 0,                            !- X,Y,Z Vertex 3 {m}
  13, 8, 0;                               !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {de05c93a-7137-4ed2-8320-35e55ddc0617}, !- Handle
  Face 64,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {db2a3fda-cb7b-470d-8b89-ca881ffe365f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {2b42b5e0-c753-4156-9ccf-a4484783739f}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 1 {m}
  10.15, 1.95, 0,                         !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 2.7;                       !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {00907fe9-4685-45fc-adcd-fdf152b89b90}, !- Handle
  TZ_0-A1.B,                              !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {8918173d-14b9-4167-bb7d-235d791e6c22}, !- Zone Air Inlet Port List
  {871b3711-bc58-477e-8147-d3d733a00930}, !- Zone Air Exhaust Port List
  {ac84a652-e0fc-4b17-84b9-993e5794a313}, !- Zone Air Node Name
  {6bebb80a-e621-4b1e-a310-cd4c461d9b20}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {fd3c5229-cc69-4ad6-80b3-4c6433f3758d}, !- Group Rendering Name
  {b7de7a59-3d2e-4013-8fc6-840000681259}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {ef31afdb-5d93-4e94-86ee-88eea857b2c2}, !- Handle
  Node 1,                                 !- Name
  {ac84a652-e0fc-4b17-84b9-993e5794a313}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {ac84a652-e0fc-4b17-84b9-993e5794a313}, !- Handle
  {00907fe9-4685-45fc-adcd-fdf152b89b90}, !- Source Object
  11,                                     !- Outlet Port
  {ef31afdb-5d93-4e94-86ee-88eea857b2c2}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {8918173d-14b9-4167-bb7d-235d791e6c22}, !- Handle
  {00907fe9-4685-45fc-adcd-fdf152b89b90}; !- HVAC Component

OS:PortList,
  {871b3711-bc58-477e-8147-d3d733a00930}, !- Handle
  {00907fe9-4685-45fc-adcd-fdf152b89b90}; !- HVAC Component

OS:PortList,
  {6bebb80a-e621-4b1e-a310-cd4c461d9b20}, !- Handle
  {00907fe9-4685-45fc-adcd-fdf152b89b90}; !- HVAC Component

OS:Sizing:Zone,
  {c1fa4734-70f8-4c44-a764-5c0b242fd8e4}, !- Handle
  {00907fe9-4685-45fc-adcd-fdf152b89b90}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {8c7efe77-b33e-44c7-8da6-c7ade337d7f0}, !- Handle
  Zone HVAC Equipment List 1,             !- Name
  {00907fe9-4685-45fc-adcd-fdf152b89b90}; !- Thermal Zone

OS:Rendering:Color,
  {fd3c5229-cc69-4ad6-80b3-4c6433f3758d}, !- Handle
  Rendering Color 19,                     !- Name
  17,                                     !- Rendering Red Value
  119,                                    !- Rendering Green Value
  51;                                     !- Rendering Blue Value

OS:Surface,
  {0dd5acb8-226f-42ab-8f62-46952624302f}, !- Handle
  Face 65,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 5.4,                            !- X,Y,Z Vertex 1 {m}
  8.45, 8, 5.4,                           !- X,Y,Z Vertex 2 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 3 {m}
  2.8, 8, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {568db39e-c75a-4025-ba26-1d190237ebaf}, !- Handle
  Face 66,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {0dd5acb8-226f-42ab-8f62-46952624302f}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  6.9, 8, 5.1,                            !- X,Y,Z Vertex 1 {m}
  6.9, 8, 3.7,                            !- X,Y,Z Vertex 2 {m}
  4.5, 8, 3.7,                            !- X,Y,Z Vertex 3 {m}
  4.5, 8, 5.1;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {29d98935-c74a-4891-b21b-6511533e1939}, !- Handle
  Face 67,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 5.4,                            !- X,Y,Z Vertex 1 {m}
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 2 {m}
  8.45, 0, 5.4,                           !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 4 {m}
  8.45, 8, 5.4;                           !- X,Y,Z Vertex 5 {m}

OS:Surface,
  {cf7baa42-170a-4ace-8c21-1d7452bd6419}, !- Handle
  Face 68,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 5.4,                           !- X,Y,Z Vertex 1 {m}
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 2 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 3 {m}
  8.45, 0, 2.7;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {325e6415-44f6-4de7-8d25-d5c9e54b0b1d}, !- Handle
  Face 69,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {00526ae9-cd8d-45cf-abe1-4b3535818cfe}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 2 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 3 {m}
  8.45, 8, 5.4;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {91f9a9dc-4d3b-4769-b904-9eeb4052f292}, !- Handle
  Face 70,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {04c6ddc3-f0bd-485d-89e6-30f96d62d94c}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 1 {m}
  8.45, 0, 5.4,                           !- X,Y,Z Vertex 2 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 2.7;                        !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {7f9b17e8-e487-4b20-accf-65c78f8f90a1}, !- Handle
  Face 71,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {91f9a9dc-4d3b-4769-b904-9eeb4052f292}, !- Surface Name
  {8ffeed56-7d29-49d4-9364-5349d0d0626b}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.45, 1, 4.8,                           !- X,Y,Z Vertex 1 {m}
  8.45, 1, 2.7,                           !- X,Y,Z Vertex 2 {m}
  8.45, 1.8, 2.7,                         !- X,Y,Z Vertex 3 {m}
  8.45, 1.8, 4.8;                         !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {fd25c6d4-0042-4818-8607-2ca42055a1dd}, !- Handle
  Face 72,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {d952ee3d-c94b-4369-92e0-7448e3f22d79}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 1 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 2 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 3 {m}
  2.8, 8, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {b94071c8-4b72-42e0-a005-e3babb1b0ac5}, !- Handle
  Face 73,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {5e085eb3-e2a4-43d9-81bc-a9da370c325f}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {a4760eaf-778d-47e6-8ee6-971eae9710df}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 1 {m}
  2.8, 8, 5.4,                            !- X,Y,Z Vertex 2 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 3 {m}
  2.8, 0, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {9fb19b70-82b4-48f5-97b5-ca0fcbb3eac3}, !- Handle
  Face 74,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {b94071c8-4b72-42e0-a005-e3babb1b0ac5}, !- Surface Name
  {688f4817-4fd9-43af-9ac5-f6b4074b7cc0}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  2.8, 1.7, 4.8,                          !- X,Y,Z Vertex 1 {m}
  2.8, 1.7, 2.7,                          !- X,Y,Z Vertex 2 {m}
  2.8, 0.8, 2.7,                          !- X,Y,Z Vertex 3 {m}
  2.8, 0.8, 4.8;                          !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}, !- Handle
  TZ_1-A2.LK,                             !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {644d0750-c9fc-4539-a613-5f86174fce8e}, !- Zone Air Inlet Port List
  {6d1eaa0e-6955-4da0-a382-4d13c1784e3b}, !- Zone Air Exhaust Port List
  {0bccd71e-93a4-4d7e-bfef-326998387cb2}, !- Zone Air Node Name
  {6284ced9-5930-4259-bb90-332b1a0cb589}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {9f706e71-f60d-4b76-8713-2881e5501cdb}, !- Group Rendering Name
  {a462539c-4a08-4c07-bce5-109a08145875}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {c9824e1e-d697-4260-b476-17987c9079fb}, !- Handle
  Node 2,                                 !- Name
  {0bccd71e-93a4-4d7e-bfef-326998387cb2}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {0bccd71e-93a4-4d7e-bfef-326998387cb2}, !- Handle
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}, !- Source Object
  11,                                     !- Outlet Port
  {c9824e1e-d697-4260-b476-17987c9079fb}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {644d0750-c9fc-4539-a613-5f86174fce8e}, !- Handle
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}; !- HVAC Component

OS:PortList,
  {6d1eaa0e-6955-4da0-a382-4d13c1784e3b}, !- Handle
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}; !- HVAC Component

OS:PortList,
  {6284ced9-5930-4259-bb90-332b1a0cb589}, !- Handle
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}; !- HVAC Component

OS:Sizing:Zone,
  {bd384f11-97de-48f4-ab4f-a67466af86dd}, !- Handle
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {3383e074-318a-4fb0-b1f9-a917c62bca5d}, !- Handle
  Zone HVAC Equipment List 2,             !- Name
  {c26e0114-fd6d-4cd3-80e6-1649020d50f6}; !- Thermal Zone

OS:Rendering:Color,
  {9f706e71-f60d-4b76-8713-2881e5501cdb}, !- Handle
  Rendering Color 20,                     !- Name
  204,                                    !- Rendering Red Value
  102,                                    !- Rendering Green Value
  119;                                    !- Rendering Blue Value

OS:Surface,
  {d952ee3d-c94b-4369-92e0-7448e3f22d79}, !- Handle
  Face 9,                                 !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {fd25c6d4-0042-4818-8607-2ca42055a1dd}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 1 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 2 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 3 {m}
  2.8, 0, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {00857968-5220-4fdc-9958-383c24658d2f}, !- Handle
  Face 8,                                 !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Ground,                                 !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 0,                             !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 2 {m}
  8.45, 0, 0,                             !- X,Y,Z Vertex 3 {m}
  2.8, 0, 0,                              !- X,Y,Z Vertex 4 {m}
  2.8, 8, 0;                              !- X,Y,Z Vertex 5 {m}

OS:Surface,
  {04eb0b4d-7b59-493d-b21f-52655bbab278}, !- Handle
  Face 10,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {60bd1aec-e8a2-49b7-a6c9-7c0a9601951f}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 2 {m}
  8.45, 8, 0,                             !- X,Y,Z Vertex 3 {m}
  8.45, 8, 2.7;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {0487290f-3ece-4c64-b42a-7e981fde2d2b}, !- Handle
  Face 11,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {bd291602-9ac8-4b02-a445-326affc3fe45}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 1 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 2 {m}
  8.45, 0, 0,                             !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 0;                          !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {f1db9afa-991e-4e09-8f24-56a74de9af54}, !- Handle
  Face 12,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {0487290f-3ece-4c64-b42a-7e981fde2d2b}, !- Surface Name
  {f1f9ef4c-a780-4d6a-88af-d4e054665c0e}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.45, 1, 2.1,                           !- X,Y,Z Vertex 1 {m}
  8.45, 1, 0,                             !- X,Y,Z Vertex 2 {m}
  8.45, 1.8, 0,                           !- X,Y,Z Vertex 3 {m}
  8.45, 1.8, 2.1;                         !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {34520a23-47f6-4fac-99b2-b79ab6a946cc}, !- Handle
  Face 13,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 1 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 2 {m}
  2.8, 0, 0,                              !- X,Y,Z Vertex 3 {m}
  8.45, 0, 0;                             !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {e7abc0b5-f228-4ce4-a863-0544f46b1517}, !- Handle
  Face 14,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {91502b33-81f9-4095-a1dd-9cfbe7c27a00}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 1 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 2 {m}
  2.8, 8, 0,                              !- X,Y,Z Vertex 3 {m}
  2.8, 0, 0;                              !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {820c1336-eff2-45e7-ac81-f710ece26981}, !- Handle
  Face 15,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {e7abc0b5-f228-4ce4-a863-0544f46b1517}, !- Surface Name
  {33d5718e-72e9-491e-a1cb-7f3b4fadf6c9}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  2.8, 1.7, 2.1,                          !- X,Y,Z Vertex 1 {m}
  2.8, 1.7, 0,                            !- X,Y,Z Vertex 2 {m}
  2.8, 0.8, 0,                            !- X,Y,Z Vertex 3 {m}
  2.8, 0.8, 2.1;                          !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {c2a9eeed-fddf-4cfd-8af5-11c96d180547}, !- Handle
  Face 16,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {96016721-452b-4d1c-a10b-0ae224bc5f1e}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 1 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 2 {m}
  8.45, 8, 0,                             !- X,Y,Z Vertex 3 {m}
  2.8, 8, 0;                              !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {fe3987d6-ab12-452d-a5e4-accc8f56d8d1}, !- Handle
  Face 17,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {c2a9eeed-fddf-4cfd-8af5-11c96d180547}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  6.9, 8, 2.4,                            !- X,Y,Z Vertex 1 {m}
  6.9, 8, 1,                              !- X,Y,Z Vertex 2 {m}
  4.5, 8, 1,                              !- X,Y,Z Vertex 3 {m}
  4.5, 8, 2.4;                            !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}, !- Handle
  TZ_0-A1.LK,                             !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {9694df8f-7064-4af1-bc76-c761da70d716}, !- Zone Air Inlet Port List
  {18ce30f7-76e0-4f88-a187-305cd8b4ab4a}, !- Zone Air Exhaust Port List
  {21ed9792-6f96-484f-ab86-c412de129a34}, !- Zone Air Node Name
  {36c2626b-763a-4e74-8622-8c797ab40dea}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {0239d9e3-9b83-4524-9bd1-f3e6fe93a2dd}, !- Group Rendering Name
  {b8b7f23d-96e6-4910-9e90-3d638984e3ce}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {c4701d2e-d940-4b86-9b54-f4a25805b39b}, !- Handle
  Node 3,                                 !- Name
  {21ed9792-6f96-484f-ab86-c412de129a34}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {21ed9792-6f96-484f-ab86-c412de129a34}, !- Handle
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}, !- Source Object
  11,                                     !- Outlet Port
  {c4701d2e-d940-4b86-9b54-f4a25805b39b}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {9694df8f-7064-4af1-bc76-c761da70d716}, !- Handle
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}; !- HVAC Component

OS:PortList,
  {18ce30f7-76e0-4f88-a187-305cd8b4ab4a}, !- Handle
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}; !- HVAC Component

OS:PortList,
  {36c2626b-763a-4e74-8622-8c797ab40dea}, !- Handle
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}; !- HVAC Component

OS:Sizing:Zone,
  {13ae94ad-2944-4487-b28b-e3b70394fb9b}, !- Handle
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {09d1d02f-bf32-460d-b470-cbfe68be692f}, !- Handle
  Zone HVAC Equipment List 3,             !- Name
  {d013a7b0-2f29-4b8d-99da-75876c79ff4f}; !- Thermal Zone

OS:Rendering:Color,
  {0239d9e3-9b83-4524-9bd1-f3e6fe93a2dd}, !- Handle
  Rendering Color 21,                     !- Name
  51,                                     !- Rendering Red Value
  34,                                     !- Rendering Green Value
  136;                                    !- Rendering Blue Value

OS:Surface,
  {a4760eaf-778d-47e6-8ee6-971eae9710df}, !- Handle
  Face 41,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {b94071c8-4b72-42e0-a005-e3babb1b0ac5}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 5.4,                            !- X,Y,Z Vertex 1 {m}
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 2 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 3 {m}
  2.8, 8, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {688f4817-4fd9-43af-9ac5-f6b4074b7cc0}, !- Handle
  Face 75,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {a4760eaf-778d-47e6-8ee6-971eae9710df}, !- Surface Name
  {9fb19b70-82b4-48f5-97b5-ca0fcbb3eac3}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  2.8, 0.8, 4.8,                          !- X,Y,Z Vertex 1 {m}
  2.8, 0.8, 2.7,                          !- X,Y,Z Vertex 2 {m}
  2.8, 1.7, 2.7,                          !- X,Y,Z Vertex 3 {m}
  2.8, 1.7, 4.8;                          !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {331db2b4-03be-4d03-889c-602f9a635938}, !- Handle
  Face 39,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {2760d81c-c91f-4147-b959-baf19ab5b7f4}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 1 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 2 {m}
  0, 0, 2.7,                              !- X,Y,Z Vertex 3 {m}
  0, 8, 2.7;                              !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {da001ab7-a1c0-4641-8af7-4931a9fec996}, !- Handle
  Face 76,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  0, 0, 5.4,                              !- X,Y,Z Vertex 1 {m}
  0, 8, 5.4,                              !- X,Y,Z Vertex 2 {m}
  0, 8, 2.7,                              !- X,Y,Z Vertex 3 {m}
  0, 0, 2.7;                              !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {76e8d9a9-d611-4929-852a-535871cf1a1e}, !- Handle
  Face 77,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {da001ab7-a1c0-4641-8af7-4931a9fec996}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  0, 2.85, 5.1,                           !- X,Y,Z Vertex 1 {m}
  0, 2.85, 3.7,                           !- X,Y,Z Vertex 2 {m}
  0, 1.25, 3.7,                           !- X,Y,Z Vertex 3 {m}
  0, 1.25, 5.1;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {ab482bec-0193-454c-a201-666c0dc4c124}, !- Handle
  Face 78,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 1 {m}
  0, 0, 5.4,                              !- X,Y,Z Vertex 2 {m}
  0, 0, 2.7,                              !- X,Y,Z Vertex 3 {m}
  2.8, 0, 2.7;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {ebd9f1e7-08c0-476f-9ca1-08c02d0cb30d}, !- Handle
  Face 40,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  0, 8, 5.4,                              !- X,Y,Z Vertex 1 {m}
  0, 0, 5.4,                              !- X,Y,Z Vertex 2 {m}
  2.8, 0, 5.4,                            !- X,Y,Z Vertex 3 {m}
  2.8, 8, 5.4;                            !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {1caa7ce2-0d3e-46ac-848b-f72d8b64f8d6}, !- Handle
  Face 79,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {a95bb80c-fe7b-42b9-9729-cf2cee541500}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  0, 8, 5.4,                              !- X,Y,Z Vertex 1 {m}
  2.8, 8, 5.4,                            !- X,Y,Z Vertex 2 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 3 {m}
  0, 8, 2.7;                              !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}, !- Handle
  TZ_1-H,                                 !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {3b76212a-fff2-4d98-8591-ab5fdac0c714}, !- Zone Air Inlet Port List
  {2e2ea9a3-946b-4948-8cdb-517d7e29660a}, !- Zone Air Exhaust Port List
  {4d6c69b2-a8e7-4a36-b893-42cf5e5db3f2}, !- Zone Air Node Name
  {5e56ec43-a407-40d6-bc2a-7bba1393e3cb}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {185b696b-dfc2-40c5-8fd6-60735ab39de3}, !- Group Rendering Name
  ,                                       !- Thermostat Name
  No;                                     !- Use Ideal Air Loads

OS:Node,
  {9041341d-e7ab-4e61-8635-3d461b3677d1}, !- Handle
  Node 4,                                 !- Name
  {4d6c69b2-a8e7-4a36-b893-42cf5e5db3f2}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {4d6c69b2-a8e7-4a36-b893-42cf5e5db3f2}, !- Handle
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}, !- Source Object
  11,                                     !- Outlet Port
  {9041341d-e7ab-4e61-8635-3d461b3677d1}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {3b76212a-fff2-4d98-8591-ab5fdac0c714}, !- Handle
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}; !- HVAC Component

OS:PortList,
  {2e2ea9a3-946b-4948-8cdb-517d7e29660a}, !- Handle
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}; !- HVAC Component

OS:PortList,
  {5e56ec43-a407-40d6-bc2a-7bba1393e3cb}, !- Handle
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}; !- HVAC Component

OS:Sizing:Zone,
  {26db50a7-dde2-4986-b92a-63aaed29b986}, !- Handle
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {c68b7a9f-de5d-44f8-aece-4fe88c15e1d8}, !- Handle
  Zone HVAC Equipment List 4,             !- Name
  {936ce426-1354-4f7d-bebb-2f5f77c44ece}; !- Thermal Zone

OS:Rendering:Color,
  {185b696b-dfc2-40c5-8fd6-60735ab39de3}, !- Handle
  Rendering Color 22,                     !- Name
  221,                                    !- Rendering Red Value
  204,                                    !- Rendering Green Value
  119;                                    !- Rendering Blue Value

OS:Surface,
  {1344683c-f452-4f78-9cf1-28201d5bd939}, !- Handle
  Face 38,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 0, 2.7,                             !- X,Y,Z Vertex 1 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 2 {m}
  8.45, 0, 0,                             !- X,Y,Z Vertex 3 {m}
  13, 0, 0;                               !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {2b42b5e0-c753-4156-9ccf-a4484783739f}, !- Handle
  Face 34,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {de05c93a-7137-4ed2-8320-35e55ddc0617}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 1 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 0,                         !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 2.7;                       !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {44bdfec6-0732-4d7b-bada-5b3bd9ced307}, !- Handle
  Face 36,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 1 {m}
  13, 0, 2.7,                             !- X,Y,Z Vertex 2 {m}
  13, 0, 0,                               !- X,Y,Z Vertex 3 {m}
  13, 2.95, 0;                            !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {66c15cd7-b9ec-4aad-b002-887fbcac34bd}, !- Handle
  Face 37,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {44bdfec6-0732-4d7b-bada-5b3bd9ced307}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  13, 1.2, 2.4,                           !- X,Y,Z Vertex 1 {m}
  13, 1.2, 1,                             !- X,Y,Z Vertex 2 {m}
  13, 2, 1,                               !- X,Y,Z Vertex 3 {m}
  13, 2, 2.4;                             !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {238a45ac-22d0-4b30-8e4a-6af9122a8a3f}, !- Handle
  Face 35,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {ebe7e93d-365e-450e-9827-6a4563a6379b}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 1 {m}
  13, 2.95, 0,                            !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 2.7;                       !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {bd291602-9ac8-4b02-a445-326affc3fe45}, !- Handle
  Face 30,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {0487290f-3ece-4c64-b42a-7e981fde2d2b}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 3 {m}
  8.45, 0, 0;                             !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {f1f9ef4c-a780-4d6a-88af-d4e054665c0e}, !- Handle
  Face 31,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {bd291602-9ac8-4b02-a445-326affc3fe45}, !- Surface Name
  {f1db9afa-991e-4e09-8f24-56a74de9af54}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.45, 1.8, 2.1,                         !- X,Y,Z Vertex 1 {m}
  8.45, 1.8, 0,                           !- X,Y,Z Vertex 2 {m}
  8.45, 1, 0,                             !- X,Y,Z Vertex 3 {m}
  8.45, 1, 2.1;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {09c4f38b-0dec-43a7-b5de-25bcbd0e5b46}, !- Handle
  Face 29,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {86483312-5a20-4948-adca-51117d72ad05}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 0, 2.7,                             !- X,Y,Z Vertex 1 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 4 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 5 {m}
  8.45, 0, 2.7;                           !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {53c72247-78b8-4e1e-ac8c-f2766da1126f}, !- Handle
  Face 28,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Ground,                                 !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 0,                             !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 0,                          !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 0,                         !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 0,                         !- X,Y,Z Vertex 4 {m}
  13, 2.95, 0,                            !- X,Y,Z Vertex 5 {m}
  13, 0, 0;                               !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {aed8f34e-ec67-42c1-b18e-11a7744a4414}, !- Handle
  Face 32,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {245f3c3f-b2b3-4322-b92b-4ecb122f6403}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {d9af1ad5-2ccc-45ce-a61f-3b40ced0b0bc}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 1 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 0,                         !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 0;                          !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {d4817446-0b7b-41b0-a77f-b5f012052861}, !- Handle
  Face 33,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {aed8f34e-ec67-42c1-b18e-11a7744a4414}, !- Surface Name
  {6c908541-528b-40ad-b785-f8d435680300}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  9.7, 1.95, 2.1,                         !- X,Y,Z Vertex 1 {m}
  9.7, 1.95, 0,                           !- X,Y,Z Vertex 2 {m}
  8.9, 1.95, 0,                           !- X,Y,Z Vertex 3 {m}
  8.9, 1.95, 2.1;                         !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}, !- Handle
  TZ_0-A1.WC,                             !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {32f76f44-2af2-45a3-a0c2-a93ad1a9cd79}, !- Zone Air Inlet Port List
  {f4dfdf07-f25c-49bf-b22d-ea26c3f1e43e}, !- Zone Air Exhaust Port List
  {ac0b2e13-81da-4793-8ece-9c493f3a5412}, !- Zone Air Node Name
  {17cf9d16-8406-4b19-80da-2709af662dc2}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {21df3a59-3270-4ca3-b4d3-53213d3e17cc}, !- Group Rendering Name
  {55589670-40b6-4f6a-afc7-790e95c32d69}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {af4a4628-8941-4494-ac89-7d6ed75575d1}, !- Handle
  Node 5,                                 !- Name
  {ac0b2e13-81da-4793-8ece-9c493f3a5412}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {ac0b2e13-81da-4793-8ece-9c493f3a5412}, !- Handle
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}, !- Source Object
  11,                                     !- Outlet Port
  {af4a4628-8941-4494-ac89-7d6ed75575d1}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {32f76f44-2af2-45a3-a0c2-a93ad1a9cd79}, !- Handle
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}; !- HVAC Component

OS:PortList,
  {f4dfdf07-f25c-49bf-b22d-ea26c3f1e43e}, !- Handle
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}; !- HVAC Component

OS:PortList,
  {17cf9d16-8406-4b19-80da-2709af662dc2}, !- Handle
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}; !- HVAC Component

OS:Sizing:Zone,
  {13c30a75-634d-447a-9168-3c0325164f59}, !- Handle
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {e48ea021-c582-44a7-a4c8-4b8d31736dc8}, !- Handle
  Zone HVAC Equipment List 5,             !- Name
  {6db1a9be-fc44-4e0e-9c76-5d1ceadcabfe}; !- Thermal Zone

OS:Rendering:Color,
  {21df3a59-3270-4ca3-b4d3-53213d3e17cc}, !- Handle
  Rendering Color 23,                     !- Name
  153,                                    !- Rendering Red Value
  153,                                    !- Rendering Green Value
  51;                                     !- Rendering Blue Value

OS:Surface,
  {c7a489f3-fd78-4e5f-aae3-a62c0bdc99cb}, !- Handle
  Face 4,                                 !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 1 {m}
  0, 0, 2.7,                              !- X,Y,Z Vertex 2 {m}
  0, 0, 0,                                !- X,Y,Z Vertex 3 {m}
  2.8, 0, 0;                              !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {22cb6f51-f22b-4530-aa00-755256fa92f5}, !- Handle
  Face 5,                                 !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  0, 0, 2.7,                              !- X,Y,Z Vertex 1 {m}
  0, 8, 2.7,                              !- X,Y,Z Vertex 2 {m}
  0, 8, 0,                                !- X,Y,Z Vertex 3 {m}
  0, 0, 0;                                !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {bf5bc328-9619-4178-aaf8-a4387da812f4}, !- Handle
  Face 6,                                 !- Name
  GlassDoor,                              !- Sub Surface Type
  ,                                       !- Construction Name
  {22cb6f51-f22b-4530-aa00-755256fa92f5}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  0, 3.25, 2.4,                           !- X,Y,Z Vertex 1 {m}
  0, 3.25, 0,                             !- X,Y,Z Vertex 2 {m}
  0, 0.85, 0,                             !- X,Y,Z Vertex 3 {m}
  0, 0.85, 2.4;                           !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {65e961e8-90e9-4e7f-873c-dd24268721ff}, !- Handle
  Face 0,                                 !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Ground,                                 !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 0,                              !- X,Y,Z Vertex 1 {m}
  2.8, 0, 0,                              !- X,Y,Z Vertex 2 {m}
  0, 0, 0,                                !- X,Y,Z Vertex 3 {m}
  0, 8, 0;                                !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {2760d81c-c91f-4147-b959-baf19ab5b7f4}, !- Handle
  Face 1,                                 !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {331db2b4-03be-4d03-889c-602f9a635938}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 1 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 2 {m}
  0, 8, 2.7,                              !- X,Y,Z Vertex 3 {m}
  0, 0, 2.7;                              !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {87d41a0f-c447-40e6-91a2-431bb12d2e9a}, !- Handle
  Face 7,                                 !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  0, 8, 2.7,                              !- X,Y,Z Vertex 1 {m}
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 2 {m}
  2.8, 8, 0,                              !- X,Y,Z Vertex 3 {m}
  0, 8, 0;                                !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {91502b33-81f9-4095-a1dd-9cfbe7c27a00}, !- Handle
  Face 2,                                 !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {30fc9702-4196-4549-ade1-4b3b17ead3ee}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {e7abc0b5-f228-4ce4-a863-0544f46b1517}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  2.8, 8, 2.7,                            !- X,Y,Z Vertex 1 {m}
  2.8, 0, 2.7,                            !- X,Y,Z Vertex 2 {m}
  2.8, 0, 0,                              !- X,Y,Z Vertex 3 {m}
  2.8, 8, 0;                              !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {33d5718e-72e9-491e-a1cb-7f3b4fadf6c9}, !- Handle
  Face 3,                                 !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {91502b33-81f9-4095-a1dd-9cfbe7c27a00}, !- Surface Name
  {820c1336-eff2-45e7-ac81-f710ece26981}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  2.8, 0.8, 2.1,                          !- X,Y,Z Vertex 1 {m}
  2.8, 0.8, 0,                            !- X,Y,Z Vertex 2 {m}
  2.8, 1.7, 0,                            !- X,Y,Z Vertex 3 {m}
  2.8, 1.7, 2.1;                          !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {45801895-7ba0-4faf-8ef3-55403bc0271b}, !- Handle
  TZ_0-H,                                 !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {f8e4edcd-a3ce-41d3-becb-9e82291feec0}, !- Zone Air Inlet Port List
  {36e577ba-9215-4006-95cf-29a7fded9089}, !- Zone Air Exhaust Port List
  {aedc610a-a53b-46e5-a630-b49a91697550}, !- Zone Air Node Name
  {fb2e88ca-5312-4e20-9e8b-f6de9a31f9a0}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {5d18cbb5-70ee-4246-bcc5-b9a512fe5773}, !- Group Rendering Name
  ,                                       !- Thermostat Name
  No;                                     !- Use Ideal Air Loads

OS:Node,
  {214ab2a6-c46f-43b7-b681-2f2d4af0d59c}, !- Handle
  Node 6,                                 !- Name
  {aedc610a-a53b-46e5-a630-b49a91697550}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {aedc610a-a53b-46e5-a630-b49a91697550}, !- Handle
  {45801895-7ba0-4faf-8ef3-55403bc0271b}, !- Source Object
  11,                                     !- Outlet Port
  {214ab2a6-c46f-43b7-b681-2f2d4af0d59c}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {f8e4edcd-a3ce-41d3-becb-9e82291feec0}, !- Handle
  {45801895-7ba0-4faf-8ef3-55403bc0271b}; !- HVAC Component

OS:PortList,
  {36e577ba-9215-4006-95cf-29a7fded9089}, !- Handle
  {45801895-7ba0-4faf-8ef3-55403bc0271b}; !- HVAC Component

OS:PortList,
  {fb2e88ca-5312-4e20-9e8b-f6de9a31f9a0}, !- Handle
  {45801895-7ba0-4faf-8ef3-55403bc0271b}; !- HVAC Component

OS:Sizing:Zone,
  {a16919d1-71dc-4f5c-9abf-42fe3a798538}, !- Handle
  {45801895-7ba0-4faf-8ef3-55403bc0271b}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {ccfc0d42-d517-4c8f-8d0d-4e7cf2692611}, !- Handle
  Zone HVAC Equipment List 6,             !- Name
  {45801895-7ba0-4faf-8ef3-55403bc0271b}; !- Thermal Zone

OS:Rendering:Color,
  {5d18cbb5-70ee-4246-bcc5-b9a512fe5773}, !- Handle
  Rendering Color 24,                     !- Name
  136,                                    !- Rendering Red Value
  204,                                    !- Rendering Green Value
  238;                                    !- Rendering Blue Value

OS:Surface,
  {c155a487-6590-4044-b6aa-ca0ce4ebadb4}, !- Handle
  Face 80,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {e652add5-5b7f-4368-b98a-1edd03c32f8e}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 8, 2.7,                             !- X,Y,Z Vertex 1 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 4 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 5 {m}
  8.45, 8, 2.7;                           !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {30186e83-e4e1-4551-a5c4-3eaec49c749d}, !- Handle
  Face 81,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 5.4,                           !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 5.4,                       !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 5.4,                       !- X,Y,Z Vertex 4 {m}
  13, 2.95, 5.4,                          !- X,Y,Z Vertex 5 {m}
  13, 8, 5.4;                             !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {c17332f0-b6b1-41ff-a566-3f4c9da2c597}, !- Handle
  Face 82,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {13019d83-8a07-4357-9176-c658a1ab1599}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 1.95, 5.4,                       !- X,Y,Z Vertex 1 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 5.4;                       !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {00526ae9-cd8d-45cf-abe1-4b3535818cfe}, !- Handle
  Face 83,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {325e6415-44f6-4de7-8d25-d5c9e54b0b1d}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 5.4,                           !- X,Y,Z Vertex 1 {m}
  8.45, 8, 2.7,                           !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 5.4;                        !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {9c25b993-0d1e-4d9f-bb80-5bb739ecaa5d}, !- Handle
  Face 84,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 8, 5.4,                             !- X,Y,Z Vertex 1 {m}
  13, 2.95, 5.4,                          !- X,Y,Z Vertex 2 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 3 {m}
  13, 8, 2.7;                             !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {dec76289-028e-45a4-a926-93b1c927aa6b}, !- Handle
  Face 85,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {de9e4cf9-7cfb-4eea-b197-8f7d769afbb0}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 2.95, 5.4,                       !- X,Y,Z Vertex 1 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 2 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 3 {m}
  13, 2.95, 5.4;                          !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {641e97c4-03a1-4333-97f2-9381b7a7db4a}, !- Handle
  Face 86,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {6d12d041-9498-4aef-8bd8-3bf6add430c4}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 1.95, 5.4,                       !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 2.7;                       !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {21ad3baf-e238-41bd-be17-f4fddf291c00}, !- Handle
  Face 87,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {641e97c4-03a1-4333-97f2-9381b7a7db4a}, !- Surface Name
  {ec2a662c-d77d-4cfa-9f4b-84319650c02b}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.9, 1.95, 4.8,                         !- X,Y,Z Vertex 1 {m}
  8.9, 1.95, 2.7,                         !- X,Y,Z Vertex 2 {m}
  9.7, 1.95, 2.7,                         !- X,Y,Z Vertex 3 {m}
  9.7, 1.95, 4.8;                         !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {ce177c66-7cbd-48ae-9ade-5c4d9b8aca7f}, !- Handle
  Face 88,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {d4ce3151-0deb-480e-a792-330673adb37c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 8, 5.4,                           !- X,Y,Z Vertex 1 {m}
  13, 8, 5.4,                             !- X,Y,Z Vertex 2 {m}
  13, 8, 2.7,                             !- X,Y,Z Vertex 3 {m}
  8.45, 8, 2.7;                           !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {c56e3179-c7ae-45d8-b398-3b85519b79d9}, !- Handle
  Face 89,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {ce177c66-7cbd-48ae-9ade-5c4d9b8aca7f}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  11.4, 8, 5.1,                           !- X,Y,Z Vertex 1 {m}
  11.4, 8, 3.7,                           !- X,Y,Z Vertex 2 {m}
  9.8, 8, 3.7,                            !- X,Y,Z Vertex 3 {m}
  9.8, 8, 5.1;                            !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {e966c782-dbbc-425c-bb68-6539603cd6a7}, !- Handle
  TZ_1-A2.B,                              !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {4db1fe32-ee5d-49e2-94ae-6e875d650c6c}, !- Zone Air Inlet Port List
  {2c247811-38c4-49ef-981d-e73f1b85867c}, !- Zone Air Exhaust Port List
  {cba18b1c-9777-4f15-a24b-a148954d2697}, !- Zone Air Node Name
  {63fdc579-7b46-4956-b00d-99c335e0c317}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {5b3a1125-fc4f-41a6-a0c6-8eda7622c38f}, !- Group Rendering Name
  {a07d3c4b-1528-4112-b9c7-6c7278c87f41}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {e8cdbb5d-9847-4480-9a31-d76986ec5d58}, !- Handle
  Node 7,                                 !- Name
  {cba18b1c-9777-4f15-a24b-a148954d2697}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {cba18b1c-9777-4f15-a24b-a148954d2697}, !- Handle
  {e966c782-dbbc-425c-bb68-6539603cd6a7}, !- Source Object
  11,                                     !- Outlet Port
  {e8cdbb5d-9847-4480-9a31-d76986ec5d58}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {4db1fe32-ee5d-49e2-94ae-6e875d650c6c}, !- Handle
  {e966c782-dbbc-425c-bb68-6539603cd6a7}; !- HVAC Component

OS:PortList,
  {2c247811-38c4-49ef-981d-e73f1b85867c}, !- Handle
  {e966c782-dbbc-425c-bb68-6539603cd6a7}; !- HVAC Component

OS:PortList,
  {63fdc579-7b46-4956-b00d-99c335e0c317}, !- Handle
  {e966c782-dbbc-425c-bb68-6539603cd6a7}; !- HVAC Component

OS:Sizing:Zone,
  {7caef8db-2e15-4cde-8f7f-237cd73e6b35}, !- Handle
  {e966c782-dbbc-425c-bb68-6539603cd6a7}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {229f0f91-37a0-485d-af20-882006290490}, !- Handle
  Zone HVAC Equipment List 7,             !- Name
  {e966c782-dbbc-425c-bb68-6539603cd6a7}; !- Thermal Zone

OS:Rendering:Color,
  {5b3a1125-fc4f-41a6-a0c6-8eda7622c38f}, !- Handle
  Rendering Color 25,                     !- Name
  136,                                    !- Rendering Red Value
  34,                                     !- Rendering Green Value
  85;                                     !- Rendering Blue Value

OS:Surface,
  {13019d83-8a07-4357-9176-c658a1ab1599}, !- Handle
  Face 90,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {c17332f0-b6b1-41ff-a566-3f4c9da2c597}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  10.15, 2.95, 5.4,                       !- X,Y,Z Vertex 1 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 5.4;                       !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {de9e4cf9-7cfb-4eea-b197-8f7d769afbb0}, !- Handle
  Face 91,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {dec76289-028e-45a4-a926-93b1c927aa6b}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 2.95, 5.4,                          !- X,Y,Z Vertex 1 {m}
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  10.15, 2.95, 5.4;                       !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {6d12d041-9498-4aef-8bd8-3bf6add430c4}, !- Handle
  Face 92,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {641e97c4-03a1-4333-97f2-9381b7a7db4a}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 1 {m}
  10.15, 1.95, 5.4,                       !- X,Y,Z Vertex 2 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 2.7;                        !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {ec2a662c-d77d-4cfa-9f4b-84319650c02b}, !- Handle
  Face 93,                                !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {6d12d041-9498-4aef-8bd8-3bf6add430c4}, !- Surface Name
  {21ad3baf-e238-41bd-be17-f4fddf291c00}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  9.7, 1.95, 4.8,                         !- X,Y,Z Vertex 1 {m}
  9.7, 1.95, 2.7,                         !- X,Y,Z Vertex 2 {m}
  8.9, 1.95, 2.7,                         !- X,Y,Z Vertex 3 {m}
  8.9, 1.95, 4.8;                         !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {e5c12426-cdf3-466f-b74c-888ef586901b}, !- Handle
  Face 94,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 2.95, 5.4,                          !- X,Y,Z Vertex 1 {m}
  13, 0, 5.4,                             !- X,Y,Z Vertex 2 {m}
  13, 0, 2.7,                             !- X,Y,Z Vertex 3 {m}
  13, 2.95, 2.7;                          !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {f3eeeb58-2100-489e-9ed1-099dd49f51d6}, !- Handle
  Face 95,                                !- Name
  OperableWindow,                         !- Sub Surface Type
  ,                                       !- Construction Name
  {e5c12426-cdf3-466f-b74c-888ef586901b}, !- Surface Name
  ,                                       !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  13, 1.2, 5.1,                           !- X,Y,Z Vertex 1 {m}
  13, 1.2, 3.7,                           !- X,Y,Z Vertex 2 {m}
  13, 2, 3.7,                             !- X,Y,Z Vertex 3 {m}
  13, 2, 5.1;                             !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {d0bd1b83-1788-4edf-9e3a-11e0bcfd286d}, !- Handle
  Face 96,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 0, 5.4,                             !- X,Y,Z Vertex 1 {m}
  8.45, 0, 5.4,                           !- X,Y,Z Vertex 2 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 3 {m}
  13, 0, 2.7;                             !- X,Y,Z Vertex 4 {m}

OS:Surface,
  {86483312-5a20-4948-adca-51117d72ad05}, !- Handle
  Face 97,                                !- Name
  Floor,                                  !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {09c4f38b-0dec-43a7-b5de-25bcbd0e5b46}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 2.95, 2.7,                          !- X,Y,Z Vertex 1 {m}
  13, 0, 2.7,                             !- X,Y,Z Vertex 2 {m}
  8.45, 0, 2.7,                           !- X,Y,Z Vertex 3 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 4 {m}
  10.15, 1.95, 2.7,                       !- X,Y,Z Vertex 5 {m}
  10.15, 2.95, 2.7;                       !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {bacf3b05-1587-45ab-8dcc-a2495db2954f}, !- Handle
  Face 98,                                !- Name
  RoofCeiling,                            !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Outdoors,                               !- Outside Boundary Condition
  ,                                       !- Outside Boundary Condition Object
  SunExposed,                             !- Sun Exposure
  WindExposed,                            !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  13, 0, 5.4,                             !- X,Y,Z Vertex 1 {m}
  13, 2.95, 5.4,                          !- X,Y,Z Vertex 2 {m}
  10.15, 2.95, 5.4,                       !- X,Y,Z Vertex 3 {m}
  10.15, 1.95, 5.4,                       !- X,Y,Z Vertex 4 {m}
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 5 {m}
  8.45, 0, 5.4;                           !- X,Y,Z Vertex 6 {m}

OS:Surface,
  {04c6ddc3-f0bd-485d-89e6-30f96d62d94c}, !- Handle
  Face 99,                                !- Name
  Wall,                                   !- Surface Type
  ,                                       !- Construction Name
  {75fb129a-62d1-47d5-a888-02236133620c}, !- Space Name
  Surface,                                !- Outside Boundary Condition
  {91f9a9dc-4d3b-4769-b904-9eeb4052f292}, !- Outside Boundary Condition Object
  NoSun,                                  !- Sun Exposure
  NoWind,                                 !- Wind Exposure
  ,                                       !- View Factor to Ground
  ,                                       !- Number of Vertices
  8.45, 0, 5.4,                           !- X,Y,Z Vertex 1 {m}
  8.45, 1.95, 5.4,                        !- X,Y,Z Vertex 2 {m}
  8.45, 1.95, 2.7,                        !- X,Y,Z Vertex 3 {m}
  8.45, 0, 2.7;                           !- X,Y,Z Vertex 4 {m}

OS:SubSurface,
  {8ffeed56-7d29-49d4-9364-5349d0d0626b}, !- Handle
  Face 100,                               !- Name
  Door,                                   !- Sub Surface Type
  ,                                       !- Construction Name
  {04c6ddc3-f0bd-485d-89e6-30f96d62d94c}, !- Surface Name
  {7f9b17e8-e487-4b20-accf-65c78f8f90a1}, !- Outside Boundary Condition Object
  ,                                       !- View Factor to Ground
  ,                                       !- Frame and Divider Name
  ,                                       !- Multiplier
  ,                                       !- Number of Vertices
  8.45, 1.8, 4.8,                         !- X,Y,Z Vertex 1 {m}
  8.45, 1.8, 2.7,                         !- X,Y,Z Vertex 2 {m}
  8.45, 1, 2.7,                           !- X,Y,Z Vertex 3 {m}
  8.45, 1, 4.8;                           !- X,Y,Z Vertex 4 {m}

OS:ThermalZone,
  {3fb89b5f-20ce-4142-85bb-655534344f94}, !- Handle
  TZ_1-A2.WC,                             !- Name
  1,                                      !- Multiplier
  ,                                       !- Ceiling Height {m}
  ,                                       !- Volume {m3}
  ,                                       !- Floor Area {m2}
  ,                                       !- Zone Inside Convection Algorithm
  ,                                       !- Zone Outside Convection Algorithm
  ,                                       !- Zone Conditioning Equipment List Name
  {db85783d-7873-49ad-8456-8f1a8eacbae0}, !- Zone Air Inlet Port List
  {6f07a742-2136-4420-98e6-93593bc43829}, !- Zone Air Exhaust Port List
  {5b3cfc38-aa42-40e6-bc2f-ed8d4e4abce7}, !- Zone Air Node Name
  {1742bf8d-12d4-431a-92e7-a960f7e691d0}, !- Zone Return Air Port List
  ,                                       !- Primary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Primary Daylighting Control
  ,                                       !- Secondary Daylighting Control Name
  ,                                       !- Fraction of Zone Controlled by Secondary Daylighting Control
  ,                                       !- Illuminance Map Name
  {5f220ef3-e4a0-4b35-8722-26be098b6937}, !- Group Rendering Name
  {57a978c3-c475-4082-8b48-3a7d3ed7ff69}, !- Thermostat Name
  Yes;                                    !- Use Ideal Air Loads

OS:Node,
  {090653c1-6a98-4dac-afd2-91e37f8ab334}, !- Handle
  Node 8,                                 !- Name
  {5b3cfc38-aa42-40e6-bc2f-ed8d4e4abce7}, !- Inlet Port
  ;                                       !- Outlet Port

OS:Connection,
  {5b3cfc38-aa42-40e6-bc2f-ed8d4e4abce7}, !- Handle
  {3fb89b5f-20ce-4142-85bb-655534344f94}, !- Source Object
  11,                                     !- Outlet Port
  {090653c1-6a98-4dac-afd2-91e37f8ab334}, !- Target Object
  2;                                      !- Inlet Port

OS:PortList,
  {db85783d-7873-49ad-8456-8f1a8eacbae0}, !- Handle
  {3fb89b5f-20ce-4142-85bb-655534344f94}; !- HVAC Component

OS:PortList,
  {6f07a742-2136-4420-98e6-93593bc43829}, !- Handle
  {3fb89b5f-20ce-4142-85bb-655534344f94}; !- HVAC Component

OS:PortList,
  {1742bf8d-12d4-431a-92e7-a960f7e691d0}, !- Handle
  {3fb89b5f-20ce-4142-85bb-655534344f94}; !- HVAC Component

OS:Sizing:Zone,
  {9f9b380d-c9cc-41bf-91f6-4d0b47a732ee}, !- Handle
  {3fb89b5f-20ce-4142-85bb-655534344f94}, !- Zone or ZoneList Name
  SupplyAirTemperature,                   !- Zone Cooling Design Supply Air Temperature Input Method
  14,                                     !- Zone Cooling Design Supply Air Temperature {C}
  11.11,                                  !- Zone Cooling Design Supply Air Temperature Difference {deltaC}
  SupplyAirTemperature,                   !- Zone Heating Design Supply Air Temperature Input Method
  40,                                     !- Zone Heating Design Supply Air Temperature {C}
  11.11,                                  !- Zone Heating Design Supply Air Temperature Difference {deltaC}
  0.0085,                                 !- Zone Cooling Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  0.008,                                  !- Zone Heating Design Supply Air Humidity Ratio {kg-H2O/kg-air}
  ,                                       !- Zone Heating Sizing Factor
  ,                                       !- Zone Cooling Sizing Factor
  DesignDay,                              !- Cooling Design Air Flow Method
  ,                                       !- Cooling Design Air Flow Rate {m3/s}
  ,                                       !- Cooling Minimum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Cooling Minimum Air Flow {m3/s}
  ,                                       !- Cooling Minimum Air Flow Fraction
  DesignDay,                              !- Heating Design Air Flow Method
  ,                                       !- Heating Design Air Flow Rate {m3/s}
  ,                                       !- Heating Maximum Air Flow per Zone Floor Area {m3/s-m2}
  ,                                       !- Heating Maximum Air Flow {m3/s}
  ,                                       !- Heating Maximum Air Flow Fraction
  No,                                     !- Account for Dedicated Outdoor Air System
  NeutralSupplyAir,                       !- Dedicated Outdoor Air System Control Strategy
  autosize,                               !- Dedicated Outdoor Air Low Setpoint Temperature for Design {C}
  autosize,                               !- Dedicated Outdoor Air High Setpoint Temperature for Design {C}
  Sensible Load Only No Latent Load,      !- Zone Load Sizing Method
  HumidityRatioDifference,                !- Zone Latent Cooling Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Dehumidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Cooling Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  HumidityRatioDifference,                !- Zone Latent Heating Design Supply Air Humidity Ratio Input Method
  ,                                       !- Zone Humidification Design Supply Air Humidity Ratio {kgWater/kgDryAir}
  0.005,                                  !- Zone Humidification Design Supply Air Humidity Ratio Difference {kgWater/kgDryAir}
  ,                                       !- Zone Humidistat Dehumidification Set Point Schedule Name
  ,                                       !- Zone Humidistat Humidification Set Point Schedule Name
  ,                                       !- Design Zone Air Distribution Effectiveness in Cooling Mode
  ,                                       !- Design Zone Air Distribution Effectiveness in Heating Mode
  ,                                       !- Design Zone Secondary Recirculation Fraction {dimensionless}
  ,                                       !- Design Minimum Zone Ventilation Efficiency {dimensionless}
  Coincident;                             !- Sizing Option

OS:ZoneHVAC:EquipmentList,
  {769a01b7-b895-4832-b494-0cfb64237e20}, !- Handle
  Zone HVAC Equipment List 8,             !- Name
  {3fb89b5f-20ce-4142-85bb-655534344f94}; !- Thermal Zone

OS:Rendering:Color,
  {5f220ef3-e4a0-4b35-8722-26be098b6937}, !- Handle
  Rendering Color 26,                     !- Name
  68,                                     !- Rendering Red Value
  170,                                    !- Rendering Green Value
  153;                                    !- Rendering Blue Value

OS:ScheduleTypeLimits,
  {baf3cf4f-1f20-44c6-9fff-127d46579899}, !- Handle
  Dimensionless,                          !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous;                             !- Numeric Type

OS:ScheduleTypeLimits,
  {84d9af42-03c6-487e-a8ed-335c69829283}, !- Handle
  Dimensionless 1,                        !- Name
  -1,                                     !- Lower Limit Value
  1,                                      !- Upper Limit Value
  Continuous;                             !- Numeric Type

OS:ScheduleTypeLimits,
  {d1272f4a-3c34-41cb-aa41-7016c9768629}, !- Handle
  Integer,                                !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Discrete;                               !- Numeric Type

OS:ScheduleTypeLimits,
  {49634cc1-a21f-452d-88aa-b256b5555afb}, !- Handle
  Dimensionless 2,                        !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous;                             !- Numeric Type

OS:ScheduleTypeLimits,
  {3206a878-69d3-4c3f-a342-78272f3f9bb4}, !- Handle
  Integer 1,                              !- Name
  0,                                      !- Lower Limit Value
  4,                                      !- Upper Limit Value
  Discrete;                               !- Numeric Type

OS:ScheduleTypeLimits,
  {8288f491-7594-4791-bc6d-a20535b730b8}, !- Handle
  Dimensionless 3,                        !- Name
  0.1,                                    !- Lower Limit Value
  1000,                                   !- Upper Limit Value
  Continuous;                             !- Numeric Type

OS:ScheduleTypeLimits,
  {37c5c1bc-8f5e-42d0-b39b-a2e3b8120e56}, !- Handle
  OnOff,                                  !- Name
  0,                                      !- Lower Limit Value
  1,                                      !- Upper Limit Value
  Discrete,                               !- Numeric Type
  Availability;                           !- Unit Type

OS:ScheduleTypeLimits,
  {df55b113-7436-450f-b422-0e6fda873275}, !- Handle
  Capacity,                               !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Capacity;                               !- Unit Type

OS:ScheduleTypeLimits,
  {162c745c-d6fd-425b-94c9-5346c91881ec}, !- Handle
  ControlMode,                            !- Name
  0,                                      !- Lower Limit Value
  1,                                      !- Upper Limit Value
  Discrete,                               !- Numeric Type
  ControlMode;                            !- Unit Type

OS:ScheduleTypeLimits,
  {0e9f779a-93a1-4e45-836e-d8b456f58b88}, !- Handle
  DeltaTemperature,                       !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  DeltaTemperature;                       !- Unit Type

OS:ScheduleTypeLimits,
  {43f96691-a985-45e0-af4f-c8754ee6ab50}, !- Handle
  Dimensionless 4,                        !- Name
  0,                                      !- Lower Limit Value
  1,                                      !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Dimensionless;                          !- Unit Type

OS:ScheduleTypeLimits,
  {2ef9a0a9-fb63-420b-95ef-fda1d25581ac}, !- Handle
  LinearPowerDensity,                     !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  LinearPowerDensity;                     !- Unit Type

OS:ScheduleTypeLimits,
  {ba3a759f-aa4a-4421-8d43-6547feb5bf06}, !- Handle
  MassFlowRate,                           !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  MassFlowRate;                           !- Unit Type

OS:ScheduleTypeLimits,
  {59bf7fda-3e00-4aad-8af7-5ba7325b6b46}, !- Handle
  Percent,                                !- Name
  0,                                      !- Lower Limit Value
  100,                                    !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Percent;                                !- Unit Type

OS:ScheduleTypeLimits,
  {f0fbb042-057d-49de-839d-7fa4a7419797}, !- Handle
  Pressure,                               !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Pressure;                               !- Unit Type

OS:ScheduleTypeLimits,
  {c9862f87-f06f-48a5-8570-16a6bbc2c8cb}, !- Handle
  RotationsPerMinute,                     !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  RotationsPerMinute;                     !- Unit Type

OS:ScheduleTypeLimits,
  {08abeb68-7671-469d-a896-7aca3c92498a}, !- Handle
  Temperature,                            !- Name
  ,                                       !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Temperature;                            !- Unit Type

OS:ScheduleTypeLimits,
  {213e9409-65e6-45c6-a22c-0953310d98cb}, !- Handle
  Temperature 1,                          !- Name
  ,                                       !- Lower Limit Value
  0,                                      !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Temperature;                            !- Unit Type

OS:ScheduleTypeLimits,
  {0e1901cc-43a5-4280-a897-104fca81e4eb}, !- Handle
  Temperature 2,                          !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Temperature;                            !- Unit Type

OS:ScheduleTypeLimits,
  {e92f549d-ec6a-4ee8-99ab-cbc5fe7e0348}, !- Handle
  Temperature 3,                          !- Name
  0,                                      !- Lower Limit Value
  100,                                    !- Upper Limit Value
  Continuous,                             !- Numeric Type
  Temperature;                            !- Unit Type

OS:ScheduleTypeLimits,
  {74d52450-5e15-4fab-8a38-05216e54a731}, !- Handle
  VolumetricFlowRate,                     !- Name
  0,                                      !- Lower Limit Value
  ,                                       !- Upper Limit Value
  Continuous,                             !- Numeric Type
  VolumetricFlowRate;                     !- Unit Type

OS:Schedule:Ruleset,
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Handle
  Heating setpoint,                       !- Name
  {08abeb68-7671-469d-a896-7aca3c92498a}, !- Schedule Type Limits Name
  {faa87d5d-fb54-46bf-9ece-96f1f9fb52b9}; !- Default Day Schedule Name

OS:Schedule:Day,
  {faa87d5d-fb54-46bf-9ece-96f1f9fb52b9}, !- Handle
  Schedule Day 1,                         !- Name
  {08abeb68-7671-469d-a896-7aca3c92498a}, !- Schedule Type Limits Name
  ,                                       !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  20;                                     !- Value Until Time 1

OS:Schedule:Ruleset,
  {316832f9-2591-45db-8e7c-ab44035b87b9}, !- Handle
  Cooling setpoint,                       !- Name
  {08abeb68-7671-469d-a896-7aca3c92498a}, !- Schedule Type Limits Name
  {0be2dbfe-cf3e-4448-9514-bddcd16600ea}; !- Default Day Schedule Name

OS:Schedule:Day,
  {0be2dbfe-cf3e-4448-9514-bddcd16600ea}, !- Handle
  Schedule Day 2,                         !- Name
  {08abeb68-7671-469d-a896-7aca3c92498a}, !- Schedule Type Limits Name
  ,                                       !- Interpolate to Timestep
  24,                                     !- Hour 1
  0,                                      !- Minute 1
  26;                                     !- Value Until Time 1

OS:ThermostatSetpoint:DualSetpoint,
  {b7de7a59-3d2e-4013-8fc6-840000681259}, !- Handle
  Thermostat Setpoint Dual Setpoint 1,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:ThermostatSetpoint:DualSetpoint,
  {b8b7f23d-96e6-4910-9e90-3d638984e3ce}, !- Handle
  Thermostat Setpoint Dual Setpoint 2,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:ThermostatSetpoint:DualSetpoint,
  {55589670-40b6-4f6a-afc7-790e95c32d69}, !- Handle
  Thermostat Setpoint Dual Setpoint 3,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:ThermostatSetpoint:DualSetpoint,
  {a462539c-4a08-4c07-bce5-109a08145875}, !- Handle
  Thermostat Setpoint Dual Setpoint 4,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:ThermostatSetpoint:DualSetpoint,
  {57a978c3-c475-4082-8b48-3a7d3ed7ff69}, !- Handle
  Thermostat Setpoint Dual Setpoint 5,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:ThermostatSetpoint:DualSetpoint,
  {a07d3c4b-1528-4112-b9c7-6c7278c87f41}, !- Handle
  Thermostat Setpoint Dual Setpoint 6,    !- Name
  {8be8fcd0-b8aa-424f-a3d6-d53a60ac7248}, !- Heating Setpoint Temperature Schedule Name
  {316832f9-2591-45db-8e7c-ab44035b87b9}; !- Cooling Setpoint Temperature Schedule Name

OS:WeatherFile,
  {96584efe-1184-444c-ae0b-b73551aac624}, !- Handle
  MILAN,                                  !- City
  -,                                      !- State Province Region
  ITA,                                    !- Country
  IWEC Data,                              !- Data Source
  160660,                                 !- WMO Number
  45.62,                                  !- Latitude {deg}
  8.73,                                   !- Longitude {deg}
  1,                                      !- Time Zone {hr}
  211,                                    !- Elevation {m}
  ITA_Milan.160660_IWEC.epw,              !- Url
  1EBE5C87,                               !- Checksum
  ,                                       !- Start Date Actual Year
  Sunday;                                 !- Start Day of Week

