==== Base does not Surround subsurface details ====
Surface=FACE 5 No-Overlap
Surface#=   34 NSides=    4
Vertex     1=(           0.00,           0.00,           2.70)
Vertex     2=(          -5.66,           5.66,           2.70)
Vertex     3=(          -5.66,           5.66,           0.00)
Vertex     4=(           0.00,           0.00,           0.00)
SubSurface=FACE 6
Surface#=   39 NSides=    4
Vertex     1=(          -2.30,           2.30,           2.40)
Vertex     2=(          -2.30,           2.30,           0.00)
Vertex     3=(          -0.60,           0.60,           0.00)
Vertex     4=(          -0.60,           0.60,           2.40)
================================
Shadowing Combinations
..Solar Distribution=FullExterior
..In the following, only the first 10 reference surfaces will be shown.
..But all surfaces are used in the calculations.
==================================
Surface=FACE 20 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 58 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 59 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 60 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 61 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 62
==================================
Surface=FACE 62 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 63 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 64 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 18 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 19 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 10 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 11 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 12 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 13 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 14 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 15 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 16 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 17
==================================
Surface=FACE 17 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 8 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 9 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 30 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 31 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 32 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 33 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 34 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 35 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 36 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 37
==================================
Surface=FACE 37 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 38 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 28 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 29 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 2 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 3 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 4 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 5 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 6
==================================
Surface=FACE 6 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 7 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 0 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 1 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 82 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 83 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 84 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 85 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 86 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 87 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 88 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 89
==================================
Surface=FACE 89 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 80 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 81 is used as Receiving Surface in calculations and is non-convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 65 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 66
==================================
Surface=FACE 66 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 68 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 69 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 70 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 71 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 73 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 74 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 72 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 67 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 90 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 91 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 92 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 93 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 94 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 95
==================================
Surface=FACE 95 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 96 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 99 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 100 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 97 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 98 is used as Receiving Surface in calculations and is non-convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 41 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 75 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 76 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=1
....Surface=FACE 77
==================================
Surface=FACE 77 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 78 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 79 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 39 is not used as Receiving Surface in calculations.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
==================================
Surface=FACE 40 is used as Receiving Surface in calculations and is convex.
Number of general casting surfaces=0
Number of back surfaces=0
Number of receiving sub surfaces=0
