# OpenStudio Results

## Model Summary

Data | Value
--- | ---
Building Name | Two story apartment
Total Site Energy | 34,761 kWh
Total Building Area | 208 m^2
Total Site EUI | 167.12 kWh/m^2
OpenStudio Standards Building Type | n/a

| Value
--- | ---
Weather File | MILAN - ITA IWEC Data WMO#=160660
Latitude | 45.62
Longitude | 8.73
Elevation | 211 m
Time Zone | 1.00
North Axis Angle | -45.0
ASHRAE Climate Zone |

| Maximum Dry Bulb (C) | Daily Temperature Range (K) | Humidity Value | Humidity Type | Wind Speed (m/s) | Wind Direction
--- | --- | --- | --- | --- | --- | ---
None | 0.0 | 0.0 | 0.0 |  | 0.0 | 0.0

Time Setpoint Not Met | Time (hr)
--- | ---
During Heating | 0.0
During Cooling | 0.0
During Occupied Heating | 0.0
During Occupied Cooling | 0.0

Tolerance for Time Setpoint Not Met | Temperature (C)
--- | ---
Heating | 0.2
Cooling | 0.2

## Annual Overview

End Use | Consumption (kWh)
--- | ---
Heating | 23,308
Cooling | 1,306
Interior Lighting | 5,911
Exterior Lighting | 0
Interior Equipment | 4,239
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

Fuel | Consumption (kWh)
--- | ---
Electricity | 10,150
Natural Gas | 0
Gasoline | 0
Diesel | 0
Coal | 0
Fuel Oil No 1 | 0
Fuel Oil No 2 | 0
Propane | 0
Other Fuel 1 | 0
Other Fuel 2 | 0
District Cooling | 1,306
District Heating Water | 23,308
District Heating Steam | 0

End Use | Consumption (kWh)
--- | ---
Heating | 0
Cooling | 0
Interior Lighting | 5,911
Exterior Lighting | 0
Interior Equipment | 4,239
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

End Use | Consumption (kWh)
--- | ---
Heating | 0
Cooling | 0
Interior Lighting | 0
Exterior Lighting | 0
Interior Equipment | 0
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

## Monthly Overview

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting | 502.1 | 453.51 | 502.1 | 485.9 | 502.1 | 485.9 | 502.1 | 502.1 | 485.9 | 502.1 | 485.9 | 502.1 | 5911.79
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment | 359.97 | 325.13 | 359.97 | 348.36 | 359.97 | 348.36 | 359.97 | 359.97 | 348.36 | 359.97 | 348.36 | 359.97 | 4238.32
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total | 862.06 | 778.64 | 862.06 | 834.26 | 862.06 | 834.26 | 862.06 | 862.06 | 834.26 | 862.06 | 834.26 | 862.06 | 10150.11

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  | 48.67 | 280.91 | 595.21 | 333.79 | 46.4 |  |  |  | 1304.99
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total |  |  |  |  | 48.67 | 280.91 | 595.21 | 333.79 | 46.4 |  |  |  | 1304.99

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating | 5001.86 | 3900.22 | 2667.2 | 1672.86 | 545.72 | 152.31 | 4.8 | 17.17 | 376.86 | 1424.14 | 3066.5 | 4477.33 | 23306.98
Cooling |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total | 5001.86 | 3900.22 | 2667.2 | 1672.86 | 545.72 | 152.31 | 4.8 | 17.17 | 376.86 | 1424.14 | 3066.5 | 4477.33 | 23306.98

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748 | 1.1748
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166 | 0.8166
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99 | 1.99

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  | 1655.24 | 4713.66 | 4921.47 | 3539.7 | 1660.79 |  |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total |  |  |  |  | 1655.24 | 4713.66 | 4921.47 | 3539.7 | 1660.79 |  |  |

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating | 12333.74 | 10190.36 | 8846.0 | 7885.99 | 4435.14 | 4301.23 | 566.32 | 1396.11 | 4157.98 | 6961.16 | 8765.88 | 11114.51
Cooling |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total | 12333.74 | 10190.36 | 8846.0 | 7885.99 | 4435.14 | 4301.23 | 566.32 | 1396.11 | 4157.98 | 6961.16 | 8765.88 | 11114.51

## Utility Bills/Rates

##### No Data to Show for Utility Bills/Rates

## Envelope Summary

Construction | Net Area (m^2) | Surface Count | R Value (m^2*K/W)
--- | --- | --- | ---
Typical IEAD Roof R-17.24 10 | 104.0 | 4 | 2.90
Typical Insulated Steel Framed Exterior Wall R-11.24 4 | 205.4 | 18 | 1.83

Construction | Net Area (m^2) | Surface Count | U-factor (W/m^2*K) | SHGC | VLT
--- | --- | --- | --- | --- | ---
U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 23 | 15.7 | 7 | 3.35 | 0.36 | 0.27
U 0.88 SHGC 0.16 Sgl Ref-A-L Clr 6mm | 5.8 | 1 | 150.00 | 0.07 | 0.08

Material Name
##### (Material Layers in Construction 'U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 23':)
U 0.59 SHGC 0.36 Simple Glazing U-0.59 SHGC 0.36 23
##### (Material Layers in Construction 'U 0.88 SHGC 0.16 Sgl Ref-A-L Clr 6mm':)
REF A CLEAR LO 6MM

Description | Total (%) | North (%) | East (%) | South (%) | West (%)
--- | --- | --- | --- | --- | ---
Gross Window-Wall Ratio | 9.45 | 15.95 | 5.19 | 0.0 | 18.52
Gross Window-Wall Ratio (Conditioned) | 8.76 | 20.33 | 5.19 | 0.0 | 0.0
Skylight-Roof Ratio | 0.0 |  |  |  |

## Space Type Breakdown

Space Type Name | Floor Area (m^2) | Standards Building Type | Standards Space Type
--- | --- | --- | ---
Bedroom | 49 |  |
MidriseApartment Apartment | 114 | MidriseApartment | Apartment
MidriseApartment Corridor | 45 | MidriseApartment | Corridor

## Space Type Summary

Definition | Value | Unit | Inst. Multiplier
--- | --- | --- | ---
Bedroom People Definition | 0.0310 | people/m^2 | 1.0
Bedroom Elec Equip Definition | 5.0000 | W/m^2 | 1.0
Bedroom Lights Definition | 6.0000 | W/m^2 | 1.0
Bedroom Infiltration Level: Average | 0.6000 | ach |
Category II Ventilation Residential (outdoor air method Sum) | 25.2000 | m^3/h/person |

Definition | Value | Unit | Inst. Multiplier
--- | --- | --- | ---
MidriseApartment Apartment People Definition | 0.0283 | people/m^2 | 1.0
MidriseApartment Apartment Elec Equip Definition | 5.3820 | W/m^2 | 1.0
MidriseApartment Apartment Lights Definition | 3.8750 | W/m^2 | 1.0
MidriseApartment Apartment Infiltration | 0.0011 | m^3/h/ext wall area m^2 |
MidriseApartment Apartment Ventilation (outdoor air method Sum) | 61.1644 | m^3/h/person |

Definition | Value | Unit | Inst. Multiplier
--- | --- | --- | ---
MidriseApartment Corridor Lights Definition | 9.9028 | W/m^2 | 1.0
MidriseApartment Corridor Infiltration | 0.0011 | m^3/h/ext wall area m^2 |

## Interior Lighting Summary

Lights | Zone | Lighting Power Density (W/m^2) | Total Power (W) | Schedule Name | Scheduled Hours/Week (hr) | Actual Load Hours/Week (hr) | Return Air Fraction | Annual Consumption (kWh)
--- | --- | --- | --- | --- | --- | --- | --- | ---
1-A2.B BEDROOM LIGHTS |  | 6.0 | 148.07 | BEDROOM SCHEDULE LIGHT | 49.0 | 49.0 | 0.0000 | 377.78
0-A1.B BEDROOM LIGHTS |  | 6.0 | 148.07 | BEDROOM SCHEDULE LIGHT | 49.0 | 49.0 | 0.0000 | 377.78
1-A2.WC MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 45.42 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 130.56
1-A2.LK MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 175.15 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 502.78
0-A1.WC MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 45.42 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 130.56
0-A1.LK MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 175.15 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 502.78
1-H MIDRISEAPARTMENT CORRIDOR LIGHTS |  | 9.9 | 221.82 | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.0 | 168.0 | 0.0000 | 1944.44
0-H MIDRISEAPARTMENT CORRIDOR LIGHTS |  | 9.9 | 221.82 | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.0 | 168.0 | 0.0000 | 1944.44

Load Name | Definition Name | Load Type | Load (units) | Multiplier | Total Load (W)
--- | --- | --- | --- | --- | ---
##### (Space Name: '1-A2.WC', Area: 12 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 45
##### (Space Name: '1-H', Area: 22 m^2, Total LPD: 9.9 W/m^2) |  |  |  |  |
MidriseApartment Corridor Lights | MidriseApartment Corridor Lights Definition | Spacetype | 9.9 (W/m^2) | 1 | 222
##### (Space Name: '0-H', Area: 22 m^2, Total LPD: 9.9 W/m^2) |  |  |  |  |
MidriseApartment Corridor Lights | MidriseApartment Corridor Lights Definition | Spacetype | 9.9 (W/m^2) | 1 | 222
##### (Space Name: '1-A2.LK', Area: 45 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 175
##### (Space Name: '0-A1.WC', Area: 12 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 45
##### (Space Name: '1-A2.B', Area: 25 m^2, Total LPD: 6.0 W/m^2) |  |  |  |  |
Bedroom Lights | Bedroom Lights Definition | Spacetype | 6.0 (W/m^2) | 1 | 148
##### (Space Name: '0-A1.B', Area: 25 m^2, Total LPD: 6.0 W/m^2) |  |  |  |  |
Bedroom Lights | Bedroom Lights Definition | Spacetype | 6.0 (W/m^2) | 1 | 148
##### (Space Name: '0-A1.LK', Area: 45 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 175

Space Name | Control Name | Zone Controlled (type, fraction) | Illuminance Setpoint (lux)
--- | --- | --- | ---

## Plug Loads Summary

| Electricity Annual Value (kWh)
--- | ---
InteriorEquipment:Electricity:Zone:TZ_1-A2.B | 352.78
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.B | 352.78
InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 352.78
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 352.78
InteriorEquipment:Electricity:Zone:TZ_1-A2.WC | 363.89
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.WC | 363.89
InteriorEquipment:Electricity:Zone:TZ_1-A2.LK | 1402.78
General:InteriorEquipment:Electricity:Zone:TZ_1-A2.LK | 1402.78
InteriorEquipment:Electricity:Zone:TZ_0-A1.WC | 363.89
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.WC | 363.89
InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 1402.78
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 1402.78

Equipment Name | Definition | Load (units) | Inheritance Level | Multiplier | Total Load (W)
--- | --- | --- | --- | --- | ---
##### (Space Name: 0-A1.B, Area: 25 m^2) |  |  |  |  |
Bedroom Elec Equip | Bedroom Elec Equip Definition | 5.0 (W/m^2) | spacetype | 1.0 | 123
##### (Space Name: 0-A1.LK, Area: 45 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 243
##### (Space Name: 0-A1.WC, Area: 12 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 63
##### (Space Name: 1-A2.B, Area: 25 m^2) |  |  |  |  |
Bedroom Elec Equip | Bedroom Elec Equip Definition | 5.0 (W/m^2) | spacetype | 1.0 | 123
##### (Space Name: 1-A2.LK, Area: 45 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 243
##### (Space Name: 1-A2.WC, Area: 12 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 63

## Exterior Lighting

##### No Data to Show for Exterior Lighting

## Water Use Equipment

##### No Data to Show for Water Use Equipment

## HVAC Load Profiles

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Average Outdoor Air Dry Bulb (C) | 0.3 | 2.2 | 7.5 | 10.9 | 16.3 | 19.7 | 23.1 | 22.2 | 17.6 | 12.5 | 6.5 | 2.2
Cooling Load (kWh) | 0.0 | 0.0 | 0.0 | 0.0 | 48.67 | 280.91 | 595.21 | 333.79 | 46.4 | 0.0 | 0.0 | 0.0
Heating Load (kWh) | 5001.86 | 3900.22 | 2667.2 | 1672.86 | 545.72 | 152.31 | 4.8 | 17.17 | 376.86 | 1424.14 | 3066.5 | 4477.33

## Zone Conditions

Zone | Unmet Htg (hr) | Unmet Htg - Occ (hr) | < 13 (C) | 13-16 (C) | 16-18 (C) | 18-20 (C) | 20-21 (C) | 21-22 (C) | 22-23 (C) | 23-24 (C) | 24-26 (C) | 26-28 (C) | 28-30 (C) | >= 30 (C) | Unmet Clg (hr) | Unmet Clg - Occ (hr) | Mean Temp (C)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 0 | 0 | 0 | 0 | 0 | 138 | 6154 | 637 | 695 | 551 | 562 | 23 | 0 | 0 | 0 | 0 | 20.9 (C)
TZ_0-A1.LK | 0 | 0 | 0 | 0 | 0 | 121 | 6100 | 580 | 572 | 518 | 733 | 136 | 0 | 0 | 0 | 0 | 21.0 (C)
TZ_0-A1.WC | 0 | 0 | 0 | 0 | 0 | 175 | 6273 | 537 | 474 | 455 | 673 | 173 | 0 | 0 | 0 | 0 | 20.9 (C)
TZ_0-H | 0 | 0 | 2276 | 1420 | 938 | 889 | 443 | 402 | 458 | 419 | 725 | 451 | 255 | 84 | 0 | 0 | 17.8 (C)
TZ_1-A2.B | 0 | 0 | 0 | 0 | 0 | 143 | 5650 | 433 | 454 | 379 | 967 | 734 | 0 | 0 | 0 | 0 | 21.5 (C)
TZ_1-A2.LK | 0 | 0 | 0 | 0 | 0 | 135 | 5709 | 402 | 424 | 359 | 909 | 822 | 0 | 0 | 0 | 0 | 21.5 (C)
TZ_1-A2.WC | 0 | 0 | 0 | 0 | 0 | 195 | 5897 | 422 | 369 | 355 | 838 | 684 | 0 | 0 | 0 | 0 | 21.3 (C)
TZ_1-H | 0 | 0 | 2620 | 1198 | 775 | 769 | 386 | 320 | 344 | 374 | 616 | 498 | 378 | 482 | 0 | 0 | 17.9 (C)

Zone | < 30 (%) | 30-35 (%) | 35-40 (%) | 40-45 (%) | 45-50 (%) | 50-55 (%) | 55-60 (%) | 60-65 (%) | 65-70 (%) | 70-75 (%) | 75-80 (%) | >= 80 (%) | Mean Relative Humidity (%)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 2361 | 896 | 581 | 585 | 513 | 631 | 627 | 739 | 602 | 468 | 444 | 313 | 46.0 (%)
TZ_0-A1.LK | 2444 | 881 | 580 | 602 | 584 | 634 | 632 | 702 | 630 | 505 | 372 | 194 | 45.1 (%)
TZ_0-A1.WC | 2540 | 868 | 564 | 607 | 591 | 629 | 592 | 687 | 571 | 508 | 385 | 218 | 44.7 (%)
TZ_0-H | 725 | 667 | 880 | 973 | 904 | 1031 | 1024 | 1028 | 733 | 545 | 206 | 44 | 50.4 (%)
TZ_1-A2.B | 2409 | 961 | 780 | 806 | 650 | 634 | 659 | 644 | 471 | 390 | 250 | 106 | 43.2 (%)
TZ_1-A2.LK | 2485 | 937 | 697 | 789 | 669 | 635 | 691 | 670 | 504 | 424 | 183 | 76 | 43.0 (%)
TZ_1-A2.WC | 2571 | 923 | 642 | 718 | 662 | 637 | 641 | 666 | 511 | 411 | 266 | 112 | 43.1 (%)
TZ_1-H | 733 | 625 | 841 | 910 | 1022 | 1038 | 1187 | 1123 | 690 | 422 | 166 | 3 | 50.2 (%)

## Zone Overview

| Area (m^2) | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Volume (m^3) | Multiplier | Above Ground Gross Wall Area (m^2) | Underground Gross Wall Area (m^2) | Window Glass Area (m^2) | Lighting (W/m^2) | People (m^2/person) | Plug and Process (W/m^2)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 24.68 | Yes | Yes | 66.63 | 1.00 | 25.92 | 0.0 | 2.24 | 6.0 | 32.26 | 5.0
TZ_0-A1.LK | 45.2 | Yes | Yes | 122.04 | 1.00 | 30.51 | 0.0 | 3.36 | 3.88 | 35.32 | 5.38
TZ_0-A1.WC | 11.72 | Yes | Yes | 31.65 | 1.00 | 20.25 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_0-H | 22.4 | No | Yes | 60.48 | 1.00 | 36.72 | 0.0 | 5.76 | 9.9 | 0.0 | 0.0
TZ_1-A2.B | 24.68 | Yes | Yes | 66.63 | 1.00 | 25.92 | 0.0 | 2.24 | 6.0 | 32.26 | 5.0
TZ_1-A2.LK | 45.2 | Yes | Yes | 122.04 | 1.00 | 30.51 | 0.0 | 3.36 | 3.88 | 35.32 | 5.38
TZ_1-A2.WC | 11.72 | Yes | Yes | 31.65 | 1.00 | 20.25 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_1-H | 22.4 | No | Yes | 60.48 | 1.00 | 36.72 | 0.0 | 2.24 | 9.9 | 0.0 | 0.0
Total | 208.0 |  |  | 561.6 |  | 226.8 | 0.0 | 21.44 | 5.68 | 43.76 | 4.13
Conditioned Total | 163.2 |  |  | 440.64 |  | 153.36 | 0.0 | 13.44 | 4.52 | 34.34 | 5.27
Unconditioned Total | 44.8 |  |  | 120.96 |  | 73.44 | 0.0 | 8.0 | 9.9 | 0.0 | 0.0
Not Part of Total | 0.0 |  |  | 0.0 |  | 0.0 | 0.0 | 0.0 | 0.0 | 0.0 | 0.0

| Heating/Cooling | Calculated Design Load | Design Load With Sizing Factor | Calculated Design Air Flow (m^3/h) | Design Air Flow With Sizing Factor (m^3/h) | Date/Time Of Peak | Outdoor Temperature at Peak Load (C) | Outdoor Humidity Ratio at Peak Load (kgWater/kgAir)
--- | --- | --- | --- | --- | --- | --- | --- | ---
None | Cooling | 0.0 (W) | 0.0 (W) | 0.0 | 0.0 |  | 0.0 | 0.0
None | Heating | 0.0 (W) | 0.0 (W) | 0.0 | 0.0 |  | 0.0 | 0.0

## Zone Equipment Detail

##### No Data to Show for Zone Equipment Detail

## Air Loops Detail

##### No Data to Show for Air Loops Detail

## Plant Loops Detail

##### No Data to Show for Plant Loops Detail

## Outdoor Air

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume (m^3) | Avg. Mechanical Ventilation (ach) | Min. Mechanical Ventilation (ach) | Avg. Infiltration (ach) | Min. Infiltration (ach) | Avg. Simple Ventilation (ach) | Min. Simple Ventilation (ach)
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 0.61 | 0.77 | 67 | 0.0 | 0.0 | 0.625 | 0.049 | 0.241 | 0.006
TZ_0-A1.LK | 0.88 | 1.28 | 122 | 0.0 | 0.0 | 1.053 | 0.056 | 0.455 | 0.009
TZ_0-A1.WC | 0.23 | 0.33 | 32 | 0.0 | 0.0 | 2.695 | 0.144 | 0.455 | 0.009
TZ_1-A2.B | 0.61 | 0.77 | 67 | 0.0 | 0.0 | 0.626 | 0.05 | 0.241 | 0.006
TZ_1-A2.LK | 0.88 | 1.28 | 122 | 0.0 | 0.0 | 1.055 | 0.056 | 0.456 | 0.009
TZ_1-A2.WC | 0.23 | 0.33 | 32 | 0.0 | 0.0 | 2.698 | 0.144 | 0.455 | 0.009

## Cash Flow

##### No Data to Show for Cash Flow

## Site and Source Summary

| Total Energy (kWh) | Energy Per Total Building Area (kWh/m^2) | Energy Per Conditioned Building Area (kWh/m^2)
--- | --- | --- | ---
Total Site Energy | 34761.1 | 167.1 | 213.0
Net Site Energy | 34761.1 | 167.1 | 213.0
Total Source Energy | 117738.9 | 566.1 | 721.4
Net Source Energy | 117738.9 | 566.1 | 721.4

| Site=>Source Conversion Factor
--- | ---
Electricity | 3.167
Natural Gas | 1.084
District Cooling | 1.056
District Heating | 0.0

## Schedule Overview

Schedule | Type Limits | Rules | Use Count
--- | --- | --- | ---
Air Velocity Schedule | Velocity | 0 | 1
ApartmentMidRise BLDG_ELEVATORS Pre2004 | Dimensionless | 0 | 2
ApartmentMidRise EQP_APT_SCH | Dimensionless | 0 | 4
Bedroom Schedule Activity | ActivityLevel | 0 | 2
Bedroom Schedule Equipment | Dimensionless | 2 | 2
Bedroom Schedule Light | Dimensionless | 2 | 2
Bedroom Schedule Occupancy | Dimensionless | 2 | 2
Clothing Schedule | ClothingInsulation | 1 | 1
Cooling setpoint | Temperature | 0 | 6
Heating setpoint | Temperature | 0 | 6
MidriseApartment Activity | ActivityLevel | 0 | 4
MidriseApartment Apartment Light | Dimensionless | 0 | 4
MidriseApartment Apartment Occ | Dimensionless | 0 | 4
MidriseApartment Corridor Light | Dimensionless | 0 | 2
MidriseApartment Infil | Dimensionless | 0 | 6
Schedule Infiltration | Dimensionless | 0 | 2
Work Efficiency Schedule | Dimensionless | 0 | 1

## Measure Warnings

Description | Count
--- | ---
Number of measures in workflow | 1
Number of measures with warnings | 0
Total number of warnings | 0