
@article{bib:sackinger:jssc:25:1:1990,
  author={Sackinger, E. and Guggenbuhl, W.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={A high-swing, high-impedance MOS cascode circuit},
  month={Feb.},
  year={1990},
  volume={25},
  number={1},
  pages={289-298},
  keywords={Voltage;Feedback circuits;Mirrors;Output feedback;Impedance;MOSFETs;Capacitance;Circuit noise;Operational amplifiers;Laboratories},
  doi={10.1109/4.50316}}

@article{bib:bult:jssc:25:6:dec:1990,
  author={Bult, K. and Geelen, G.J.G.M.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={A fast-settling CMOS op amp for SC circuits with 90-dB DC gain}, 
  year={1990},
  volume={25},
  number={6},
  pages={1379-1384},
  keywords={Operational amplifiers;Converters;Voltage;Feedback;Analog circuits;Filters;MOSFETs;Frequency measurement;Gain measurement;Bandwidth},
  doi={10.1109/4.62165}}

@article{bib:bult:aicsp:1991,
   Author = {Bult, K. and G. J. G. M. Geelen},
   Title = {{The CMOS gain-boosting technique}},
   Journal = {Analog Integrated Circuits and Signal Processing},
   Volume = {1},
   Number = {2},
   Pages = {119-135},
   Abstract = {The gain-boosting technique improves accuracy of cascoded CMOS circuits without any speed penalty. This is achieved by increasing the effect of the cascode transistor by means of an additional gain-stage, thus increasing the output impedance of the subcircuit. Used in opamp design, this technique allows the combination of the high-frequency behavior of a single-stage opamp with the high DC-gain of a multistage design. Bode-plot measurements show a DC-gain of 90 dB and a unity-gain frequency of 116 MHz (16 pF load). Settling measurements with a feedback factor of 1/3 show a fast single-pole settling behavior corresponding with a closed-loop bandwidth of 18 MHz (35 pF load) and a settling accuracy better than 0.03 percent. A more general use of this technique is presented in the form of a transistor-like building block: the Super-MOST. This compound circuit behaves as a normal MOS-transistor but has an intrinsic gain gm.ro of more than 90 dB. The building block is self-biasing and therefore very easy to design with. An opamp consisting of only 8 Super-MOST's and 4 normal MOST's has been measured showing results equivalent to the design mentioned above.},
   Month = {Jan.},
   Year = {1991} }


@book{bib:sansen:book:2006,
  author={Willy M. C. Sansen},
  title={Analog Design Essentials},
  publisher={Springer New York, NY},
  year={2006},
  isbn ={978-0-387-25746-4},
  doi={10.1007/b135984}
}

@article{bib:yukawa:jssc:20:3:1985,
  author={Yukawa, A.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={A CMOS 8-Bit High-Speed A/D Converter IC}, 
  year={1985},
  volume={20},
  number={3},
  pages={775-779},
  doi={10.1109/JSSC.1985.105238}
}

@article{bib:allstot:jssc:17:6:1982,
  author={Allstot, D.J.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={A precision variable-supply CMOS comparator}, 
  year={1982},
  volume={17},
  number={6},
  pages={1080-1087},
  doi={10.1109/JSSC.1982.1051864}
}

@book{bib:gregorian:book:1999,
  author =       {Roubik Gregorian},
  title =        {Introduction to CMOS Op-Amps and Comparators},
  publisher =    {John Wiley & Sons},
  year =         {1999},
}

@incollection{bib:sansen:aacd:2016,
  title={Opamps, Gm-blocks or inverters?},
  author={Sansen, Willy},
  booktitle={Efficient Sensor Interfaces, Advanced Amplifiers and Low Power RF Systems: Advances in Analog Circuit Design 2015},
  pages={125--138},
  year={2016},
  publisher={Springer}
}

@article{bib:ohri:jssc:14:1:1979,
  author={Ohri, K.B. and Callahan, M.J.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={Integrated PCM codec}, 
  year={1979},
  volume={14},
  number={1},
  pages={38-46},
  doi={10.1109/JSSC.1979.1051139}
}

@article{bib:castello:jssc:25:3:1990,
  author={Castello, R. and Grassi, A.G. and Donati, S.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={A 500-nA sixth-order bandpass SC filter}, 
  year={1990},
  volume={25},
  number={3},
  pages={669-676},
  doi={10.1109/4.102659}
}

@article{bib:alini:jssc:27:12:1992,
  author={Alini, R. and Baschirotto, A. and Castello, R.},
  journal={IEEE Journal of Solid-State Circuits}, 
  title={Tunable BiCMOS continuous-time filter for high-frequency applications}, 
  year={1992},
  volume={27},
  number={12},
  pages={1905-1915},
  doi={10.1109/4.173121}
}

@inproceedings{bib:hori:esscirc:2003,
  author={Shinichi Hori and Tadashi Maeda and hitoshi Yano and Noriaki Matsuno and Keiichi Numata and Nobuhide Yoshida and Yuji Takahashi and Tomoyuki Yamase and Walkington, R. and Hikaru, H.},
  booktitle={ESSCIRC 2004 - 29th European Solid-State Circuits Conference (IEEE Cat. No.03EX705)}, 
  title={A widely tunable CMOS Gm-C filter with a negative source degeneration resistor transconductor}, 
  year={2003},
  volume={},
  number={},
  pages={449-452},
  doi={10.1109/ESSCIRC.2003.1257169}
}

@inproceedings{bib:liscidini:isscc:2009,
  author={Liscidini, Antonio and Pirola, Alberto and Castello, Rinaldo},
  booktitle={2009 IEEE International Solid-State Circuits Conference - Digest of Technical Papers}, 
  title={A 1.25mW 75dB-SFDR CT filter with in-band noise reduction}, 
  year={2009},
  volume={},
  number={},
  pages={336-337,337a},
  doi={10.1109/ISSCC.2009.4977445}
}

@inproceedings{bib:damico:isscc:2006,
  author={D'Amico, S. and Conta, M. and Baschirotto, A.},
  booktitle={2006 IEEE International Solid State Circuits Conference - Digest of Technical Papers}, 
  title={A 4.1mW 79dB-DR 4th-order Source-FollowerBased Continuous-Time Filter for WLAN Receivers}, 
  year={2006},
  volume={},
  number={},
  pages={1378-1387},
  doi={10.1109/ISSCC.2006.1696187}
}

@article{bib:damico:tmtt:62:8:2014,
  author={D'Amico, Stefano and Spagnolo, Annachiara and Donno, Andrea and Chironi, Vincenzo and Wambacq, Piet and Baschirotto, Andrea},
  journal={IEEE Transactions on Microwave Theory and Techniques}, 
  title={A Low-Power Analog Baseband Section for 60-GHz Receivers in 90-nm CMOS}, 
  year={2014},
  volume={62},
  number={8},
  pages={1724-1735},
  doi={10.1109/TMTT.2014.2332877}
}

