# OpenStudio Results

## Model Summary

Data | Value
--- | ---
Building Name | Building 1
Total Site Energy | 59,189 kWh
Total Building Area | 338 m^2
Total Site EUI | 175.12 kWh/m^2
OpenStudio Standards Building Type | n/a

| Value
--- | ---
Weather File | MILAN - ITA IWEC Data WMO#=160660
Latitude | 45.62
Longitude | 8.73
Elevation | 211 m
Time Zone | 1.00
North Axis Angle | 0.00
ASHRAE Climate Zone |

| Maximum Dry Bulb (C) | Daily Temperature Range (K) | Humidity Value | Humidity Type | Wind Speed (m/s) | Wind Direction
--- | --- | --- | --- | --- | --- | ---
None | 0.0 | 0.0 | 0.0 |  | 0.0 | 0.0

Time Setpoint Not Met | Time (hr)
--- | ---
During Heating | 0.0
During Cooling | 0.0
During Occupied Heating | 0.0
During Occupied Cooling | 0.0

Tolerance for Time Setpoint Not Met | Temperature (C)
--- | ---
Heating | 0.2
Cooling | 0.2

## Annual Overview

End Use | Consumption (kWh)
--- | ---
Heating | 40,106
Cooling | 2,722
Interior Lighting | 7,344
Exterior Lighting | 0
Interior Equipment | 9,017
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

Fuel | Consumption (kWh)
--- | ---
Electricity | 16,361
Natural Gas | 0
Gasoline | 0
Diesel | 0
Coal | 0
Fuel Oil No 1 | 0
Fuel Oil No 2 | 0
Propane | 0
Other Fuel 1 | 0
Other Fuel 2 | 0
District Cooling | 2,722
District Heating Water | 40,106
District Heating Steam | 0

End Use | Consumption (kWh)
--- | ---
Heating | 0
Cooling | 0
Interior Lighting | 7,344
Exterior Lighting | 0
Interior Equipment | 9,017
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

End Use | Consumption (kWh)
--- | ---
Heating | 0
Cooling | 0
Interior Lighting | 0
Exterior Lighting | 0
Interior Equipment | 0
Exterior Equipment | 0
Fans | 0
Pumps | 0
Heat Rejection | 0
Humidification | 0
Heat Recovery | 0
Water Systems | 0
Refrigeration | 0
Generators | 0

## Monthly Overview

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting | 623.79 | 563.43 | 623.79 | 603.67 | 623.79 | 603.67 | 623.79 | 623.79 | 603.67 | 623.79 | 603.67 | 623.79 | 7344.64
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment | 765.77 | 691.66 | 765.77 | 741.07 | 765.77 | 741.07 | 765.77 | 765.77 | 741.07 | 765.77 | 741.07 | 765.77 | 9016.35
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total | 1389.56 | 1255.09 | 1389.56 | 1344.74 | 1389.56 | 1344.74 | 1389.56 | 1389.56 | 1344.74 | 1389.56 | 1344.74 | 1389.56 | 16360.99

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  | 0.06 | 0.93 | 117.44 | 549.89 | 1159.06 | 729.08 | 164.3 | 1.0 |  |  | 2721.75
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total |  |  | 0.06 | 0.93 | 117.44 | 549.89 | 1159.06 | 729.08 | 164.3 | 1.0 |  |  | 2721.75

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec | Total
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating | 8677.03 | 6719.08 | 4540.75 | 2873.94 | 940.57 | 268.83 | 7.38 | 27.56 | 634.61 | 2388.81 | 5262.5 | 7765.0 | 40106.06
Cooling |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |  |
Total | 8677.03 | 6719.08 | 4540.75 | 2873.94 | 940.57 | 268.83 | 7.38 | 27.56 | 634.61 | 2388.81 | 5262.5 | 7765.0 | 40106.06

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792 | 1.5792
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549 | 1.4549
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03 | 3.03

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating |  |  |  |  |  |  |  |  |  |  |  |
Cooling |  |  | 36.13 | 331.89 | 2891.62 | 7881.15 | 9110.11 | 6747.23 | 4092.94 | 143.91 |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total |  |  | 36.13 | 331.89 | 2891.62 | 7881.15 | 9110.11 | 6747.23 | 4092.94 | 143.91 |  |

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Heating | 22048.54 | 18117.73 | 15679.92 | 14052.55 | 8054.21 | 7747.35 | 1016.89 | 2386.39 | 7375.96 | 12158.94 | 15499.71 | 19707.85
Cooling |  |  |  |  |  |  |  |  |  |  |  |
Interior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Exterior Lighting |  |  |  |  |  |  |  |  |  |  |  |
Interior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Exterior Equipment |  |  |  |  |  |  |  |  |  |  |  |
Fans |  |  |  |  |  |  |  |  |  |  |  |
Pumps |  |  |  |  |  |  |  |  |  |  |  |
Heat Rejection |  |  |  |  |  |  |  |  |  |  |  |
Humidification |  |  |  |  |  |  |  |  |  |  |  |
Heat Recovery |  |  |  |  |  |  |  |  |  |  |  |
Water Systems |  |  |  |  |  |  |  |  |  |  |  |
Refrigeration |  |  |  |  |  |  |  |  |  |  |  |
Generators |  |  |  |  |  |  |  |  |  |  |  |
Total | 22048.54 | 18117.73 | 15679.92 | 14052.55 | 8054.21 | 7747.35 | 1016.89 | 2386.39 | 7375.96 | 12158.94 | 15499.71 | 19707.85

## Utility Bills/Rates

##### No Data to Show for Utility Bills/Rates

## Envelope Summary

Construction | Net Area (m^2) | Surface Count | R Value (m^2*K/W)
--- | --- | --- | ---
Typical IEAD Roof R-17.24 10 | 169.0 | 6 | 2.90
Typical Insulated Steel Framed Exterior Wall R-11.24 4 | 241.4 | 22 | 1.83

Construction | Net Area (m^2) | Surface Count | U-factor (W/m^2*K) | SHGC | VLT
--- | --- | --- | --- | --- | ---
U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 23 | 33.6 | 15 | 3.35 | 0.36 | 0.27
U 0.88 SHGC 0.16 Sgl Ref-A-L Clr 6mm | 5.8 | 1 | 150.00 | 0.07 | 0.08

Material Name
##### (Material Layers in Construction 'U 0.59 SHGC 0.36 Simple Glazing Window U-0.59 SHGC 0.36 23':)
U 0.59 SHGC 0.36 Simple Glazing U-0.59 SHGC 0.36 23
##### (Material Layers in Construction 'U 0.88 SHGC 0.16 Sgl Ref-A-L Clr 6mm':)
REF A CLEAR LO 6MM

Description | Total (%) | North (%) | East (%) | South (%) | West (%)
--- | --- | --- | --- | --- | ---
Gross Window-Wall Ratio | 14.02 | 15.95 | 6.38 | 15.95 | 17.78
Gross Window-Wall Ratio (Conditioned) | 14.25 | 20.33 | 6.38 | 15.95 | 18.23
Skylight-Roof Ratio | 0.0 |  |  |  |

## Space Type Breakdown

Space Type Name | Floor Area (m^2) | Standards Building Type | Standards Space Type
--- | --- | --- | ---
MidriseApartment Apartment | 291 | MidriseApartment | Apartment
MidriseApartment Corridor | 47 | MidriseApartment | Corridor

## Space Type Summary

Definition | Value | Unit | Inst. Multiplier
--- | --- | --- | ---
MidriseApartment Apartment People Definition | 0.0283 | people/m^2 | 1.0
MidriseApartment Apartment Elec Equip Definition | 5.3820 | W/m^2 | 1.0
MidriseApartment Apartment Lights Definition | 3.8750 | W/m^2 | 1.0
MidriseApartment Apartment Infiltration | 0.0011 | m^3/h/ext wall area m^2 |
MidriseApartment Apartment Ventilation (outdoor air method Sum) | 61.1644 | m^3/h/person |

Definition | Value | Unit | Inst. Multiplier
--- | --- | --- | ---
MidriseApartment Corridor Lights Definition | 9.9028 | W/m^2 | 1.0
MidriseApartment Corridor Infiltration | 0.0011 | m^3/h/ext wall area m^2 |

## Interior Lighting Summary

Lights | Zone | Lighting Power Density (W/m^2) | Total Power (W) | Schedule Name | Scheduled Hours/Week (hr) | Actual Load Hours/Week (hr) | Return Air Fraction | Annual Consumption (kWh)
--- | --- | --- | --- | --- | --- | --- | --- | ---
1-A3.B1 MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 74.47 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 213.89
0-A2.B MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 70.94 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 202.78
0-A1.LK MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 144.5 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 416.67
0-A2.LK MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 189.49 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 544.44
1-A3.W1 MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 41.9 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 119.44
0-A1.B MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 74.47 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 213.89
0-A1.W MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 41.9 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 119.44
0-A2.W MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 41.9 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 119.44
1-A3.B2 MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 70.94 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 202.78
1-A3.LK MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 333.99 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 961.11
1-A3.W2 MIDRISEAPARTMENT APARTMENT LIGHTS |  | 3.88 | 41.9 | MIDRISEAPARTMENT APARTMENT LIGHT | 55.16 | 55.16 | 0.0000 | 119.44
0-H MIDRISEAPARTMENT CORRIDOR LIGHTS |  | 9.9 | 234.3 | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.0 | 168.0 | 0.0000 | 2052.78
1-H MIDRISEAPARTMENT CORRIDOR LIGHTS |  | 9.9 | 234.3 | MIDRISEAPARTMENT CORRIDOR LIGHT | 168.0 | 168.0 | 0.0000 | 2052.78

Load Name | Definition Name | Load Type | Load (units) | Multiplier | Total Load (W)
--- | --- | --- | --- | --- | ---
##### (Space Name: '1-A3.B1', Area: 19 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 74
##### (Space Name: '0-A2.B', Area: 18 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 71
##### (Space Name: '0-A1.LK', Area: 37 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 144
##### (Space Name: '0-A2.LK', Area: 49 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 189
##### (Space Name: '1-A3.W1', Area: 11 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 42
##### (Space Name: '0-H', Area: 24 m^2, Total LPD: 9.9 W/m^2) |  |  |  |  |
MidriseApartment Corridor Lights | MidriseApartment Corridor Lights Definition | Spacetype | 9.9 (W/m^2) | 1 | 234
##### (Space Name: '0-A1.B', Area: 19 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 74
##### (Space Name: '1-H', Area: 24 m^2, Total LPD: 9.9 W/m^2) |  |  |  |  |
MidriseApartment Corridor Lights | MidriseApartment Corridor Lights Definition | Spacetype | 9.9 (W/m^2) | 1 | 234
##### (Space Name: '0-A1.W', Area: 11 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 42
##### (Space Name: '0-A2.W', Area: 11 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 42
##### (Space Name: '1-A3.B2', Area: 18 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 71
##### (Space Name: '1-A3.LK', Area: 86 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 334
##### (Space Name: '1-A3.W2', Area: 11 m^2, Total LPD: 3.88 W/m^2) |  |  |  |  |
MidriseApartment Apartment Lights | MidriseApartment Apartment Lights Definition | Spacetype | 3.88 (W/m^2) | 1 | 42

Space Name | Control Name | Zone Controlled (type, fraction) | Illuminance Setpoint (lux)
--- | --- | --- | ---

## Plug Loads Summary

| Electricity Annual Value (kWh)
--- | ---
InteriorEquipment:Electricity:Zone:TZ_1-A3.B1 | 597.22
General:InteriorEquipment:Electricity:Zone:TZ_1-A3.B1 | 597.22
InteriorEquipment:Electricity:Zone:TZ_0-A2.B | 566.67
General:InteriorEquipment:Electricity:Zone:TZ_0-A2.B | 566.67
InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 1155.56
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.LK | 1155.56
InteriorEquipment:Electricity:Zone:TZ_0-A2.LK | 1516.67
General:InteriorEquipment:Electricity:Zone:TZ_0-A2.LK | 1516.67
InteriorEquipment:Electricity:Zone:TZ_1-A3.W1 | 336.11
General:InteriorEquipment:Electricity:Zone:TZ_1-A3.W1 | 336.11
InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 597.22
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.B | 597.22
InteriorEquipment:Electricity:Zone:TZ_0-A1.W | 336.11
General:InteriorEquipment:Electricity:Zone:TZ_0-A1.W | 336.11
InteriorEquipment:Electricity:Zone:TZ_0-A2.W | 336.11
General:InteriorEquipment:Electricity:Zone:TZ_0-A2.W | 336.11
InteriorEquipment:Electricity:Zone:TZ_1-A3.B2 | 566.67
General:InteriorEquipment:Electricity:Zone:TZ_1-A3.B2 | 566.67
InteriorEquipment:Electricity:Zone:TZ_1-A3.LK | 2672.22
General:InteriorEquipment:Electricity:Zone:TZ_1-A3.LK | 2672.22
InteriorEquipment:Electricity:Zone:TZ_1-A3.W2 | 336.11
General:InteriorEquipment:Electricity:Zone:TZ_1-A3.W2 | 336.11

Equipment Name | Definition | Load (units) | Inheritance Level | Multiplier | Total Load (W)
--- | --- | --- | --- | --- | ---
##### (Space Name: 0-A1.B, Area: 19 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 103
##### (Space Name: 0-A1.LK, Area: 37 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 201
##### (Space Name: 0-A1.W, Area: 11 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 58
##### (Space Name: 0-A2.B, Area: 18 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 99
##### (Space Name: 0-A2.LK, Area: 49 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 263
##### (Space Name: 0-A2.W, Area: 11 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 58
##### (Space Name: 1-A3.B1, Area: 19 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 103
##### (Space Name: 1-A3.B2, Area: 18 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 99
##### (Space Name: 1-A3.LK, Area: 86 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 464
##### (Space Name: 1-A3.W1, Area: 11 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 58
##### (Space Name: 1-A3.W2, Area: 11 m^2) |  |  |  |  |
MidriseApartment Apartment Elec Equip | MidriseApartment Apartment Elec Equip Definition | 5.38 (W/m^2) | spacetype | 1.0 | 58

## Exterior Lighting

##### No Data to Show for Exterior Lighting

## Water Use Equipment

##### No Data to Show for Water Use Equipment

## HVAC Load Profiles

| Jan | Feb | Mar | Apr | May | Jun | Jul | Aug | Sep | Oct | Nov | Dec
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Average Outdoor Air Dry Bulb (C) | 0.3 | 2.2 | 7.5 | 10.9 | 16.3 | 19.7 | 23.1 | 22.2 | 17.6 | 12.5 | 6.5 | 2.2
Cooling Load (kWh) | 0.0 | 0.0 | 0.06 | 0.93 | 117.44 | 549.89 | 1159.06 | 729.08 | 164.3 | 1.0 | 0.0 | 0.0
Heating Load (kWh) | 8677.03 | 6719.08 | 4540.75 | 2873.94 | 940.57 | 268.83 | 7.38 | 27.56 | 634.61 | 2388.81 | 5262.5 | 7765.0

## Zone Conditions

Zone | Unmet Htg (hr) | Unmet Htg - Occ (hr) | < 13 (C) | 13-16 (C) | 16-18 (C) | 18-20 (C) | 20-21 (C) | 21-22 (C) | 22-23 (C) | 23-24 (C) | 24-26 (C) | 26-28 (C) | 28-30 (C) | >= 30 (C) | Unmet Clg (hr) | Unmet Clg - Occ (hr) | Mean Temp (C)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 0 | 0 | 0 | 0 | 0 | 171 | 6238 | 564 | 526 | 495 | 653 | 113 | 0 | 0 | 0 | 0 | 20.9 (C)
TZ_0-A1.LK | 0 | 0 | 0 | 0 | 0 | 161 | 5934 | 619 | 663 | 592 | 711 | 80 | 0 | 0 | 0 | 0 | 21.0 (C)
TZ_0-A1.W | 0 | 0 | 0 | 0 | 0 | 151 | 5954 | 598 | 625 | 592 | 756 | 84 | 0 | 0 | 0 | 0 | 21.0 (C)
TZ_0-A2.B | 0 | 0 | 0 | 0 | 0 | 161 | 6004 | 574 | 508 | 483 | 792 | 238 | 0 | 0 | 0 | 0 | 21.1 (C)
TZ_0-A2.LK | 0 | 0 | 0 | 0 | 0 | 134 | 5931 | 585 | 588 | 511 | 808 | 203 | 0 | 0 | 0 | 0 | 21.1 (C)
TZ_0-A2.W | 0 | 0 | 0 | 0 | 0 | 124 | 5904 | 603 | 622 | 584 | 811 | 112 | 0 | 0 | 0 | 0 | 21.1 (C)
TZ_0-H | 0 | 0 | 1562 | 1809 | 1023 | 1015 | 476 | 419 | 483 | 507 | 766 | 441 | 206 | 53 | 0 | 0 | 18.4 (C)
TZ_1-A3.B1 | 0 | 0 | 0 | 0 | 0 | 161 | 5834 | 431 | 405 | 372 | 872 | 685 | 0 | 0 | 0 | 0 | 21.4 (C)
TZ_1-A3.B2 | 0 | 0 | 0 | 0 | 0 | 164 | 5621 | 439 | 414 | 382 | 937 | 803 | 0 | 0 | 0 | 0 | 21.5 (C)
TZ_1-A3.LK | 0 | 0 | 0 | 0 | 0 | 118 | 5578 | 412 | 443 | 380 | 940 | 889 | 0 | 0 | 0 | 0 | 21.5 (C)
TZ_1-A3.W1 | 0 | 0 | 0 | 0 | 0 | 148 | 5510 | 450 | 441 | 411 | 955 | 845 | 0 | 0 | 0 | 0 | 21.5 (C)
TZ_1-A3.W2 | 0 | 0 | 0 | 0 | 0 | 153 | 5437 | 436 | 459 | 404 | 989 | 882 | 0 | 0 | 0 | 0 | 21.6 (C)
TZ_1-H | 0 | 0 | 2050 | 1408 | 854 | 890 | 390 | 345 | 369 | 372 | 690 | 541 | 425 | 426 | 0 | 0 | 18.7 (C)

Zone | < 30 (%) | 30-35 (%) | 35-40 (%) | 40-45 (%) | 45-50 (%) | 50-55 (%) | 55-60 (%) | 60-65 (%) | 65-70 (%) | 70-75 (%) | 75-80 (%) | >= 80 (%) | Mean Relative Humidity (%)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 2514 | 857 | 568 | 601 | 566 | 627 | 587 | 708 | 588 | 517 | 410 | 217 | 45.0 (%)
TZ_0-A1.LK | 2383 | 885 | 595 | 588 | 545 | 646 | 618 | 746 | 687 | 478 | 398 | 191 | 45.5 (%)
TZ_0-A1.W | 2450 | 878 | 588 | 602 | 585 | 624 | 638 | 737 | 596 | 470 | 383 | 209 | 45.0 (%)
TZ_0-A2.B | 2532 | 880 | 595 | 625 | 613 | 631 | 611 | 672 | 551 | 485 | 373 | 192 | 44.4 (%)
TZ_0-A2.LK | 2467 | 894 | 591 | 621 | 600 | 660 | 611 | 698 | 594 | 488 | 358 | 178 | 44.7 (%)
TZ_0-A2.W | 2459 | 880 | 590 | 609 | 596 | 641 | 624 | 767 | 563 | 466 | 363 | 202 | 44.8 (%)
TZ_0-H | 929 | 788 | 946 | 925 | 1023 | 907 | 999 | 900 | 738 | 432 | 151 | 22 | 48.8 (%)
TZ_1-A3.B1 | 2555 | 907 | 664 | 723 | 645 | 658 | 652 | 663 | 522 | 425 | 251 | 95 | 43.2 (%)
TZ_1-A3.B2 | 2611 | 927 | 671 | 792 | 650 | 634 | 625 | 625 | 478 | 421 | 234 | 92 | 42.6 (%)
TZ_1-A3.LK | 2507 | 940 | 701 | 825 | 648 | 662 | 672 | 635 | 502 | 420 | 174 | 74 | 42.8 (%)
TZ_1-A3.W1 | 2514 | 944 | 694 | 816 | 681 | 654 | 688 | 642 | 484 | 396 | 181 | 66 | 42.7 (%)
TZ_1-A3.W2 | 2534 | 936 | 717 | 822 | 677 | 657 | 678 | 638 | 477 | 378 | 182 | 64 | 42.5 (%)
TZ_1-H | 901 | 793 | 979 | 1103 | 961 | 1133 | 1095 | 876 | 600 | 265 | 54 | 0 | 47.7 (%)

## Zone Overview

| Area (m^2) | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Volume (m^3) | Multiplier | Above Ground Gross Wall Area (m^2) | Underground Gross Wall Area (m^2) | Window Glass Area (m^2) | Lighting (W/m^2) | People (m^2/person) | Plug and Process (W/m^2)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 19.22 | Yes | Yes | 51.89 | 1.00 | 22.68 | 0.0 | 2.24 | 3.88 | 35.32 | 5.38
TZ_0-A1.LK | 37.29 | Yes | Yes | 100.68 | 1.00 | 15.25 | 0.0 | 3.36 | 3.88 | 35.32 | 5.38
TZ_0-A1.W | 10.81 | Yes | Yes | 29.19 | 1.00 | 7.43 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_0-A2.B | 18.31 | Yes | Yes | 49.43 | 1.00 | 22.14 | 0.0 | 2.24 | 3.88 | 35.32 | 5.38
TZ_0-A2.LK | 48.9 | Yes | Yes | 132.03 | 1.00 | 35.1 | 0.0 | 5.6 | 3.88 | 35.32 | 5.38
TZ_0-A2.W | 10.81 | Yes | Yes | 29.19 | 1.00 | 7.43 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_0-H | 23.66 | No | Yes | 63.88 | 1.00 | 30.38 | 0.0 | 5.76 | 9.9 | 0.0 | 0.0
TZ_1-A3.B1 | 19.22 | Yes | Yes | 51.89 | 1.00 | 22.68 | 0.0 | 2.24 | 3.88 | 35.32 | 5.38
TZ_1-A3.B2 | 18.31 | Yes | Yes | 49.43 | 1.00 | 22.14 | 0.0 | 2.24 | 3.88 | 35.32 | 5.38
TZ_1-A3.LK | 86.19 | Yes | Yes | 232.71 | 1.00 | 50.36 | 0.0 | 8.96 | 3.88 | 35.32 | 5.38
TZ_1-A3.W1 | 10.81 | Yes | Yes | 29.19 | 1.00 | 7.43 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_1-A3.W2 | 10.81 | Yes | Yes | 29.19 | 1.00 | 7.43 | 0.0 | 1.12 | 3.88 | 35.32 | 5.38
TZ_1-H | 23.66 | No | Yes | 63.88 | 1.00 | 30.38 | 0.0 | 2.24 | 9.9 | 0.0 | 0.0
Total | 338.0 |  |  | 912.6 |  | 280.8 | 0.0 | 39.36 | 4.72 | 41.07 | 4.63
Conditioned Total | 290.68 |  |  | 784.84 |  | 220.05 | 0.0 | 31.36 | 3.88 | 35.32 | 5.38
Unconditioned Total | 47.32 |  |  | 127.76 |  | 60.75 | 0.0 | 8.0 | 9.9 | 0.0 | 0.0
Not Part of Total | 0.0 |  |  | 0.0 |  | 0.0 | 0.0 | 0.0 | 0.0 | 0.0 | 0.0

| Heating/Cooling | Calculated Design Load | Design Load With Sizing Factor | Calculated Design Air Flow (m^3/h) | Design Air Flow With Sizing Factor (m^3/h) | Date/Time Of Peak | Outdoor Temperature at Peak Load (C) | Outdoor Humidity Ratio at Peak Load (kgWater/kgAir)
--- | --- | --- | --- | --- | --- | --- | --- | ---
None | Cooling | 0.0 (W) | 0.0 (W) | 0.0 | 0.0 |  | 0.0 | 0.0
None | Heating | 0.0 (W) | 0.0 (W) | 0.0 | 0.0 |  | 0.0 | 0.0

## Zone Equipment Detail

##### No Data to Show for Zone Equipment Detail

## Air Loops Detail

##### No Data to Show for Air Loops Detail

## Plant Loops Detail

##### No Data to Show for Plant Loops Detail

## Outdoor Air

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume (m^3) | Avg. Mechanical Ventilation (ach) | Min. Mechanical Ventilation (ach) | Avg. Infiltration (ach) | Min. Infiltration (ach) | Avg. Simple Ventilation (ach) | Min. Simple Ventilation (ach)
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TZ_0-A1.B | 0.37 | 0.54 | 52 | 0.0 | 0.0 | 1.841 | 0.098 | 0.455 | 0.011
TZ_0-A1.LK | 0.72 | 1.06 | 101 | 0.0 | 0.0 | 0.639 | 0.034 | 0.455 | 0.011
TZ_0-A1.W | 0.21 | 0.31 | 29 | 0.0 | 0.0 | 1.072 | 0.057 | 0.455 | 0.011
TZ_0-A2.B | 0.35 | 0.52 | 49 | 0.0 | 0.0 | 1.888 | 0.101 | 0.455 | 0.011
TZ_0-A2.LK | 0.95 | 1.38 | 132 | 0.0 | 0.0 | 1.121 | 0.06 | 0.455 | 0.011
TZ_0-A2.W | 0.21 | 0.31 | 29 | 0.0 | 0.0 | 1.072 | 0.057 | 0.455 | 0.011
TZ_1-A3.B1 | 0.37 | 0.54 | 52 | 0.0 | 0.0 | 1.844 | 0.099 | 0.456 | 0.011
TZ_1-A3.B2 | 0.35 | 0.52 | 49 | 0.0 | 0.0 | 1.89 | 0.102 | 0.456 | 0.011
TZ_1-A3.LK | 1.67 | 2.44 | 233 | 0.0 | 0.0 | 0.913 | 0.049 | 0.456 | 0.011
TZ_1-A3.W1 | 0.21 | 0.31 | 29 | 0.0 | 0.0 | 1.074 | 0.058 | 0.456 | 0.011
TZ_1-A3.W2 | 0.21 | 0.31 | 29 | 0.0 | 0.0 | 1.074 | 0.058 | 0.456 | 0.011

## Cash Flow

##### No Data to Show for Cash Flow

## Site and Source Summary

| Total Energy (kWh) | Energy Per Total Building Area (kWh/m^2) | Energy Per Conditioned Building Area (kWh/m^2)
--- | --- | --- | ---
Total Site Energy | 59188.9 | 175.1 | 203.6
Net Site Energy | 59188.9 | 175.1 | 203.6
Total Source Energy | 199605.6 | 590.5 | 686.7
Net Source Energy | 199605.6 | 590.5 | 686.7

| Site=>Source Conversion Factor
--- | ---
Electricity | 3.167
Natural Gas | 1.084
District Cooling | 1.056
District Heating | 0.0

## Schedule Overview

Schedule | Type Limits | Rules | Use Count
--- | --- | --- | ---
Air Velocity Schedule | Velocity | 0 | 1
ApartmentMidRise BLDG_ELEVATORS Pre2004 | Dimensionless | 0 | 2
ApartmentMidRise EQP_APT_SCH | Dimensionless | 0 | 11
Clothing Schedule | ClothingInsulation | 1 | 1
Cooling Setpoint | Temperature | 0 | 11
Heating Setpoint | Temperature | 0 | 11
MidriseApartment Activity | ActivityLevel | 0 | 11
MidriseApartment Apartment Light | Dimensionless | 0 | 11
MidriseApartment Apartment Occ | Dimensionless | 0 | 11
MidriseApartment Corridor Light | Dimensionless | 0 | 2
MidriseApartment Infil | Dimensionless | 0 | 13
Work Efficiency Schedule | Dimensionless | 0 | 1

## Measure Warnings

Description | Count
--- | ---
Number of measures in workflow | 1
Number of measures with warnings | 0
Total number of warnings | 0