    % Matlab EQuilibrium Toolbox
    % Version 6.2.0 1-Jan-1970
    %
    % HELP
    %   meqhelp     - Main symbol dictionary and various types of help per code
    %
    % LIUQE Equilibrium reconstruction
    %   liu         - LIUQE top level equilibrium reconstuction
    %   liup        - LIUQE default algorithm configuration parameters
    %   liug        - LIUQE geometry and electromagnetic parameters
    %   liux        - LIUQE diagnostic measurements
    %   liuc        - LIUQE ancillary data
    %   liut        - LIUQE reconstruction
    %   liuzf       - LIUQE calling scheme for vertical stabilisation functions
    %   liudz       - LIUQE vertical stabilisation function based on shift fitting
    %   liuz0       - LIUQE vertical stabilisation function based on ZA-Z0
    %
    %  RT LIUQE Simulink equilibrium reconstruction
    %   liusimc     - LIUQE initialisation for LIUSIM model
    %
    % FBT Free Boundary Tokamak Equilibrium
    %   fbt         - FBTE top level function
    %   fbtp        - FBTE default configuration parameters
    %   fbtg        - FBTE geometry and electromagnetic parameters
    %   fbtc        - FBTE ancillary data
    %   fbtx        - FBTE input data retrieval/handling
    %   fbtt        - FBTE equilibrium calculation
    %
    % FGS Free Boundary Static Forward solver
    %   fge         - FGS top level function
    %   fgep        - FGS default configuration parameters
    %   fgeg        - FGS geometry and electromagnetic parameters
    %   fgec        - FGS ancillary data
    %   fgsx        - FGS input data retrieval/handling
    %   fget        - FGS equilibrium calculation
    %
    % FGE Free Boundary Evolutive Forward Solver
    %   fge         - FGE top level function
    %   fgep        - FGE default configuration parameters
    %   fgeg        - FGE geometry and electromagnetic parameters
    %   fgec        - FGE ancillary data
    %   fgex        - FGE input data retrieval/handling
    %   fget        - FGE equilibrium (time-stepping) calculation
    %
    % MEQ MatlabEQuilibrium Toolbox
    %  MEX files for libmeq toolbox
    %   asxymex      - Localise extrema and saddle points of a 2D-map
    %   bavxmex      - Find points inside X-point polygon
    %   bboxmex      - Domain bounding box
    %   bslvmex      - Block solving algorithm
    %   fbndmex      - Find LCFS
    %   gszrmex      - Solve Poisson equation
    %   iatamex      - LDL matrix inversion
    %   ipm4mex      - Interior point method for aX>0 and no equality constraints
    %   ipmhmex      - Fit FE elements with Interior Point Method
    %   fsgimex      - Flux surface geometrical integrals
    %   nfdbmex      - Normal flux derivative on boundary
    %   pdommex      - Find plasma domain
    %   respmex      - Build internal response matrix
    %   rtcimex      - Isoflux contouring
    %
    %   fetr         - TRiangular Finite Elements
    %   febi         - Bilinear finite elements
    %   gszrc        - Ancillary data for GSZR Poisson solver
    %   meq2psi      - Convert MEQ LY structure to PSITBXPSI object
    %   meqc         - MEQ ancillary data
    %   meqfbp       - Plasma contribution to boundary condition for Poisson solver
    %   meqg         - MEQ geometry and electromagnetic parameters
    %   meqint       - Equilibrium integrals
    %   meqmesh      - Computational grid related quantities
    %   meqpdom      - Plasma domain parameters
    %   meqpost      - General equilibrium post-processing
    %   meqxk        - Extracts samples from LX/LY structure
    %   meqxconvert  - Convert meq equilibrium from one representation to another
    %   meqreprocess - Reprocess meq equilibrium to compute post-processing and more
    %
    %  Base functions for p',TT'
    %   bfhelp      - Calling scheme for base functions for p',TT'
    %   bf3imex     - 3 base functions for p',TT' by tabular interpolation
    %   bf3pmex     - 3 polynomial base functions for p',TT'
    %   bfabmex     - Polynomial base functions for p',TT'
    %   bfef        - Constant and polynomial base functions for p',TT'
    %   bfprmex     - Tabular base function integrals for p',TT'
    %   bffbt       - FBT base functions for p',TT'
    %
    % PLOTTING
    %   meqplott     - Time slice plot
    %   meqplotevo   - Time evolution
    %   meqplotfancy - fancy plot
    %   meqmovie     - Movie of time history
    %
    % SPECIFIC TOKAMAKS
    %  TCV GENERIC
    %   mds2meq     - Read TCV MDS nodes to meq structure
    %   ts2LY       - From Simulink timeseries to LY object
    %
    %  TCV LIUQE
    %   liuqe       - TCV LIUQE equilibrium reconstuction
    %   liuptcv     - TCV LIUQE configuration parameters
    %   liugtcv     - TCV LIUQE geometry and electromagnetic parameters
    %   liuxtcv     - TCV LIUQE diagnostic measurements
    %   liuxrtc     - TCV LIUQE diagnostic measurements from RTC tree
    %   meqgtcv     - TCV MEQ geometry and electromagnetic parameters
    %
    %  RESULTS tree
    %   meqwtcv     - Writes MEQ data in TCV tree
    %   liuwtcv     - Write LIUQE specific data in TCV tree
    %   psiwtcv     - Write PSITBX specific data in TCV tree
    %   liuanasrv   - Called by ANASRV to compute and write in RESULTS tree
    %   liuqe_times - Determine time array for LIUQE anasrv call
    %
    %  TCV FBTE
    %   fbte        - TCV FBTE equilibrium calculation
    %   fbtptcv     - TCV FBT configuration parameters
    %   fbtgtcv     - TCV FBT geometry and electromagnetic parameters
    %   fbtwtcv     - Write FBT specific data in TCV tree
    %
    %  CREATE(ITER) LIUQE
    %   liupcreate  - CREATE(ITER) LIUQE algorithm configuration parameters
    %   liugcreate  - CREATE(ITER) LIUQE geometry
    %   liuxcreate  - CREATE(ITER) LIUQE diagnostic measurements
    %   createf     - CREATE(ITER) Locates equilibrium file
    %
    %  RFX LIUQE
    %   liuprfx     - RFX LIUQE configuration parameters
    %   liugrfx     - RFX LIUQE geometry and electromagnetic parameters
    %   liuxrfx     - RFX LIUQE diagnostic measurements
    %
    % DEVELOPERS
    %  Code generation
    %   meqld       - Selects ld script for MEQ
    %   mkcsf       - Makes C code for S-function blocks using Legacy Tool
    %   mkldl       - Generates code for LDL inversion
    %   mkmeqh      - Generates include file MEQ.H
    %   liucomp     - function liucomp(L1,LY1,L2,LY2,labels)
    %   liuxcomp    - LIUQE measurement signal comparison
    %
    % [+MEQ MatlabEQuilibrium Toolbox+] Swiss Plasma Center EPFL Lausanne 2022. All rights reserved.